Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	1024	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Melanie Roberts	Locality:
	Date Desc.:	10/10/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6261481 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	651453  Datum: AGD84	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition 
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Hypernatric  Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	A1c	0 - 0.1 m	; Loamy sand; 20-50%, Ironstone, coarse fragments; Field pH 7.1 (pH meter); 
	A2ec	0.1 - 0.3 m	; 50-90%, Ironstone, coarse fragments; Field pH 7.4 (pH meter); 
	B21c	0.3 - 0.7 m	, 20-50% ; Light clay; Strong grade of structure; 10-20%, Ironstone, coarse fragments; Field pH 8.1 (pH 
	meter); 
	B22c	0.7 - 1.5 m	; Light clay; Massive grade of structure; Field pH 7.4 (pH meter); 
	B23	1.5 - 1.6 m	; Light medium clay; Massive grade of structure; Field pH 4.9 (pH meter); 
	Morphological Notes
	A2ec	Bleached sandy loam.
	B21c	Clay some gravel, mottled clay
	B22c	Saprolite.
	B23	Kaolinite.
	Observation Notes
	Site Notes
	Soil pit a loamy gravel. Recharge area for lower slopes. Downslope of site is waterlogged area with lucerne balansa clover.

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	1024	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.8B	22B	4.47A	1.1	1.03	0.49	7.09D
	6.7H
	0 - 0.1	5.8B	22B	4.47A	1.1	1.03	0.49	7.09D
	6.7H
	0.1 - 0.3	6.7B	6B	1.35A	0.54	0.24	0.34	2.47D
	8H
	0.1 - 0.3	6.7B	6B	1.35A	0.54	0.24	0.34	2.47D
	8H
	0.3 - 0.7	7.5B	55B	1.66E	4.98	1.52	4.29	15B	12.45D	28.60
	8.7H
	0.3 - 0.7	7.5B	55B	1.66E	4.98	1.52	4.29	15B	12.45D	28.60
	8.7H
	0.7 - 1.5	7.5B	94B	0.68E	4.63	1.39	6.17	14B	12.87D	44.07
	8.5H
	0.7 - 1.5	7.5B	94B	0.68E	4.63	1.39	6.17	14B	12.87D	44.07
	8.5H
	1.5 - 1.6	4.5B	150B	0.04H	2.63	0.34	2.23	0.3J	5.24D
	5H
	1.5 - 1.6	4.5B	150B	0.04H	2.63	0.34	2.23	0.3J	5.24D
	5H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.7D	110B	0.114E	5.8	4.8
	0 - 0.1	1.7D	110B	0.114E	5.8	4.8
	0.1 - 0.3	0.21D	27B	0.012E	4.1	3.9
	0.1 - 0.3	0.21D	27B	0.012E	4.1	3.9
	0.3 - 0.7	<2C	0.15D	40B	0.014E	9	41.3
	0.3 - 0.7	<2C	0.15D	40B	0.014E	9	41.3
	0.7 - 1.5	0.09D	44B	0.009E	6.2	35.4
	0.7 - 1.5	0.09D	44B	0.009E	6.2	35.4
	1.5 - 1.6	0.14D	26B	0.006E	2	46.3
	1.5 - 1.6	0.14D	26B	0.006E	2	46.3
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts

	Project Name:	Nyabing Kukerin land resourcs survey
	Project Code:	NYA	Site ID:	1024	Observation 	1
	Agency Name:	Agriculture Western Australia
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	18A1_NR	Bicarbonate-extractable potassium (not recorded)
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	4G_NR	pH buffering capacity, (method not recorded)
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A1	Total nitrogen - semimicro Kjeldahl, steam distillation
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1e	Nitrate-N, in presence of nitrite
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9B_NR	Bicarbonate-extractable phosphorus  (not recorded)
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)