Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0120	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Rohan Marold	Locality:
	Date Desc.:	12/03/97	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6224438 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	625294  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Rises
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	4 % 	Aspect:	No Data
	Surface Soil Condition 	Loose
	Erosion	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Hypocalcic Mottled-Mesonatric Yellow Sodosol     	Principal Profile Form:	Dy5.43
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments
	Profile Morphology
	Ap	0 - 0.14 m	Black (2.5Y2/2-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; Water repellent; Field pH 5 (pH meter); Abrupt change to - 
	A21e	0.14 - 0.52 m	Light brownish grey (10YR6/2-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Field pH 6 (pH meter); Abrupt, Wavy change to - 
	B21	0.52 - 0.85 m	Olive yellow (2.5Y6/6-Moist); , 0-0% ; Sandy light clay; Moderate grade of structure, 50-100 mm, 
	Columnar; Smooth-ped fabric; Dry; Very firm consistence; Common (10 - 20 %), Ferruginous, Medium 
	(2 -6 mm), Soft segregations; Field pH 8.4 (pH meter); Clear change to - 
	B3	0.85 - 1.25 m	Olive yellow (2.5Y6/6-Moist); , 10YR68, 10-20% , 5-15mm, Prominent; Sandy light clay; Weak grade of 
	structure, 5-10 mm, Polyhedral; Smooth-ped fabric; Dry; Firm consistence; Common (10 - 20 %), 
	Ferruginous, Medium (2 -6 mm), Soft segregations; Field pH 9.1 (pH meter); Gradual change to - 
	C	1.25 - 1.8 m	Light grey (2.5Y7/1-Moist); , 10YR68, 10-20% , 5-15mm, Prominent; Sandy clay loam; Single grain 
	grade of structure; Sandy (grains prominent) fabric; Dry; Weak consistence; Field pH 9.3 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Alkaline grey deep sandy duplex

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0120	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.5B	6B	2.4H	0.36	0.18	0.14	0.29J	3.08D
	5.5H
	0 - 0.15	4.5B	6B	2.4H	0.36	0.18	0.14	0.29J	3.08D
	5.5H
	0.15 - 0.5	5.6B	2B	0.88A	0.09	0.03	0.06	1.06D
	6.6H
	0.15 - 0.5	5.6B	2B	0.88A	0.09	0.03	0.06	1.06D
	6.6H
	0.5 - 0.55	7.1B	4B	1.93E	1.8	0.21	0.74	6B	4.68D	12.33
	8.9H
	0.5 - 0.55	7.1B	4B	1.93E	1.8	0.21	0.74	6B	4.68D	12.33
	8.9H
	0.55 - 0.7	7.5B	8B	4.39E	5.06	0.63	2.12	15B	12.2D	14.13
	9.1H
	0.55 - 0.7	7.5B	8B	4.39E	5.06	0.63	2.12	15B	12.2D	14.13
	9.1H
	0.7 - 1	7.6B	9B	2.72E	5.36	0.46	1.89	12B	10.43D	15.75
	9.2H	2.72E	5.36	0.46	1.89	12B	10.43D
	7.6B
	9.2H
	0.7 - 1	7.6B	9B	2.72E	5.36	0.46	1.89	12B	10.43D	15.75
	9.2H	2.72E	5.36	0.46	1.89	12B	10.43D
	7.6B
	9.2H
	0.7 - 1	7.6B	9B	2.72E	5.36	0.46	1.89	12B	10.43D	15.75
	9.2H	2.72E	5.36	0.46	1.89	12B	10.43D
	7.6B
	9.2H
	0.7 - 1	7.6B	9B	2.72E	5.36	0.46	1.89	12B	10.43D	15.75
	9.2H	2.72E	5.36	0.46	1.89	12B	10.43D
	7.6B
	9.2H
	1 - 1.3	7.7B	12B	2.66E	5.59	0.49	2.68	13B	11.42D	20.62
	9.3H
	1 - 1.3	7.7B	12B	2.66E	5.59	0.49	2.68	13B	11.42D	20.62
	9.3H
	1.3 - 1.6	7.9B	12B	1.42E	3.47	0.36	2.35	8B	7.6D	29.38
	9.4H
	1.3 - 1.6	7.9B	12B	1.42E	3.47	0.36	2.35	8B	7.6D	29.38
	9.4H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	0.88D	130B	3	3.4
	0 - 0.15	0.88D	130B	3	3.4
	0.15 - 0.5	0.12D	32B	1.4	1.9
	0.15 - 0.5	0.12D	32B	1.4	1.9
	0.5 - 0.55	<2C	0.11D	34B	5.5	22.3
	0.5 - 0.55	<2C	0.11D	34B	5.5	22.3

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0120	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.55 - 0.7	<2C	0.15D	31B	4.2	50.4
	0.55 - 0.7	<2C	0.15D	31B	4.2	50.4
	0.7 - 1	<2C	0.1D	24B	1.8	38.6
	<2C	0.1D	24B	1.8	38.6
	0.7 - 1	<2C	0.1D	24B	1.8	38.6
	<2C	0.1D	24B	1.8	38.6
	0.7 - 1	<2C	0.1D	24B	1.8	38.6
	<2C	0.1D	24B	1.8	38.6
	0.7 - 1	<2C	0.1D	24B	1.8	38.6
	<2C	0.1D	24B	1.8	38.6
	1 - 1.3	<2C	0.07D	22B	2.5	32.1
	1 - 1.3	<2C	0.07D	22B	2.5	32.1
	1.3 - 1.6	<2C	0.03D	19B	2.7	28.8
	1.3 - 1.6	<2C	0.03D	19B	2.7	28.8
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0120	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)