Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0350	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Rohan Marold	Locality:
	Date Desc.:	11/03/97	Elevation:	272 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6228706 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	600504  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition 	Soft
	Erosion	 (wind);  (scald)  (sheet)  (rill)  (mass)  (gully)  
	(stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	Dy5.42
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.12 m	Very dark grey (7.5YR3/1-Moist); ; Loamy sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Very few (0 - 2 %), Ferruginous, Fine (0 - 2 mm), 
	Concretions; Water repellent; Field pH 5.3 (pH meter); Abrupt change to - 
	A21	0.12 - 0.25 m	Light olive brown (2.5Y5/4-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Common (10 - 20 %), Ferruginous, Medium (2 -6 mm), 
	Concretions; Field pH 5.3 (pH meter); Clear change to - 
	A22	0.25 - 0.53 m	Light brownish grey (2.5Y6/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Many (20 - 50 %), Ferruginous, Medium (2 -6 mm), 
	Concretions; Field pH 7.6 (pH meter); Clear change to - 
	B21	0.53 - 0.63 m	Pale olive (5Y6/3-Moist); , 7.5YR68, 10-20% , 5-15mm, Prominent; Sandy light clay; Weak grade of 
	structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Very firm consistence; Common (10 - 20 %), 
	Ferruginous, Medium (2 -6 mm), Soft segregations; Field pH 7 (pH meter); Gradual change to - 
	B22	0.63 - 1.15 m	Pale yellow (2.5Y7/3-Moist); , 7.5YR78, 10-20% , 5-15mm, Prominent; Light clay; Weak grade of 
	structure, 5-10 mm, Subangular blocky; Smooth-ped fabric; Firm consistence; Common (10 - 20 %), 
	Ferruginous, Medium (2 -6 mm), Soft segregations; Field pH 7.6 (pH meter); Gradual change to - 
	C	1.15 - 1.65 m	White (2.5Y8/1-Moist); , 2.5Y68, 10-20% , 5-15mm, Prominent; Sandy clay loam; Single grain grade of 
	structure; Sandy (grains prominent) fabric; Weak consistence; Common (10 - 20 %), Ferruginous, 
	Medium (2 -6 mm), Soft segregations; Field pH 7.8 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	Grey deep sandy duplex--sand/gravel/clay

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0350	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4.1B	7B	1.16H	0.22	0.13	0.14	0.38J	1.65D
	5H
	0 - 0.1	4.1B	7B	1.16H	0.22	0.13	0.14	0.38J	1.65D
	5H
	0.1 - 0.25	4.2B	5B	0.6H	0.17	0.08	0.18	0.35J	1.03D
	5H
	0.1 - 0.25	4.2B	5B	0.6H	0.17	0.08	0.18	0.35J	1.03D
	5H
	0.25 - 0.5	5.4B	12B	0.87H	0.63	0.08	0.55	0.03J	2.13D
	6.3H
	0.25 - 0.5	5.4B	12B	0.87H	0.63	0.08	0.55	0.03J	2.13D
	6.3H
	0.5 - 0.8	6.6B	120B	1.54A	4.08	0.64	2.36	8.62D
	7.1H
	0.5 - 0.8	6.6B	120B	1.54A	4.08	0.64	2.36	8.62D
	7.1H
	0.8 - 1.1	7.8B	93B	1.06E	2.82	0.51	2.68	8B	7.07D	33.50
	8.7H
	0.8 - 1.1	7.8B	93B	1.06E	2.82	0.51	2.68	8B	7.07D	33.50
	8.7H
	1.1 - 1.4	7.8B	67B	0.68E	2.18	0.41	2.23	6B	5.5D	37.17
	8.8H
	1.1 - 1.4	7.8B	67B	0.68E	2.18	0.41	2.23	6B	5.5D	37.17
	8.8H
	1.4 - 1.8	7.7B	50B	0.59E	2.04	0.34	2.32	5B	5.29D	46.40
	8.7H
	1.4 - 1.8	7.7B	50B	0.59E	2.04	0.34	2.32	5B	5.29D	46.40
	8.7H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.94D	89B	3.2	4.6
	0 - 0.1	0.94D	89B	3.2	4.6
	0.1 - 0.25	0.3D	43B	2.6	5.3
	0.1 - 0.25	0.3D	43B	2.6	5.3
	0.25 - 0.5	0.21D	36B	2.4	7.2
	0.25 - 0.5	0.21D	36B	2.4	7.2
	0.5 - 0.8	0.32D	49B	5.5	44.6
	0.5 - 0.8	0.32D	49B	5.5	44.6
	0.8 - 1.1	<2C	0.14D	34B	4.1	40.1
	0.8 - 1.1	<2C	0.14D	34B	4.1	40.1
	1.1 - 1.4	<2C	0.06D	25B	1.7	31.5
	1.1 - 1.4	<2C	0.06D	25B	1.7	31.5
	1.4 - 1.8	<2C	0.05D	20B	1.7	27.1
	1.4 - 1.8	<2C	0.05D	20B	1.7	27.1
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0350	Observation 	1
	Agency Name:	Agriculture Western Australia
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)