Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0551	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Rohan Marold	Locality:
	Date Desc.:	11/03/97	Elevation:	230 metres
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6229798 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	609910  Datum: AGD84	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesonatric Brown Sodosol     	Principal Profile Form:	Dy4.22
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data and little or no knowledge of this soil.
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subrounded, Gravel; No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.1 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains prominent)
	 fabric; Dry; Loose consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Concretions; Field pH 
	4.7 (pH meter); Abrupt change to - 
	A21c	0.1 - 0.21 m	Brown (10YR4/3-Moist); , 0-0% ; Loamy sand; Single grain grade of structure; Sandy (grains prominent)
	 fabric; Dry; Loose consistence; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Concretions; 
	Field pH 4.7 (pH meter); Clear change to - 
	A22c	0.21 - 0.37 m	Light olive brown (2.5Y5/4-Moist); , 0-0% ; Sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Dry; Loose consistence; Very many (50 - 100 %), Ferruginous, Coarse (6 - 20 mm), 
	Concretions; Field pH 5.7 (pH meter); Abrupt, Wavy change to - 
	B21c	0.37 - 0.55 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Clay loam; Weak grade of structure, 2-5 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Loose consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), 
	Concretions; Field pH 5.9 (pH meter); Gradual change to - 
	B22c	0.55 - 0.95 m	Light olive brown (2.5Y5/6-Moist); , 0-0% ; Clay loam; Weak grade of structure, 2-5 mm, Polyhedral; 
	Smooth-ped fabric; Dry; Loose consistence; Few (2 - 10 %), Ferruginous, Medium (2 -6 mm), Soft 
	segregations; Field pH 5.9 (pH meter); Gradual change to - 
	B3	0.95 - 1.3 m	Olive yellow (2.5Y6/6-Moist); , 0-0% ; Clay loam; Weak grade of structure, 2-5 mm, Polyhedral; Smooth-
	ped fabric; Dry; Loose consistence; Common (10 - 20 %), Ferruginous, Coarse (6 - 20 mm), Soft 
	segregations; Field pH 6.4 (pH meter); Gradual change to - 
	C	1.3 - 1.7 m	Olive yellow (2.5Y6/8-Moist); , 0-0% ; Clay loam; Dry; Loose consistence; Many (20 - 50 %), 
	Ferruginous, Coarse (6 - 20 mm), Soft segregations; Very few (0 - 2 %), Calcareous, Very coarse (20 - 
	60 mm), Concretions; Field pH 6.4 (pH meter); 
	Morphological Notes
	Ap	         
	A21c	         
	A22c	         
	B21c	         
	B22c	         
	B3	         
  C	         
	Observation Notes
	Site Notes
	Gently undulating plain area high in the landscape with some gravel areas.  Sandy gravel/gravelly loam.   

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0551	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	4B	6B	0.71H	0.22	0.16	0.13	0.4J	1.22D
	4.9H
	0 - 0.1	4B	6B	0.71H	0.22	0.16	0.13	0.4J	1.22D
	4.9H
	0.1 - 0.4	4.3B	2B	0.58H	0.15	0.06	0.03	0.19J	0.82D
	5.3H
	0.1 - 0.4	4.3B	2B	0.58H	0.15	0.06	0.03	0.19J	0.82D
	5.3H
	0.4 - 0.55	6B	6B	6.25A	3.61	0.15	0.36	10.37D
	6.8H
	0.4 - 0.55	6B	6B	6.25A	3.61	0.15	0.36	10.37D
	6.8H
	0.55 - 0.85	6B	6B	6.76A	4	0.16	0.35	11.27D
	6.7H
	0.55 - 0.85	6B	6B	6.76A	4	0.16	0.35	11.27D
	6.7H
	0.85 - 1.05	6.1B	6B	8.82A	4.34	0.14	0.49	13.79D
	6.9H	8.82A	4.34	0.14	0.49	13.79D
	6.1B
	6.9H
	0.85 - 1.05	6.1B	6B	8.82A	4.34	0.14	0.49	13.79D
	6.9H	8.82A	4.34	0.14	0.49	13.79D
	6.1B
	6.9H
	0.85 - 1.05	6.1B	6B	8.82A	4.34	0.14	0.49	13.79D
	6.9H	8.82A	4.34	0.14	0.49	13.79D
	6.1B
	6.9H
	0.85 - 1.05	6.1B	6B	8.82A	4.34	0.14	0.49	13.79D
	6.9H	8.82A	4.34	0.14	0.49	13.79D
	6.1B
	6.9H
	1.05 - 1.35	6.8B	6B	11.01A	4.2	0.18	0.56	15.95D
	7.8H
	1.05 - 1.35	6.8B	6B	11.01A	4.2	0.18	0.56	15.95D
	7.8H
	1.35 - 1.75	7.2B	6B	8.63E	2.41	0.19	0.46	16B	11.69D	2.88
	8.2H
	1.35 - 1.75	7.2B	6B	8.63E	2.41	0.19	0.46	16B	11.69D	2.88
	8.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	0.88D	130B	2.8	3.5
	0 - 0.1	0.88D	130B	2.8	3.5
	0.1 - 0.4	0.21D	53B	2.9	3.4
	0.1 - 0.4	0.21D	53B	2.9	3.4
	0.4 - 0.55	0.18D	54B	4.7	49
	0.4 - 0.55	0.18D	54B	4.7	49

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0551	Observation 	1
	Agency Name:	Agriculture Western Australia
	0.55 - 0.85	0.11D	44B	6.1	50.1
	0.55 - 0.85	0.11D	44B	6.1	50.1
	0.85 - 1.05	0.1D	41B	8.5	49.2
	0.1D	41B	8.5	49.2
	0.85 - 1.05	0.1D	41B	8.5	49.2
	0.1D	41B	8.5	49.2
	0.85 - 1.05	0.1D	41B	8.5	49.2
	0.1D	41B	8.5	49.2
	0.85 - 1.05	0.1D	41B	8.5	49.2
	0.1D	41B	8.5	49.2
	1.05 - 1.35	0.11D	39B	7.4	44.5
	1.05 - 1.35	0.11D	39B	7.4	44.5
	1.35 - 1.75	<2C	0.07D	36B	7.8	38.4
	1.35 - 1.75	<2C	0.07D	36B	7.8	38.4
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15C1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for 
	soluble salts
	15C1_CEC	CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_K	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_MG	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15C1_NA	Exchangeable bases and CEC - alcoholic 1M ammonium chloride at pH 8.5, pretreatment for soluble salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	19B_NR	Calcium Carbonate (CaCO3) - Not recorded
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_gt2m	> 2mm particle size analysis, (method not recorded)

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	0551	Observation 	1
	Agency Name:	Agriculture Western Australia
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)