Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1381	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	25/05/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6222215 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	566666  Datum: AGD84	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Scald	Slope Category:	No Data
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Firm, Hardsetting
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Sodosolic Salic Hydrosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments; No surface coarse fragments
	Profile Morphology
	A1p	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moist; Loose consistence; Clear, Wavy change to - 
	B21	0.1 - 0.15 m	Greyish brown (2.5Y5/3-Moist); ; Sandy medium clay; Weak grade of structure, Columnar; Sandy (grains 
	prominent) fabric; Moist; Weak consistence; Clear, Irregular change to - 
	B22	0.15 - 0.3 m	Light brownish grey (2.5Y6/3-Moist); ; Sandy medium clay; Weak grade of structure, Columnar; Sandy 
	(grains prominent) fabric; Moist; Weak consistence; Clear, Wavy change to - 
	B23	0.3 - 0.5 m	Light brownish grey (2.5Y6/2-Moist); ; Fine sandy medium clay; Massive grade of structure; Sandy 
	(grains prominent) fabric; Moist; Weak consistence; Clear, Irregular change to - 
	B24	0.5 - 0.9 m	Light brownish grey (2.5Y6/3-Moist); , 10YR68, 2-10% , 5-15mm, Faint; Fine sandy medium clay; 
	Massive grade of structure; Sandy (grains prominent) fabric; Moist; Weak consistence; Clear, Smooth 
	change to - 
	B25	0.9 - 1 m	Light brownish grey (2.5Y6/3-Moist); , 10YR68, 2-10% , 5-15mm, Faint; Medium clay; Massive grade of 
	structure; Moist; Firm consistence; Abrupt, Smooth change to - 
	B31t	1 - 1.4 m	Grey (2.5Y6/1-Moist); , 10YR68, 10-20% , 15-30mm, Distinct; , 5YR46, 10-20% , 15-30mm, Prominent; 
	Medium clay; Massive grade of structure; Moist; Firm consistence; 10-20%, fine gravelly, 2-6mm, 
	subrounded, Ironstone, coarse fragments; Abrupt, Wavy change to - 
	B32	1.4 - 1.6 m	Grey (2.5Y6/1-Moist); , 10YR68, 10-20% , 15-30mm, Prominent; Medium clay; Weak grade of structure, 
	2-5 mm, Subangular blocky; Sandy (grains prominent) fabric; Wet; Weak consistence; 2-10%, fine 
	gravelly, 2-6mm, subrounded, Ironstone, coarse fragments; Sharp, Smooth change to - 
	Cm	1.6 -  m	; 
	Morphological Notes
	Observation Notes
	Site Notes
	Pit site on saline scald. Pit located where site TBO #0875 done. Pit completely filled with water after 2 days rain.

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1381	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2B	110A	3.63A	4.94	0.39	2.87	11.83D
	6.9A
	0.1 - 0.15	5.8B	120A	2.24A	6.38	0.4	4.48	13.5D
	6.5A
	0.15 - 0.3	6.5B	91A	1.57A	5.43	0.49	7.53	15.02D
	7.4A
	0.3 - 0.5	6.7B	120A	1.1A	5.95	0.63	6.83	14.51D
	7.6A
	0.5 - 0.9	6B	140A	0.6A	5.2	0.6	6.88	13.28D
	6.6A
	0.9 - 1	4.6B	140A	0.43H	4.4	0.37	6.02	0.04J	11.22D
	5.2A
	1 - 1.4	4.3B	190A	0.34H	4.44	0.32	6.06	0.09J	11.16D
	4.7A
	1.4 - 1.6	4.3B	240A	0.22H	3.28	0.22	3.25	0.05J	6.97D
	4.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	1.9A	6.8	15.7
	0.1 - 0.15	0.59A	5	30.5
	0.15 - 0.3	0.31A	5.3	33.5
	0.3 - 0.5	0.14A	5.9	35.9
	0.5 - 0.9	0.1A	6.1	38.5
	0.9 - 1	0.1A	6.8	39
	1 - 1.4	0.09A	14.3	57.2
	1.4 - 1.6	0.1A	9.1	28.1
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1381	Observation 	1
	Agency Name:	Agriculture Western Australia
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_AL	Aluminium in 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9A_S14	Total element - P(%) method S14 CCWA
	9I1	Phosphate sorption index
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75a	20 to 75u particle size analysis, (arithmetic difference)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)