Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1385	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	31/05/99	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6195418 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	548265  Datum: AGD84	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	270 degrees
	Surface Soil Condition 	Firm
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Subnatric Grey Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Cultivation. Rainfed
	Vegetation
	Surface Coarse Fragments	10-20%, medium gravelly, 6-20mm, subrounded, Ironstone; 2-10%, cobbly, 60-200mm, subrounded, Ironstone
	Profile Morphology
	A1p	0 - 0.1 m	Very dark greyish brown (10YR3/2-Moist); ; Loamy fine sand; Moist; Loose consistence; 20-50%, fine 
	gravelly, 2-6mm, subrounded, Ironstone, coarse fragments; Abrupt, Smooth change to - 
	A21c	0.1 - 0.4 m	Yellowish brown (10YR5/4-Moist); ; Loamy fine sand; Moist; Loose consistence; 50-90%, medium 
	gravelly, 6-20mm, subrounded, Ironstone, coarse fragments; Abrupt, Smooth change to - 
	B21t	0.4 - 0.8 m	Greyish brown (2.5Y5/3-Moist); , 7.5YR58, 20-50% , 5-15mm, Distinct; Medium clay; Weak grade of 
	structure, <2 mm, Subangular blocky; Wet; Very weak consistence; Clear, Smooth change to - 
	B22	0.8 - 1 m	Light brownish grey (2.5Y6/3-Moist); , 2.5YR36, 10-20% , 15-30mm, Prominent; Medium clay; Weak 
	grade of structure, 2-5 mm, Subangular blocky; Wet; Very weak consistence; 
	Morphological Notes
	Observation Notes
	Site Notes
	Soil pit began getting water seeping into it shortly after being excavated - water standing at 80cm - pit originally approx. 160 - 180cm deep. 
	Samples taken from upper surfaces & auger hole adjacent to pit. Pit dug where site TBO #1080 done

	Project Name:	Tambellup Borden land resources survey
	Project Code:	TBO	Site ID:	1385	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.1B	29A	13.49H	2.68	0.47	0.3	0.1J	16.94D
	5.7A
	0.1 - 0.4	4.9B	3A	1.58H	0.44	0.03	0.04	0.1J	2.09D
	5.9A
	0.4 - 0.8	4.9B	10A	2.75H	5.1	0.1	0.54	0.09J	8.49D
	5.7A
	0.8 - 0.9	4.2B	15A	1.1H	5.13	0.04	0.87	0.46J	7.14D
	4.9A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	5.84A	4.9	3
	0.1 - 0.4	0.58A	5.3	5.5
	0.4 - 0.8	0.43A	3.4	66.7
	0.8 - 0.9	0.19A	3.1	65.9
	Laboratory Analyses Completed for this profile
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B_AL	Aluminium in 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1	Organic carbon - Walkley and Black
	9A_S14	Total element - P(%) method S14 CCWA
	9I1	Phosphate sorption index
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75a	20 to 75u particle size analysis, (arithmetic difference)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)