Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0788	Observation ID:	1
	Agency Name:	Agriculture Western Australia
	Site Information
	Desc. By:	Angela Stuart-Street	Locality:
	Date Desc.:	10/12/98	Elevation:	No Data
	Map Ref.:	Rainfall:	No Data
	Northing/Long.:	6205476 AMG zone: 50	Runoff:	No Data
	Easting/Lat.:	491821  Datum: AGD84	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating rises 9-30m  1-3%	Pattern Type:	Rises
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	2 % 	Aspect:	90 degrees
	Surface Soil Condition 	Firm
	Erosion	 (wind);  (scald)  (sheet)  (wave)  (rill)  (mass)  
	(gully)  (stbank)  (tunnel) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric-Sodic Mesotrophic Yellow Dermosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Confidence level not specified
	Site Disturbance	Complete clearing. Pasture, native or improved, cultivated at some stage
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A1p	0 - 0.15 m	Black (10YR2/1-Moist); , 0-0% ; Sandy loam; Single grain grade of structure; Sandy (grains prominent) 
	fabric; Dry; Loose consistence; 20-50%, medium gravelly, 6-20mm, subrounded, Ironstone, coarse 
	fragments; Water repellent; Clear, Wavy change to - 
	B1c	0.15 - 0.35 m	Yellowish brown (10YR5/8-Moist); , 0-0% ; Clay loam, sandy; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Moderately moist; 20-50%, medium gravelly, 6-20mm, subrounded, Ironstone, 
	coarse fragments; Clear, Smooth change to - 
	B21	0.35 - 0.55 m	Brownish yellow (10YR6/8-Moist); , 2.5YR58, 2-10% , 0-5mm, Distinct; Light clay; Massive grade of 
	structure; Sandy (grains prominent) fabric; Moderately moist; Clear, Smooth change to - 
	B22t	0.55 - 0.8 m	Brownish yellow (10YR6/8-Moist); , 2.5YR48, 20-50% , 0-5mm, Distinct; Medium clay; Moderate grade 
	of structure, 2-5 mm, Angular blocky; Smooth-ped fabric; Moderately moist; Clear, Wavy change to - 
	B31	0.8 - 1.15 m	White (10YR8/1-Moist); , 2.5YR48, 10-20% , 0-5mm, Prominent; , 10YR58, 2-10% , 0-5mm, Distinct; 
	Light clay; Moderate grade of structure, <2 mm, Angular blocky; Smooth-ped fabric; Moderately moist; 
	Gradual, Smooth change to - 
	B32	1.15 - 1.3 m	White (10YR8/1-Moist); , 2.5Y72, 2-10% , 0-5mm, Distinct; , 10YR66, 10-20% , 0-5mm, Distinct; Light 
	clay; Weak grade of structure, <2 mm, Angular blocky; Rough-ped fabric; Moderately moist; 
	Morphological Notes
	B21	Soil very porous
	Observation Notes
	Site Notes
	on midslope of rise.

	Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0788	Observation 	1
	Agency Name:	Agriculture Western Australia
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.15	4.6B	5B	6.33H	0.71	0.05	0.29	1.45J	7.38D
	5.5H
	0.15 - 0.35	5.7B	2B	3.66A	1.66	0.05	15	20.37D
	6.8H
	0.35 - 0.55	6B	4B	2.02A	2.71	0.02	0.14	4.89D
	6.8H
	0.55 - 0.8	6B	4B	0.7A	3.58	0.02	0.2	4.5D
	6.5H
	0.8 - 1.15	5.2B	6B	0.37H	3.47	<0.02	0.33	4.18D
	5.8H
	1.15 - 1.3	4.5B	10B	0.27H	3.39	<0.02	0.68	0.3J	4.35D
	5.2H
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.15	6.65D	450B	10.3	3.6
	0.15 - 0.35	1.03D	79B	9.9	18.8
	0.35 - 0.55	0.39D	42B	7.8	61.8
	0.55 - 0.8	0.18D	40B	8.6	72
	0.8 - 1.15	0.17D	48B	8.7	66.9
	1.15 - 1.3	0.13D	28B	20.8	51.1
	Laboratory Analyses Completed for this profile
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_BSa	Exchangeable bases (Ca++) - meq per 100g of soil - Auto calculated from available
	15_NR_CMR	Exchangeable bases (Ca/Mg ratio) - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MN	Exchangeable bases (Mn++) - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_CEC	Exchangeable bases (CEC) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15E1_AL	Exchangeable Al - by compulsive exchange, no pretreatment for soluble salts
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble salts
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MN	Exchangeable bases (Mn2+) by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15J_BASES	Sum of Bases
	15L1_a	Exchangeable bases Base saturation percentage (BSP) - Auto calculated from available using Sum of Cations
	 and measured clay
	15N1_a	Exchangeable sodium percentage (ESP) - Auto calculated from available using CEC
	15N1_b	Exchangeable sodium percentage (ESP) - Auto calculated from available using Sum of Cations
	3_NR	Electrical conductivity or soluble salts - Not recorded
	4_NR	pH of soil - Not recorded

	Project Name:	Tonebridge land resources survey
	Project Code:	TON	Site ID:	0788	Observation 	1
	Agency Name:	Agriculture Western Australia
	4B_AL_NR	Aluminium in 1:5 soil/0.01M calcium chloride extract - method not recorded
	4B1	pH of 1:5 soil/0.01M calcium chloride extract - direct
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	9A3	Total Phosphorus (ppm) - semimicro kjeldahl, automated colour
	9H1	Anion storage capacity
	P10_1m2m	1000 to 2000u particle size analysis, (method not recorded)
	P10_20_75	20 to 75u particle size analysis, (method not recorded)
	P10_75_106	75 to 106u particle size analysis, (method not recorded)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_Saa	Sand (%) - Not recorded arithmetic difference, auto generated
	P10_NR_Z	Silt (%) - Not recorded
	P10106_150	106 to 150u particle size analysis, (method not recorded)
	P10150_180	150 to 180u particle size analysis, (method not recorded)
	P10180_300	180 to 300u particle size analysis, (method not recorded)
	P10300_600	300 to 600u particle size analysis, (method not recorded)
	P106001000	600 to 1000u particle size analysis, (method not recorded)