Project Name:	BUS
	Project Code:	BUS	Site ID:	P325	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	2KM south from Vasse School:
	Date Desc.:	07/03/57	Elevation:	 9 metres
	Map Ref.:	Sheet No. : 1930   1:100000	Rainfall:	0
	Northing/Long.:	115.244722222222	Runoff:	Slow
	Easting/Lat.:	-33.6944444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Petroferric Grey Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.08 m	Grey (10YR5/1-Moist); ; Sand (Fibric); Single grain grade of structure; Diffuse, Smooth change to
	 - 
	A2	0.08 - 0.2 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Diffuse, Smooth change to - 
	A3	0.2 - 0.61 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Loose 
	consistence; Diffuse, Smooth change to - 
	A4	0.61 - 0.76 m	Light brownish grey (10YR6/2-Moist); ; Sand; Massive grade of structure; Diffuse, Smooth 
	change to - 
	AB	0.76 - 1.17 m	Light grey (10YR7/1-Moist); , 10YR56; Sand; Diffuse, Smooth change to - 
	B	1.17 - 1.57 m	Light grey (10YR7/1-Moist); , 10YR56; Sandy clay loam (Heavy); Moist; Weak consistence; 
	Morphological Notes
	Observation Notes
	>157CM ON IRON PAN:                                                                                                     
	Site Notes
	SUSSEX

	Project Name:	BUS
	Project Code:	BUS	Site ID:	P325	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.08	5.5A	 0.036A	 2K	 0.7	 0.06	 0.07	 8.1E	 10.9B
	0.08 - 0.2	5.5A	 0.018A
	0.2 - 0.61	5.7A	 0.018A
	0.61 - 0.76	5.8A	 0.021A	 0.1K	 0.4	<0.01	 0.03	 1.6E	 2.2B
	0.76 - 1.17	6.4A	 0.027A
	1.17 - 1.57	5.9A	 0.08A	 1.3K	 3	<0.01	 0.27	 3.1E	 7.7B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.08	 2.44D	 0.004D	 0.108B	 51D	 39	 5	 1
	0.08 - 0.2
	0.2 - 0.61
	0.61 - 0.76
	0.76 - 1.17	 0.001D	 64D	 31	 7	 1
	1.17 - 1.57	 0.002D	 27D	 12	 11	 46
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.08
	0.08 - 0.2
	0.2 - 0.61
	0.61 - 0.76
	0.76 - 1.17
	1.17 - 1.57

	Project Name:	BUS
	Project Code:	BUS	Site ID:	P325	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance