Project Name:	BUS
	Project Code:	BUS	Site ID:	P330	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	Location 716 20 chains from south boundary along 
	Ironstone Gully Creek:
	Date Desc.:	08/03/57	Elevation:	 305 metres
	Map Ref.:	Sheet No. : 1930   1:100000	Rainfall:	0
	Northing/Long.:	115.249444444444	Runoff:	Slow
	Easting/Lat.:	-33.7455555555556	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.99 m deep,Unconsolidated 
	material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Eutrophic Yellow Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Brown podzolic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.1 m	Brown (10YR5/3-Moist); ; Sandy loam (Fibric); Single grain grade of structure; Diffuse, Smooth 
	change to - 
	0.1 - 0.46 m	Brown (10YR4/3-Moist); ; Sandy loam; 2-10%, Substrate material, coarse fragments; Many
	0.46 - 0.69 m	Brownish yellow (10YR6/8-Moist); ; Sandy clay loam; 2-10%, Substrate material, coarse 
	fragments; 
	0.69 - 0.84 m	Yellow (10YR8/6-Moist); , 10YR68; Sandy medium clay; Weak consistence; 2-10%, Substrate 
	material, coarse fragments; 
	0.84 - 0.99 m	Yellow (10YR8/6-Moist); , 10YR68; Sandy medium clay; 50-90%, Substrate material, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	>99CM ON FERRUGINOUS ROCK:                                                                                              
	Site Notes
	SUSSEX

	Project Name:	BUS
	Project Code:	BUS	Site ID:	P330	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.1A	 0.054A	 1.7K	 1.1	 0.18	 0.07	 8.6E	 11.7B
	0.1 - 0.46	6.6A	 0.042A
	0.46 - 0.69	6.8A	 0.042A
	0.69 - 0.84	6.4A	 0.045A
	0.84 - 0.99	6.6A	 0.074A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 1.99D	 0.012D	 0.154B	 21D	 65	 8	 5
	0.1 - 0.46	 0.055B
	0.46 - 0.69	 16D	 57	 6	 16
	0.69 - 0.84
	0.84 - 0.99	 0.002D	 15D	 54	 8	 21
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.46
	0.46 - 0.69
	0.69 - 0.84
	0.84 - 0.99

	Project Name:	BUS
	Project Code:	BUS	Site ID:	P330	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance