Project Name:	CAP
	Project Code:	CAP	Site ID:	P153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	On Lowrie Road 5 chains east from south east corner
	 of location 76:
	Date Desc.:	22/04/53	Elevation:	No Data
	Map Ref.:	Sheet No. : 2030   1:100000	Rainfall:	0
	Northing/Long.:	115.6625	Runoff:	No Data
	Easting/Lat.:	-33.5247222222222	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Subnatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - , , Closed or dense. *Species includes - Danthonia species
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.11 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Fibric); Single grain grade of structure; Loose 
	consistence; 2-10%, fine gravelly, 2-6mm, Gravel, coarse fragments; Field pH 6 (pH meter); 
	Clear, Smooth change to - 
	A2	0.11 - 0.22 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Loose consistence; 2-
	10%, fine gravelly, 2-6mm, Gravel, coarse fragments; Field pH 6.5 (pH meter); Clear, Smooth 
	change to - 
	B	0.22 - 0.41 m	Brownish yellow (10YR6/6-Moist); ; Sandy medium clay; Massive grade of structure; Dry; Loose 
	consistence; 10-20%, fine gravelly, 2-6mm, Gravel, coarse fragments; Field pH 6.5 (pH meter); 
	Diffuse, Smooth change to - 
	0.41 - 0.69 m	Yellow (10YR7/8-Moist); ; Sandy loam; Massive grade of structure; Weak consistence; 20-50%, 
	fine gravelly, 2-6mm, Gravel, coarse fragments; Field pH 6.5 (pH meter); Clear, Irregular change 
	to - 
	0.69 - 0.96 m	Yellow (10YR7/8-Moist); , 10YR56; Sandy clay loam; Massive grade of structure; Weak 
	consistence; 10-20%, fine gravelly, 2-6mm, Gravel, coarse fragments; Many (20 - 50 %), 
	Ferruginous, , ; Field pH 7 (pH meter); Clear, Smooth change to - 
	0.96 - 1.42 m	Grey (10YR6/1-Moist); , 5Y62; , 10YR56; Sandy medium clay; Massive grade of structure; Weak 
	consistence; Few (2 - 10 %), Ferruginous, , ; Field pH 7 (pH meter); Sharp, Smooth change to - 
	1.42 - 2.01 m	Light grey (10YR7/1-Moist); , 10YR68; Heavy clay; Massive grade of structure; Weak 
	consistence; Moderately plastic; Normal plasticity; Very many (50 - 100 %), Ferruginous, , ; Field
	 pH 7 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	DONNYBROOK

	Project Name:	CAP
	Project Code:	CAP	Site ID:	P153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.11	6.4A	 0.074A	 2.9K	 2.4	 0.32	 0.13
	0.11 - 0.22	6.9A	 0.039A
	0.22 - 0.41	6.5A	 0.057A	 0.9K	 1	 0.16	 0.38	 2E	 4.4B
	0.41 - 0.69	5.7A	 0.161A	 0.4K	 1.3	 0.04	 0.2	 2.1E	 4B
	0.69 - 0.96	6.2A	 0.179A
	0.96 - 1.42	6A	 0.295A
	1.42 - 2.01	5.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.11	 1.8D	 0.01D	 0.105B	 7	 63D	 25	 3	 6
	0.11 - 0.22
	0.22 - 0.41	 0.005D	 14	 50D	 29	 4	 17
	0.41 - 0.69	 26	 44D	 24	 1	 19
	0.69 - 0.96
	0.96 - 1.42
	1.42 - 2.01
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.11
	0.11 - 0.22
	0.22 - 0.41
	0.41 - 0.69
	0.69 - 0.96
	0.96 - 1.42
	1.42 - 2.01

	Project Name:	CAP
	Project Code:	CAP	Site ID:	P153	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance