Project Name:	CAP
	Project Code:	CAP	Site ID:	P185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	On road No. 1915 adjacent to Loc. 221:on slight 
	ridge between swales:
	Date Desc.:	26/08/53	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	115.554166666667	Runoff:	Rapid
	Easting/Lat.:	-33.5075	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Sand plain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Fragic Sesquic Aeric Podosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.04 m	Dark greyish brown (10YR4/2-Moist); ; Sand (Fibric); Single grain grade of structure; Dry; Loose 
	consistence; Field pH 7 (pH meter); Diffuse, Smooth change to - 
	A2	0.04 - 0.3 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; Field pH 7 (pH meter); Diffuse, Irregular change to - 
	A3	0.3 - 0.79 m	Brown (10YR4/3-Moist); ; Sand; Single grain grade of structure; Dry; Loose consistence; Field 
	pH 7 (pH meter); Diffuse, Smooth change to - 
	0.79 - 2.13 m	Strong brown (7.5YR5/6-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	B	2.13 - 3.17 m	Brownish yellow (10YR6/6-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; Field pH 7 (pH meter); 
	Morphological Notes
	Observation Notes
	HEAVY VEINS THROUGHOUT PROFILE (MORE WITH DEPTH):                                                                       
	Site Notes
	SOUTH-WEST LD

	Project Name:	CAP
	Project Code:	CAP	Site ID:	P185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	7.7A	 6.3K	 1.3	 0.06	 0.1
	0.04 - 0.3	7.6A	 0.61K	 0.8	 0.05	 0.1
	0.3 - 0.79	7.5A
	0.79 - 2.13	7.6A
	2.13 - 3.17	7.7A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04	 0.757D	 82D	 13	 1	 2
	0.04 - 0.3	 0.556D	 81D	 14	 1	 2
	0.3 - 0.79	 0.656D
	0.79 - 2.13	 0.505D
	2.13 - 3.17	 0.313D
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.3
	0.3 - 0.79
	0.79 - 2.13
	2.13 - 3.17

	Project Name:	CAP
	Project Code:	CAP	Site ID:	P185	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	4A1	pH of 1:5 soil/water suspension
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance