Project Name:	COB
	Project Code:	COB	Site ID:	P707	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	13KM east of Jarrahdale: Forest Dept. map sheet ref. 
	BR70 (25M on 21 degrees from E3900-N4350):
	Date Desc.:	22/10/80	Elevation:	 310 metres
	Map Ref.:	Sheet No. : 2133   1:100000	Rainfall:	1200
	Northing/Long.:	116.183333333333	Runoff:	Rapid
	Easting/Lat.:	-32.3166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	8 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Chromosol     	Principal Profile Form:	Dy5.61
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:	10-20%, , , Substrate material
	Profile Morphology
	A11	0 - 0.05 m	Dark brown (10YR3/3-Moist); ; Loamy sand; Single grain grade of structure; 90-100%, medium 
	gravelly, 6-20mm, angular, Substrate material, coarse fragments; Gradual, Smooth change to - 
	A12	0.05 - 0.1 m	Dark yellowish brown (10YR4/4-Moist); ; Loamy sand; Single grain grade of structure; 50-90%, 
	medium gravelly, 6-20mm, angular, Substrate material, coarse fragments; 
	A13	0.1 - 0.2 m	Dark yellowish brown (10YR4/4-Moist); ; Loamy sand; Single grain grade of structure; 50-90%, 
	medium gravelly, 6-20mm, angular, Substrate material, coarse fragments; 
	A21	0.2 - 0.3 m	Brown (7.5YR4/4-Moist); ; Loamy sand; Single grain grade of structure; 50-90%, medium 
	gravelly, 6-20mm, angular, Substrate material, coarse fragments; 
	A22A3	0.3 - 0.44 m	Yellowish red (5YR5/6-Moist); ; Sandy loam; Massive grade of structure; 
	B1	0.44 - 0.5 m	Yellowish red (5YR5/6-Moist); , 5YR58; Sandy clay loam (Heavy); 
	B21	0.5 - 0.6 m	Yellowish red (5YR5/8-Moist); , 2.5YR36, 10-20% ; , 10-20% ; Medium clay; 
	B22	0.6 - 0.8 m	Yellowish red (5YR5/8-Moist); , 2.5YR36, 20-50% , Distinct; , 20-50% , Distinct; Medium clay; 
	20-50%, Substrate material, coarse fragments; 
	B22	0.8 - 1 m	Yellowish red (5YR5/8-Moist); , 2.5YR36, 20-50% , Distinct; , 20-50% , Distinct; Sandy clay 
	loam; 20-50%, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-30CM AL GV IS FERRUGINOUS: 60-100CM DR MOTTLES HARDENED TO FORM INCIPIENT FERRUGINOUS GRAVEL:        
	                 
	Site Notes

	Project Name:	COB
	Project Code:	COB	Site ID:	P707	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6A	 0.018A	 2.06K	 0.77	 0.13	 0.05	 3B
	0.05 - 0.1	5.9A	 0.012A	 1.01K	 0.42	 0.03	 0.04	 1.5B
	0.1 - 0.2	5.9A	 0.009A	 2.01K	 0.29	 0.01	 0	 2.3B
	0.2 - 0.3	6.1A	 0.006A	 2.14K	 0.29	 0.04	 0.03	 2.5B
	0.3 - 0.44	6.2A	 0.006A	 3.02K	 0.21	 0.1	 0.06	 3.4B
	0.44 - 0.5	6.1A	 0.009A	 3.65K	 0.27	 0.04	 0.05	 4B
	0.5 - 0.6	6.2A	 0.009A	 2.99K	 0.16	 0.06	 0.05	 3.3B
	0.6 - 0.8	6.1A	 0.006A	 0.35K	 0.11	 0.03	 0.06	 0.6B
	0.8 - 1	6.1A	 0.006A	 0.25K	 0.04	 0.06	 0	 0.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 3.18D	 3.6D	 0.002D	 0.081B	 0.18A	 75	 43D	 42	 9	 6
	 0.011A
	0.05 - 0.1	 1.55D	 1.6D	 0.002D	 0.042B	 0.18A	 51	 44D	 43	 7	 6
	 0.005A
	0.1 - 0.2	 1.19D	 1.3D	 0.001D	 0.019B	 0.18A	 45	 42D	 45	 7	 7
	 0.005A
	0.2 - 0.3	 1.06D	 1.6D	 0D	 0.02B	 0.17A	 40	 39D	 46	 8	 8
	 0.004A
	0.3 - 0.44	 0.86D	 1.5D	 0.001D	 0.029B	 0.18A	 35	 32D	 45	 9	 15
	 0.006A
	0.44 - 0.5	 0.75D	 1.8D	 0D	 0.021B	 0.18A	 32	 29D	 37	 9	 25
	 0.008A
	0.5 - 0.6	 0.73D	 1.8D	 0D	 0.024B	 0.14A	 44	 18D	 29	 13	 40
	 0.01A
	0.6 - 0.8	 0.56D	 1.7D	 0D	 0.019B	 0.14A	 45	 21D	 30	 15	 37
	 0.006A
	0.8 - 1	 0.51D	 1.8D	 0D	 0.011B	 0.17A	 32	 27D	 30	 15	 29
	 0.006A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.44
	0.44 - 0.5
	0.5 - 0.6
	0.6 - 0.8
	0.8 - 1

	Project Name:	COB
	Project Code:	COB	Site ID:	P707	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF