Project Name:	COB
	Project Code:	COB	Site ID:	P710	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	13KM east of Jarrahdale: Forests Dept. map sheet 
	ref. BR70 (26M on 113degrees from E4500-N4000):
	Date Desc.:	29/10/80	Elevation:	 310 metres
	Map Ref.:	Sheet No. : 2133   1:100000	Rainfall:	1200
	Northing/Long.:	116.2	Runoff:	Rapid
	Easting/Lat.:	-32.3166666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mottled-Mesonatric Red Sodosol     	Principal Profile Form:	Dy5.62
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Very dark brown (10YR2/2-Moist); ; Loam (Fibric); 90-100%, medium gravelly, 6-20mm, angular, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	A12	0.05 - 0.1 m	Dark brown (10YR3/3-Moist); ; Sandy loam; 90-100%, medium gravelly, 6-20mm, angular, 
	Substrate material, coarse fragments; Abundant, fine (1-2mm) roots; 
	A13	0.1 - 0.2 m	Dark brown (10YR3/3-Moist); ; Sandy loam; 90-100%, fine gravelly, 2-6mm, rounded, Substrate 
	material, coarse fragments; 
	A21	0.2 - 0.3 m	Brown (10YR4/3-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, Substrate 
	material, coarse fragments; Few
	A22	0.3 - 0.6 m	Brown (10YR4/3-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, Substrate 
	material, coarse fragments; FewClear change to - 
	B21	0.6 - 0.8 m	Weak red (10R4/4-Moist); , 7.5YR56; , 2.5Y44; Sandy clay loam; 90-100%, coarse gravelly, 20-
	60mm, angular, Clay, coarse fragments; Few
	B22	0.8 - 1 m	Yellowish red (5YR5/8-Moist); , 2.5YR36; , 2.5Y44; Sandy clay loam; 50-90%, coarse gravelly, 
	20-60mm, angular, Clay, coarse fragments; Few
	Morphological Notes
	Observation Notes
	0-60CM AL GV IS FERRUGINOUS: 20-60CM FEW IRREGULAR LUMPS OF RECEMENTED LATERITE (<50MM):                        
	        
	Site Notes

	Project Name:	COB
	Project Code:	COB	Site ID:	P710	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.7A	 0.116A	 24K	 8.22	 0.34	 1.27	 33.8B
	0.05 - 0.1	6.4A	 0.065A	 3.97K	 3.49	 0.21	 0.55	 8.2B
	0.1 - 0.2	6.4A	 0.021A	 1.76K	 0.74	 0.14	 0.13	 2.8B
	0.2 - 0.3	6.6A	 0.03A	 1.72K	 0.63	 0.04	 0.22	 2.6B
	0.3 - 0.6	6.4A	 0.009A	 0.38K	 0.19	 0	 0.05	 0.6B
	0.6 - 0.8	6.8A	 0.039A	 0.61K	 0.27	 0.23	 0.23	 1.3B
	0.8 - 1	6.8A	 0.065A	 0.66K	 0.23	 0.22	 0.39	 1.5B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 16.5D	 21.1D	 0.017D	 0.741B	 0.2A	 88	 44D	 27	 11	 6
	 0.048A
	0.05 - 0.1	 7.34D	 6.6D	 0.006D	 0.183B	 0.16A	 84	 39D	 43	 8	 8
	 0.013A
	0.1 - 0.2	 2.42D	 3.4D	 0.003D	 0.048B	 0.14A	 74	 44D	 44	 11	 2
	 0.008A
	0.2 - 0.3	 1.15D	 2.7D	 0.003D	 0.041B	 0.14A	 66	 50D	 40	 9	 2
	 0.009A
	0.3 - 0.6	 0.53D	 1.9D	 0.001D	 0.022B	 0.15A	 58	 42D	 46	 8	 5
	 0.008A
	0.6 - 0.8	 0.55D	 2.5D	 0.001D	 0.021B	 0.06A	 69	 32D	 28	 15	 28
	 0.014A
	0.8 - 1	 0.34D	 2.8D	 0.001D	 0.017B	 0.05A	 56	 32D	 25	 13	 31
	 0.016A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 1

	Project Name:	COB
	Project Code:	COB	Site ID:	P710	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF