Project Name:	COB
	Project Code:	COB	Site ID:	P712	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	13KM east of Jarrahdale: Forests Dept. map sheet 
	ref. BR70 (36.5M on 340 degrees from E4350-N3850):
	Date Desc.:	23/10/80	Elevation:	 295 metres
	Map Ref.:	Sheet No. : 2133   1:100000	Rainfall:	1200
	Northing/Long.:	116.2	Runoff:	Rapid
	Easting/Lat.:	-32.3333333333334	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Ridge	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	9.5 % 	Aspect:	225 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	Uc5.11
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:	10-20%, , , Substrate material
	Profile Morphology
	0 - 0.05 m	Brown (7.5YR4/4-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, Substrate 
	material, coarse fragments; Abundant, fine (1-2mm) roots; 
	0.05 - 0.1 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	0.1 - 0.2 m	Strong brown (7.5YR5/6-Moist); ; Sandy loam; 90-100%, fine gravelly, 2-6mm, rounded, 
	Substrate material, coarse fragments; Common, fine (1-2mm) roots; 
	0.2 - 0.3 m	Strong brown (7.5YR5/6-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, 
	Substrate material, coarse fragments; 
	0.3 - 0.6 m	Strong brown (7.5YR5/6-Moist); ; Sandy loam; 90-100%, medium gravelly, 6-20mm, rounded, 
	Substrate material, coarse fragments; 
	0.6 - 0.8 m	Yellowish brown (10YR5/6-Moist); ; Sandy loam; 90-100%, medium gravelly, 6-20mm, rounded, 
	Substrate material, coarse fragments; 
	0.8 - 1 m	Yellowish brown (10YR5/6-Moist); ; Sandy loam; 90-100%, fine gravelly, 2-6mm, rounded, 
	Substrate material, coarse fragments; 
	1 - 1.2 m	Yellowish brown (10YR5/6-Moist); ; Loamy sand; 90-100%, fine gravelly, 2-6mm, rounded, 
	Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-120CM AL GV IS FERRUGINOUS: 5-30CM FEW LARGER RECEMENTED GRAVELS: 30-120CM <20MM FERRUGINOUS GV 
	ALSO:                 
	Site Notes

	Project Name:	COB
	Project Code:	COB	Site ID:	P712	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.4A	 0.033A	 2.89K	 1	 0.06	 0.27	 4.2B
	0.05 - 0.1	6.6A	 0.045A	 1.14K	 0.69	 0.03	 0.25	 2.1B
	0.1 - 0.2	6.5A	 0.018A	 0.86K	 0.73	 0	 0.12	 1.7B
	0.2 - 0.3	6.7A	 0.033A	 0.58K	 0.68	 0	 0.23	 1.5B
	0.3 - 0.6	6.8A	 0.027A	 0.35K	 0.36	 0	 0.17	 0.9B
	0.6 - 0.8	6.8A	 0.012A	 0.12K	 0.17	 0	 0.1	 0.4B
	0.8 - 1	6.8A	 0.009A	 0.08K	 0.08	 0	 0.07	 0.2B
	1 - 1.2	6.7A	 0.006A	 0.22K	 0.07	 0	 0.07	 0.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.98D	 4.6D	 0.001D	 0.088B	 0.13A	 67	 32D	 54	 6	 9
	 0.009A
	0.05 - 0.1	 1.6D	 2.5D	 0D	 0.036B	 0.13A	 58	 33D	 52	 7	 9
	 0.006A
	0.1 - 0.2	 1.21D	 1.6D	 0.001D	 0.033B	 0.12A	 49	 31D	 53	 5	 11
	 0.006A
	0.2 - 0.3	 0.96D	 1.3D	 0D	 0.029B	 0.13A	 64	 33D	 50	 7	 13
	 0.009A
	0.3 - 0.6	 0.69D	 1.5D	 0D	 0.027B	 0.13A	 75	 30D	 49	 7	 15
	 0.009A
	0.6 - 0.8	 0.49D	 1.5D	 0D	 0.037B	 0.1A	 86	 35D	 48	 11	 9
	 0.011A
	0.8 - 1	 0.38D	 2.2D	 0D	 0.026B	 0.07A	 83	 51D	 37	 10	 6
	 0.013A
	1 - 1.2	 0.43D	 3.4D	 0D	 0.034B	 0.05A	 83	 48D	 42	 11	 3
	 0.014A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 1
	1 - 1.2

	Project Name:	COB
	Project Code:	COB	Site ID:	P712	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF