Project Name:	COO
	Project Code:	COO	Site ID:	P110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	~1 chain north of north western corner of 
	experimental plot:
	Date Desc.:	29/04/52	Elevation:	No Data
	Map Ref.:	Sheet No. : 2032   1:100000	Rainfall:	0
	Northing/Long.:	115.903611111111	Runoff:	Slow
	Easting/Lat.:	-32.7505555555556	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Grey Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.13 m	Grey (10YR5/1-Moist); ; Sand (Sapric); Single grain grade of structure; Loose consistence; 
	0.13 - 0.33 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Loose 
	0.33 - 0.63 m	Yellowish brown (10YR5/6-Moist); , 5Y52; Sandy medium clay; 
	0.63 - 1.37 m	Greyish brown (10YR5/2-Moist); , 10YR58; Medium clay; 20-50%, coarse gravelly, 20-60mm, 
	rounded, Substrate material, coarse fragments; 
	1.37 - 1.73 m	Grey (10YR6/1-Moist); , 10YR54; Sandy medium clay (Heavy); 
	1.73 - 1.83 m	Grey (10YR6/1-Moist); , 10YR54; Sandy medium clay (Light); 
	Morphological Notes
	Observation Notes
	63-137CM QZ GV ALSO:                                                                                                    
	Site Notes
	SOUTH-WEST LD

	Project Name:	COO
	Project Code:	COO	Site ID:	P110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5A	 0.042A	 0.9K	 0.1	 0.06	 0.07	 1.1B
	0.13 - 0.33	5.1A	 0.018A
	0.33 - 0.63	5.5A	 0.039A	 0.6K	 1.3	 0.05	 0.14
	0.63 - 1.37	6A	 0.036A
	1.37 - 1.73	6.3A	 0.065A
	1.73 - 1.83	6.4A	 0.06A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13
	0.13 - 0.33
	0.33 - 0.63	 4	 54D	 18	 3	 23
	0.63 - 1.37	 43	 63D	 17	 5	 13
	1.37 - 1.73
	1.73 - 1.83
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.33
	0.33 - 0.63
	0.63 - 1.37
	1.37 - 1.73
	1.73 - 1.83

	Project Name:	COO
	Project Code:	COO	Site ID:	P110	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance