Project Name:	DWE
	Project Code:	DWE	Site ID:	P679	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	21KM east of Dwellingup: Forests Dept. map sheet 
	Ref. CQ75 (1650E-4750N):
	Date Desc.:	13/05/76	Elevation:	 310 metres
	Map Ref.:	Sheet No. : 2132   1:100000	Rainfall:	970
	Northing/Long.:	116.266666666667	Runoff:	Rapid
	Easting/Lat.:	-32.6666666666667	Drainage:	Well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Dolerite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	5.2 % 	Aspect:	180 degrees
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Paralithic Orthic Tenosol     	Principal Profile Form:	Uc5.11
	ASC Confidence:	Great Soil Group:	Siliceous sand
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Shrub, , . *Species includes - Pteridium esculentum
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:	2-10%, , , Substrate material
	Profile Morphology
	0 - 0.1 m	Dark brown (10YR3/3-Moist); ; Sandy loam; Single grain grade of structure; Very weak 
	consistence; 50-90%, angular, Substrate material, coarse fragments; 
	0.1 - 0.2 m	Yellowish red (5YR5/6-Moist); ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 90-100%, coarse gravelly, 20-60mm, angular, Substrate material, coarse 
	0.2 - 0.3 m	Yellowish red (5YR5/6-Moist); ; Loamy sand; Single grain grade of structure; Loose 
	consistence; 90-100%, coarse gravelly, 20-60mm, angular, Substrate material, coarse 
	0.3 - 0.6 m	Brown (7.5YR5/4-Moist); ; Loamy sand (Heavy); Single grain grade of structure; Loose 
	consistence; 90-100%, coarse gravelly, 20-60mm, angular, Substrate material, coarse 
	fragments; 
	0.6 - 0.9 m	Yellowish red (5YR5/6-Moist); ; Clayey sand; Single grain grade of structure; Loose 
	consistence; 90-100%, coarse gravelly, 20-60mm, angular, Substrate material, coarse 
	Morphological Notes
	Observation Notes
	0-90CM AL GV IS FERRUGINOUS: 10-89CM FINE <3MM PISOLITIC FERRUGINOUS GRAVEL ALSO:30-60CM SAMPLE 
	SUSPECT:                
	Site Notes

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P679	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6.2A	 0.018A	 5.69K	 1.26	 0.19	 0.09	 7.2B
	0.1 - 0.2	6.4A	 0.009A	 1.7K	 0.41	 0.08	 0.03	 2.2B
	0.2 - 0.3	6.5A	 0.006A	 1.62K	 0.34	 0.06	 0.02	 2B
	0.3 - 0.6	6.4A	 0.036A	 9.88K	 0.127	 0.16	 0.14	 11.5B
	0.6 - 0.9	6.7A	 0.009A	 2.42K	 0.44	 0.06	 0.05	 3B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.52D	 11D	 0.033A	 0.09B	 0.149A	 56	 52D	 34	 5	 8
	0.1 - 0.2	 1.36D	 3.3D	 0.021A	 0.031B	 0.144A	 67	 50D	 38	 6	 6
	0.2 - 0.3	 1.54D	 2.5D	 0.018A	 0.022B	 0.146A	 68	 48D	 39	 5	 7
	0.3 - 0.6	 3.19D	 2.8D	 0.019A	 0.048B	 0.143A	 68	 47D	 38	 5	 8
	0.6 - 0.9	 1.19D	 2.5D	 0.017A	 0.023B	 0.138A	 81	 48D	 38	 8	 7
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.9

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P679	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF