Project Name:	DWE
	Project Code:	DWE	Site ID:	P682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	21KM east of Dwellingup: Forests Dept. map sheet 
	Ref. CQ75 (5200N):
	Date Desc.:	01/05/76	Elevation:	 300 metres
	Map Ref.:	Sheet No. : 2132   1:100000	Rainfall:	970
	Northing/Long.:	116.266666666667	Runoff:	Slow
	Easting/Lat.:	-32.6666666666667	Drainage:	Imperfectly drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Drainage depression	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mesotrophic Chomosolic Redoxic Hydrosol     	Principal Profile Form:	Dg4.81
	ASC Confidence:	Great Soil Group:	Gleyed podzolic 
	All necessary analytical data are available.	soil
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , Closed or dense. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.1 m	Very dark grey (10YR3/1-Moist); ; Sandy loam (Fibric); Massive grade of structure; Moderately 
	moist; Weak consistence; 
	A21	0.1 - 0.2 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); ; Sandy loam; Massive grade of 
	structure; Moderately moist; Very weak consistence; 
	A22	0.2 - 0.3 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); ; Sandy loam; Massive grade of 
	structure; Moist; Very weak consistence; 
	A23	0.3 - 0.45 m	Greyish brown (10YR5/2-Moist); Light grey (10YR7/1-Dry); ; Sandy loam (Light); Massive grade of 
	structure; Moist; Very weak consistence; Abrupt change to - 
	A3B1	0.45 - 0.58 m	Light brownish grey (10YR6/2-Moist); Light grey (10YR7/1-Dry); ; Clayey sand (Light); Massive 
	grade of structure; Moist; Very weak consistence; 10-20%, coarse gravelly, 20-60mm, angular, 
	Substrate material, coarse fragments; 
	B21	0.58 - 0.67 m	Light grey (10YR7/1-Moist); , 7.5YR56; Sandy clay loam; Massive grade of structure; Moist; Firm 
	consistence; 10-20%, fine gravelly, 2-6mm, angular, Quartz, coarse fragments; 
	B22	0.67 - 0.9 m	White (2.5Y8/2-Moist); , 10YR66; , 2.5YR48; Medium clay; Massive grade of structure; Moist; 
	Very weak consistence; 2-10%, medium gravelly, 6-20mm, angular, Substrate material, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	45-90CM AL GV IS FERRUGINOUS:  LAYERS RE NUMBERED 15/10/92                                                              
	Site Notes

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	 0.021A	 4.73K	 2.08	 0.32	 0.13
	0.1 - 0.2	6.1A	 0.009A	 1.47K	 1.01	 0.25	 0.06
	0.2 - 0.3	6.2A	 0.006A	 0.83K	 0.74	 0.23	 0.04
	0.3 - 0.45	6.1A	 0.006A	 0.86K	 0.73	 0.1	 0.04
	0.45 - 0.58	6.1A	 0.003A	 0.45K	 0.52	 0.06	 0.03
	0.58 - 0.67	6A	 0.006A	 0.64K	 1.5	 0.12	 0.06
	0.67 - 0.9	5.8A	 0.009A	 0.87K	 2.72	 0.18	 0.1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 3.73D	 8.6D	 0.023A	 0.104B	 0.069A	 8	 54D	 28	 7	 8
	0.1 - 0.2	 1.86D	 4.8D	 0.012A	 0.038B	 0.065A	 10	 51D	 31	 8	 11
	0.2 - 0.3	 1.36D	 4.5D	 0.01A	 0.021B	 0.063A	 6	 53D	 31	 6	 10
	0.3 - 0.45	 0.88D	 4D	 0.008A	 0.013B	 0.052A	 4	 52D	 35	 5	 9
	0.45 - 0.58	 1D	 5D	 0.006A	 0.009B	 0.065A	 34	 50D	 35	 6	 9
	0.58 - 0.67	 1.3D	 2.5D	 0.008A	 0.009B	 0.07A	 39	 44D	 21	 7	 26
	0.67 - 0.9	 0.35D	 1.5D	 0.005A	 0.009B	 0.066A	 18	 25D	 18	 9	 47
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.45
	0.45 - 0.58
	0.58 - 0.67
	0.67 - 0.9

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P682	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF