Project Name:	DWE
	Project Code:	DWE	Site ID:	P705	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	1.5KM north east of Dwellingup on Eastern side of 
	Banksiadale Road:
	Date Desc.:	11/11/77	Elevation:	 270 metres
	Map Ref.:	Sheet No. : 2132   1:100000	Rainfall:	1310
	Northing/Long.:	116.066666666667	Runoff:	Rapid
	Easting/Lat.:	-32.7	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Plateau
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Brown Kandosol     	Principal Profile Form:	Dy5.61
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Brown (10YR5/3-Moist); ; Sand; Single grain grade of structure; 10-20%, Substrate material, 
	coarse fragments; Diffuse change to - 
	0.05 - 0.11 m	Brown (10YR5/3-Moist); , 10YR56; Sand; Single grain grade of structure; 10-20%, Substrate 
	material, coarse fragments; 
	0.11 - 0.2 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; 50-90%, Substrate 
	material, coarse fragments; 
	0.2 - 0.3 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; 90-100%, Substrate 
	material, coarse fragments; 
	0.3 - 0.6 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; 90-100%, Substrate 
	material, coarse fragments; 
	0.6 - 0.75 m	Yellowish brown (10YR5/6-Moist); ; Clayey sand; Single grain grade of structure; 90-100%, 
	Substrate material, coarse fragments; Abrupt change to - 
	0.75 - 0.9 m	Strong brown (7.5YR5/6-Moist); , 2.5YR56; Sandy clay loam (Light); Massive grade of structure; 
	90-100%, Substrate material, coarse fragments; 
	0.9 - 1 m	Strong brown (7.5YR5/6-Moist); , 2.5YR56; Sandy clay loam; Massive grade of structure; 90-
	100%, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	0-100CM AL GV IS FERRUGINOUS LAYERS RE NUMBERED 15/10/92                                                                
	Site Notes

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P705	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A	 0.012A	 3.05K	 0.76	 0.04	 0.04
	0.05 - 0.11	6.6A	 0.006A	 1.33K	 0.47	 0.02	 0.02
	0.11 - 0.2	6.4A	 0.003A	 0.5K	 0.29	 0.02	 0.01
	0.2 - 0.3	6.5A	 0.009A	 0.78K	 0.22	 0.02	 0.03
	0.3 - 0.6	6.4A	 0.003A	 2.8K	 0.56	 0.02	 0.02
	0.6 - 0.75	6.5A	 0.003A	 1.53K	 0.3	 0.02	 0.01
	0.75 - 0.9	6.4A	 0.009A	 0.75K	 0.22	 0.03	 0.03
	0.9 - 1	6.3A	 0.003A	 0.78K	 0.19	 0.03	 0.02
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 2.72D	 6D	 0.003D	 0.1B	 0.074A	 25	 55D	 38	 2	 5
	 0.01A
	0.05 - 0.11	 2.1D	 5D	 0.001D	 0.05B	 0.067A	 37	 50D	 43	 1	 3
	 0.05A
	0.11 - 0.2	 1.58D	 3D	 0.001D	 0.02B	 0.08A	 58	 51D	 43	 2	 4
	 0.049A
	0.2 - 0.3	 1D	 1.5D	 0.001D	 0.02B	 0.073A	 65	 53D	 39	 3	 4
	 0.05A
	0.3 - 0.6	 1.62D	 17D	 0.001D	 0.03B	 0.088A	 68	 51D	 39	 2	 7
	 0.006A
	0.6 - 0.75	 1.05D	 2.5D	 0.002D	 0.02B	 0.094A	 82	 47D	 34	 6	 11
	 0.01A
	0.75 - 0.9	 0.65D	 2D	 0.004D	 0.02B	 0.11A	 90	 41D	 30	 8	 20
	 0.01A
	0.9 - 1	 0.6D	 2D	 0.006D	 0.02B	 0.118A	 78	 39D	 23	 9	 28
	 0.013A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.11
	0.11 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.75
	0.75 - 0.9
	0.9 - 1

	Project Name:	DWE
	Project Code:	DWE	Site ID:	P705	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF