Project Name:	FRA
	Project Code:	FRA	Site ID:	P264	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	L.W. Pym	Locality:	L.D. Sheet 444/80 - Lot 376:10 chains north east 
	from south east corner
	Date Desc.:	26/11/55	Elevation:	 268 metres
	Map Ref.:	Sheet No. : 2329   1:100000	Rainfall:	0
	Northing/Long.:	117.138888888889	Runoff:	Slow
	Easting/Lat.:	-34.2975	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Peneplain
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Footslope	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Mesotrophic Grey Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Very dark grey (5Y3/1-Moist); ; Loamy sand (Fibric); ; FragmentDry; Loose consistence; Field pH 
	6 (pH meter); Clear, Smooth change to - 
	A2	0.13 - 0.33 m	Greyish brown (2.5Y5/2-Moist); ; Loamy sand; Weak grade of structure; FragmentDry; Loose 
	consistence; Field pH 6 (pH meter); Clear, Wavy change to - 
	A3	0.33 - 0.48 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; Dry; Loose 
	consistence; 50-90%, stony, 200-600mm, Quartz, coarse fragments; Field pH 6 (pH meter); 
	Clear, Smooth change to - 
	B	0.48 - 0.86 m	Light grey (10YR7/1-Moist); , 2.5YR48; , 10YR51; Medium clay; 20-50 mm, Angular blocky; Dry; 
	Rigid consistence; Moderately plastic; Normal plasticity; 2-10%, Quartz, coarse fragments; Field
	 pH 6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	48-86CM FEW QZ FLOATERS:                                                                                                
	Site Notes
	HAY

	Project Name:	FRA
	Project Code:	FRA	Site ID:	P264	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	6.1A	 0.045A	 8.6K	 1.9	 0.28	 0.16	 17.1E	 28B
	0.13 - 0.33	6.4A	 0.021A
	0.33 - 0.48	6.4A	 0.018A
	0.48 - 0.86	5.8A	 0.06A	 0.8K	 4.4	 0.16	 0.67	 5.3E	 11.4B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 4.8D	 0.027D	 0.264B	 57D	 23	 8	 5
	0.13 - 0.33	 55D	 32	 6	 5
	0.33 - 0.48	 54D	 36	 8	 2
	0.48 - 0.86	 32D	 12	 10	 45
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.33
	0.33 - 0.48
	0.48 - 0.86

	Project Name:	FRA
	Project Code:	FRA	Site ID:	P264	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance