Project Name:	GAR
	Project Code:	GAR	Site ID:	P519	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	On Brickhouse Station 23KM east of homestead and 
	100 chains south of Gascoyne River:
	Date Desc.:	21/06/63	Elevation:	 30 metres
	Map Ref.:	Sheet No. : 1748   1:100000	Rainfall:	220
	Northing/Long.:	114	Runoff:	Very slow
	Easting/Lat.:	-24.7833333333334	Drainage:	Very poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:	Severe (sheet) 
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Hypernatric Red Sodosol     	Principal Profile Form:	Dr4.33
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:	Low Strata - Shrub, 0.26-0.5m, Very sparse. *Species includes - None recorded
	Tall Strata - Tree, 3.01-6m, Isolated plants. *Species includes - Acacia species
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Red (2.5YR4/6-Moist); ; Sand (Heavy); Single grain grade of structure; 2-10%, fine gravelly, 2-
	6mm, Quartz, coarse fragments; Clear change to - 
	A	0.05 - 0.13 m	Red (2.5YR4/6-Moist); ; Sand; Single grain grade of structure; CommonClear change to - 
	A2sb	0.13 - 0.15 m	Light reddish brown (2.5YR6/4-Dry); ; Sandy loam; Massive grade of structure; Clear change to - 
	B	0.15 - 0.23 m	Dark red (2.5YR3/6-Moist); ; Sandy light clay; Weak grade of structure, 20-50 mm, Subangular 
	blocky; Moderately moist; Weak consistence; CommonGradual change to - 
	0.3 - 0.38 m	Reddish brown (2.5YR4/4-Moist); ; Medium clay; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Weak consistence; Diffuse change to - 
	0.48 - 0.56 m	Reddish brown (2.5YR4/4-Moist); ; Light clay; 50-100 mm, Columnar; Diffuse change to - 
	0.66 - 0.76 m	Red (2.5YR4/6-Moist); ; Sandy light clay; 50-100 mm, Columnar; Few (2 - 10 %), Gypseous, Fine 
	(0 - 2 mm), ; Diffuse change to - 
	0.91 - 0.99 m	Red (2.5YR4/8-Moist); ; Sandy light clay (Light); Massive grade of structure; Very strong 
	consistence; Few (2 - 10 %), Gypseous, , ; 
	1.27 - 1.47 m	Red (2.5YR4/6-Moist); ; Sandy clay loam (Light); Few (2 - 10 %), Gypseous, , ; 
	1.73 - 1.88 m	Red (2.5YR4/6-Moist); ; Loamy fine sand; Very few (0 - 2 %), Gypseous, , ; 
	Morphological Notes
	Observation Notes
	48-56CM BLACK MAGANESE SPECKS: 66-76CM MANY BLACK FACES AND ALONG ROOT CHANNELS: 0-5CM WIND 
	BLOWN KAOLIN:               
	Site Notes
	CARNARVON

	Project Name:	GAR
	Project Code:	GAR	Site ID:	P519	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	8.2A	 0.045A	 0.7K	 0.65	 0.7	 7.2
	0.05 - 0.13	8.9A	 0.027A	 0.21K	 0.21	 0.4	 5.6
	0.13 - 0.15	9A	 0.036A	 0.31K	 0.35	 0.3	 8
	0.15 - 0.23	8.8A	 0.11A	 0.25K	 0.21	 0.2	 12.6
	0.3 - 0.38	8.5A	 0.446A	 1.3K	 1.62	 0.35	 30.4
	0.48 - 0.56	7.9A	 0.952A	 4.6K	 6.8	 0.5	 48.4
	0.66 - 0.76	6.9A	 1.81A	 24K	 26.2	 0.7	 130
	0.91 - 0.99	7.1A	 1.87A	 36.1K	 38.2	 1	 145
	1.27 - 1.47	7.4A	 1.81A	 31K	 31	 0.9	 125
	1.73 - 1.88	7.9A	 1.31A	 106K	 42	 0.8	 53.4
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.1A	 0.022D	 0.19C	 22D	 69	 4	 5
	0.05 - 0.13	 0.1A	 0.023D	 0.2C	 22D	 65	 7	 5
	0.13 - 0.15	 0.1A	 0.024D	 0.28C	 21D	 60	 11	 7
	0.15 - 0.23	 0.2A	 11D	 43	 14	 28
	0.3 - 0.38	 0.3A
	0.48 - 0.56
	0.66 - 0.76	 0.3A
	0.91 - 0.99	 0.1A	 12D	 56	 7	 23
	1.27 - 1.47	 0.1A
	1.73 - 1.88	 0.1A	 10D	 71	 5	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.13
	0.13 - 0.15
	0.15 - 0.23
	0.3 - 0.38
	0.48 - 0.56
	0.66 - 0.76
	0.91 - 0.99
	1.27 - 1.47
	1.73 - 1.88

	Project Name:	GAR
	Project Code:	GAR	Site ID:	P519	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	12_HCL_FE	Total element - Fe(%) - Total acid(HCl) extractable Fe
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	17A_HCL	Total element - K(%) - By boiling HCl
	19A1	Carbonates - rapid titration
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance