Project Name:	IVS
	Project Code:	IVS	Site ID:	P571	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	2.74KM north and 304M east of base line: Peninsula 
	area - south of LakeLefroy:
	Date Desc.:	01/05/68	Elevation:	No Data
	Map Ref.:	Sheet No. : 2235   1:100000	Rainfall:	250
	Northing/Long.:	116.663611111111	Runoff:	No Data
	Easting/Lat.:	-31.4586111111111	Drainage:	No Data
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Sand 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Sand plain
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Lunette	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcareous Petroferric Orthic Tenosol     	Principal Profile Form:	Gn1.13
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:
	Vegetation:	Low Strata - Tussock grass, , . *Species includes - None recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.1 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/6-Dry); ; Loamy sand; Field pH 6.5 (pH meter); 
	0.1 - 0.2 m	Dark red (2.5YR3/6-Moist); Dark red (2.5YR3/6-Dry); , 2.5YR20; Sandy loam; Loose consistence; 
	Field pH 7.5 (pH meter); 
	0.2 - 0.3 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/8-Dry); , 2.5YR20, 2-10% ; , 2-10% ; Sandy loam; Loose 
	consistence; Manganiferous pan, Moderately cemented; Field pH 7 (pH meter); 
	k	0.3 - 0.5 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/8-Dry); ; Sandy clay loam; Loose consistence; Few (2 - 
	10 %), Unidentified, , Soft segregations; Manganiferous pan, Moderately cemented; Field pH 9 
	(pH meter); 
	k	0.5 - 0.6 m	Dark red (2.5YR3/6-Moist); Red (2.5YR4/8-Dry); ; Sandy clay loam; Firm consistence; Few (2 - 10
	 %), Unidentified, , Soft segregations; Few (2 - 10 %), Gypseous, Coarse (6 - 20 mm), Soft 
	segregations; Field pH 9 (pH meter); 
	Morphological Notes
	Observation Notes
	>60CM CARBONATE LAYER: LAYERS RE NUMBERED 15/10/92                                                                      
	Site Notes
	LAKE LEFROY

	Project Name:	IVS
	Project Code:	IVS	Site ID:	P571	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	7.5A
	0.1 - 0.2	8.8A
	0.2 - 0.3	8.1A
	0.3 - 0.5	9.5A
	0.5 - 0.6	9.6A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	<1A	 0	 49D	 42	 5	 4
	0.1 - 0.2	 1A	 0	 45D	 41	 7	 6
	0.2 - 0.3	<1A	 0	 45D	 45	 2	 7
	0.3 - 0.5	 1A	 1	 41D	 38	 7	 10
	0.5 - 0.6	 5A	 9	 37D	 38	 5	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.5
	0.5 - 0.6

	Project Name:	IVS
	Project Code:	IVS	Site ID:	P571	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	19A1	Carbonates - rapid titration
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance