Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P782	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	amg ref.: 381750. 6323250
	Date Desc.:	23/05/85	Elevation:	No Data
	Map Ref.:	1:50000	Rainfall:	No Data
	Northing/Long.:	115.73333333333	Runoff:	No Data
	Easting/Lat.:	-33.2166666666667	Drainage:	Rapidly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Confidence level not specified
	Site Disturbance:
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A11	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Few, coarse (>5mm) roots; 
	A12	0.05 - 0.1 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Very weak consistence; Few, 
	coarse (>5mm) roots; 
	A2	0.1 - 0.2 m	Grey (10YR5/1-Moist); Grey (10YR6/1-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Few, medium (2-5mm) roots; 
	A21	0.2 - 0.3 m	Grey (10YR6/1-Moist); Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of 
	structure; Loose consistence; 
	A22	0.3 - 0.6 m	Light grey (10YR7/1-Moist); White (10YR8/1-Moist); ; Sand; Single grain grade of structure; 
	Loose consistence; 
	A23	0.6 - 1 m	White (10YR8/1-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	A24	1 - 1.5 m	Very pale brown (10YR7/3-Moist); ; Sand; Single grain grade of structure; Loose consistence; 
	A3	1.5 - 2 m	; Sand; Single grain grade of structure; Loose consistence; 
	A3	2 - 2.4 m	; Sand; Single grain grade of structure; Loose consistence; 
	B2h	2.4 - 3 m	Strong brown (7.5YR5/6-Moist); Brownish yellow (10YR6/6-Moist); ; Sand; Single grain grade of 
	structure; Loose consistence; , Unidentified, Medium (2 -6 mm), Nodules; 
	B2h	3 - 3.5 m	Strong brown (7.5YR5/8-Moist); Dark yellowish brown (10YR4/4-Moist); ; Sand; Single grain 
	grade of structure; Loose consistence; , Unidentified, Medium (2 -6 mm), Nodules; 
	B2h	3.5 - 4 m	Brownish yellow (10YR6/8-Moist); ; Sand; Single grain grade of structure; Loose consistence; , 
	Unidentified, Medium (2 -6 mm), Nodules; 
	4 - 4.5 m	; Sand; Single grain grade of structure; , Unidentified, Coarse (6 - 20 mm), Nodules; 
	4.5 - 5 m	; Sand; Single grain grade of structure; , Unidentified, Coarse (6 - 20 mm), Nodules; 
	5 - 5.5 m	Yellow (2.5Y7/6-Moist); ; Sand; Single grain grade of structure; Few (2 - 10 %), Unidentified, , 
	Nodules; 

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P782	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	5.5 - 6 m	Pale yellow (2.5Y7/4-Moist); ; Sand; Single grain grade of structure; Few (2 - 10 %), Unidentified,
	 Medium (2 -6 mm), Nodules; Few, medium (2-5mm) roots; 
	Morphological Notes
	Observation Notes
	Bott. S.pit 100 cm, auger samples below, from a hole about 1 m of sampling face. B.D. samples, each of 4 bulked cores from 
	following depths: 0-6.8, 27-33, 72-78 cm.
	Site Notes
	Karrakatta sand (grey phase). Free external drainage. Still under native vegegation: Jarrah- Banksia woodland. Aeolian sand of 
	marine origin (Spearwood Dune System) Low relief, 0-1 degree slope, S aspect.

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P782	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.7A	0.01A	0.87K	0.14	0	0.09	3.3D
	0.05 - 0.1	5.9A	0.01A	1.4K	0.2	0	0.1	3.1D
	0.1 - 0.2	5.9A	0.01A	0.68K	0.13	0	0.09
	0.2 - 0.3	6A	<0.005A	0.2K	0.03	0	0.07
	0.3 - 0.6	5.8A	<0.005A	0.12K	0.01	0	0.07
	0.6 - 1	6A	<0.005A	0.12K	0.03	0	0.07
	1 - 1.5	5.8A	0.01A	0.03K	0	0	0.08
	1.5 - 2	5.9A	<0.005A	0.03K	0.01	0	0.05
	2 - 2.4	6A	<0.005A	0.05K	0.01	0	0.07
	2.4 - 3	6.1A	<0.005A	0.11K	0.03	0	0.08
	3 - 3.5	6.1A	<0.005A	0.11K	0.03	0	0.09
	3.5 - 4	6.1A	0.01A	0.08K	0.03	0	0.08
	4 - 4.5	6.2A	0.01A	0.11K	0.08	0	0
	4.5 - 5	6.2A	0.01A	0.06K	0.11	0	0
	5 - 5.5	6.1A	0.01A	0.08K	0.08	0	0
	5.5 - 6	6.2A	<0.005A	0.05K	0.08	0	0
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	0.911D	1.2D	8.2F	0.002B	96D	2
	0.05 - 0.1	1.36D	0.6D	6.1F	0.038B	97D	1
	0.1 - 0.2	0.292D	0.4D	3.7F	0.01B	95D	4	0	1
	0.2 - 0.3	0.107D	0.6D	2.9F	0.012B	97D	3	1	1
	0.3 - 0.6	0.1D	0.5D	2F	0.009B	97D	3	1	0
	0.6 - 1	0.089D	0.4D	2.7F	0.002B	96D	4	0	1
	1 - 1.5	0D	0.5D	1.7F	0.002B	95D	4	0	1
	1.5 - 2	0.06D	0.4D	2.1F	0.002B	93D	7	0	1
	2 - 2.4	0.064D	2.1D	3F	0.002B	94D	6	1	0
	2.4 - 3	0.116D	2.7D	5.1F	0.008B	89D	10	0	1
	3 - 3.5	0.211D	3.5D	7.6F	0.012B	90D	8	0	1
	3.5 - 4	0.113D	2.3D	6.9F	0.01B	91D	8	0	2
	4 - 4.5	0D	2.4D	8.7F	0.004B	88D	10	0	2
	4.5 - 5	0.03D	2D	10F	0.002B	90D	8	0	3
	5 - 5.5	0D	1D	6F	0.002B	90D	9	0	1
	5.5 - 6	0.031D	0.7D	4.5F	0B	92D	7	0	0
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 1
	1 - 1.5
	1.5 - 2
	2 - 2.4

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P782	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	2.4 - 3
	3 - 3.5
	3.5 - 4
	4 - 4.5
	4.5 - 5
	5 - 5.5
	5.5 - 6

	Project Name:	Kemerton
	Project Code:	KEM	Site ID:	P782	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	13A1_AL	Oxalate-extractable aluminium
	13A1_FE	Oxalate-extractable iron
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	2_LOI	Loss on Ignition (%)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_NR	Total element - P(%) - Not recorded
	9E	Available P (mg/kg) - Bray P
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance