Project Name:	MAP
	Project Code:	MAP	Site ID:	P696	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	5.4KM N.W. of Pemberton and 0.6KM east of House 
	Brook Rd: in 50M X 50Mplot:
	Date Desc.:	16/12/76	Elevation:	 140 metres
	Map Ref.:	Sheet No. : 2129   1:100000	Rainfall:	1300
	Northing/Long.:	116	Runoff:	Rapid
	Easting/Lat.:	-34.4	Drainage:	Moderately well drained
	Geology
	ExposureType:	Auger boring	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Mesotrophic Red Kandosol     	Principal Profile Form:	Gn2.14
	ASC Confidence:	Great Soil Group:	Red earth
	No analytical data are available but confidence is fair.
	Site Disturbance:
	Vegetation:
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark reddish brown (5YR3/2-Moist); , 5YR34; Sandy loam (Fibric); Massive grade of structure; 
	Very weak consistence; 50-90%, medium gravelly, 6-20mm, subangular, Substrate material, 
	coarse fragments; Abundant, fine (1-2mm) roots; 
	0.05 - 0.1 m	Dark reddish brown (5YR3/4-Moist); ; Sandy loam; Massive grade of structure; Very weak 
	consistence; 50-90%, medium gravelly, 6-20mm, subangular, Substrate material, coarse 
	fragments; Few, fine (1-2mm) roots; 
	0.1 - 0.2 m	Yellowish red (5YR4/6-Moist); ; Sandy loam; Massive grade of structure; Weak consistence; 50-
	90%, medium gravelly, 6-20mm, subangular, Substrate material, coarse fragments; Few, fine (1-
	2mm) roots; 
	0.2 - 0.3 m	Yellowish red (5YR4/6-Moist); ; Sandy clay loam; Massive grade of structure; Very weak 
	consistence; 90-100%, medium gravelly, 6-20mm, subangular, Substrate material, coarse 
	fragments; Few, fine (1-2mm) roots; 
	0.3 - 0.6 m	Yellowish red (5YR4/6-Moist); , 7.5YR54; , 10R56; Sandy clay loam; Massive grade of structure; 
	Strong consistence; 50-90%, medium gravelly, 6-20mm, subangular, Substrate material, coarse
	 fragments; Few, fine (1-2mm) roots; 
	0.6 - 0.8 m	Red (2.5YR4/8-Moist); ; Light clay; Massive grade of structure; Strong consistence; 50-90%, 
	medium gravelly, 6-20mm, angular, Substrate material, coarse fragments; Few, fine (1-2mm) 
	roots; 
	0.8 - 0.9 m	Red (2.5YR4/8-Moist); , 5YR48; Light clay; Massive grade of structure; 10-20%, medium gravelly,
	 6-20mm, angular, Substrate material, coarse fragments; Few, fine (1-2mm) roots; 
	Morphological Notes
	Observation Notes
	0-90CM AL GV IS FERRUGINOUS:  LAYERS RE NUMBERED 15/10/92                                                               
	Site Notes

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P696	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.3A	 0.074A	 20.5K	 7.4	 0.44	 1.05	 29.4B
	0.05 - 0.1	6.9A	 0.045A	 7.21K	 2.91	 0.23	 0.88	 11.2B
	0.1 - 0.2	6.6A	 0.033A	 2.7K	 1.4	 0.14	 0.53	 4.8B
	0.2 - 0.3	6.6A	 0.018A	 1.32K	 0.77	 0.11	 0.35	 2.6B
	0.3 - 0.6	6.8A	 0.015A	 0.86K	 0.51	 0.14	 0.13	 1.6B
	0.6 - 0.8	6.1A	 0.018A	 0.63K	 0.65	 0.17	 0.2	 1.7B
	0.8 - 0.9	6A	 0.024A	 0.17K	 0.44	 0.15	 0.21	 1B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 9.77D	 5D	 0.013D	 0.379B	 0.137A	 48
	 0.031A
	0.05 - 0.1	 4.52D	 5D	 0.008D	 0.169B	 0.126A	 52
	 0.017A
	0.1 - 0.2	 2.46D	 4D	 0.007D	 0.111B	 0.135A	 56
	 0.017A
	0.2 - 0.3	 1.4D	 3D	 0.005D	 0.061B	 0.134A	 63
	 0.015A
	0.3 - 0.6	 0.84D	 2D	 0.003D	 0.029B	 0.122A	 58
	 0.009A
	0.6 - 0.8	 0.84D	 2D	 0.004D	 0.029B	 0.094A	 41
	 0.008A
	0.8 - 0.9	 0.56D	 4D	 0.004D	 0.022B	 0.067A	 23
	 0.007A
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.1
	0.1 - 0.2
	0.2 - 0.3
	0.3 - 0.6
	0.6 - 0.8
	0.8 - 0.9

	Project Name:	MAP
	Project Code:	MAP	Site ID:	P696	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	10B	Extractable sulfur(mg/kg) - Phosphate extractable sulfur
	12_XRF_CU	Total element - Cu(mg/kg) - X-Ray Fuoresence
	12_XRF_FE	Total element - Fe(%) - X-Ray Fuoresence
	12_XRF_MN	Total element - Mn(mg/kg) - X-Ray Fuoresence
	12_XRF_ZN	Total element - Zn(mg/kg) - X-Ray Fuoresence
	12B1_CU	Ammonium bicarbonate/EDTA - extractable copper
	12B1_ZN	Ammonium bicarbonate/EDTA - extractable zinc
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	17A1	Total potassium - X-ray fluorescence
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	9A1	Total phosphorus - X-ray fluorescence
	9E	Available P (mg/kg) - Bray P
	P10_GRAV	Gravel (%)
	TE_XRF_MG	Total Element Mg - By XRF
	TE_XRFCA	Total Element Ca - By XRF
	TE_XRFTIO2	Total Element TiO2 - By XRF