Project Name:	MEX
	Project Code:	MEX	Site ID:	P162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	On Base B3 4.8KM and 78 chains south from Base A:
	Date Desc.:	25/03/53	Elevation:	No Data
	Map Ref.:	Sheet No. : 2528   1:100000	Rainfall:	710
	Northing/Long.:	118.205	Runoff:	Moderately rapid
	Easting/Lat.:	-34.6744444444445	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Peneplain
	1-3%
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Yellow Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Solodized solonetz
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.025 m	Dark grey (10YR4/1-Moist); ; Loamy fine sand; Single grain grade of structure; Moist; Loose 
	consistence; Diffuse, Irregular change to - 
	A2	0.025 - 0.15 m	Light grey (2.5Y7/2-Moist); ; Fine sand; Single grain grade of structure; Dry; Loose consistence; 
	Clear, Irregular change to - 
	B	0.15 - 0.89 m	Light yellowish brown (10YR6/4-Moist); , 10YR56; , 2.5YR58; Medium clay; Massive grade of 
	structure; Dry; Very strong consistence; 
	0.89 - 1.17 m	Grey (10YR6/1-Moist); , 10YR56; , 2.5YR58; Fine sandy medium clay; Massive grade of 
	structure; 
	1.17 - 1.29 m	Grey (10YR6/1-Moist); , 10YR88; , 2.5YR58; Fine sandy medium clay; 
	1.29 - 1.55 m	Light grey (10YR7/1-Moist); , 10YR88; Fine sand; 
	1.55 - 2.9 m	Light grey (10YR7/1-Moist); , 2.5Y84, 2-10% ; , 2.5YR58, 2-10% ; Fine sand; 
	Morphological Notes
	Observation Notes
	15-89CM B HORIZON COL. STRUCTURE TO 38CM:117-129CM SMALL AREAS OF CLAY:                                                 
	Site Notes
	PLANTAGENET LD

	Project Name:	MEX
	Project Code:	MEX	Site ID:	P162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	6A	 0.06A
	0.025 - 0.15	6.1A	 0.024A
	0.15 - 0.89	6.6A	 0.131A	 2K	 5.8	 0.67	 2.3	 6.8E
	0.89 - 1.17	9.2A	 0.583A
	1.17 - 1.29	9.5A	 0.429A
	1.29 - 1.55	8.9A	 0.134A
	1.55 - 2.9	8.6A	 0.345A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 1.52D	 0.001D	 0.043B
	0.025 - 	 0.021B
	0.15
	0.15 - 0.89	 0.001D	 36	 6D	 50	 1	 36
	0.89 - 1.17
	1.17 - 1.29
	1.29 - 1.55
	1.55 - 2.9
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.15
	0.15 - 0.89
	0.89 - 1.17
	1.17 - 1.29
	1.29 - 1.55
	1.55 - 2.9

	Project Name:	MEX
	Project Code:	MEX	Site ID:	P162	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance