Project Name:	MEX
	Project Code:	MEX	Site ID:	P164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	1.6KM west from B3 along most northerly east west 
	access Road:
	Date Desc.:	26/03/53	Elevation:	No Data
	Map Ref.:	Rainfall:	710
	Northing/Long.:	Runoff:	Rapid
	Easting/Lat.:	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Peneplain
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Ferric-Petroferric Bleached-Leptic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1A2cb	0 - 0.05 m	Grey (10YR6/1-Moist); ; Fine sand; Single grain grade of structure; Moist; Loose consistence; 
	Diffuse, Smooth change to - 
	A3	0.05 - 0.2 m	Light grey (10YR7/2-Moist); ; Fine sand; Single grain grade of structure; Moderately moist; Loose
	 consistence; Diffuse, Smooth change to - 
	A4	0.2 - 0.36 m	White (2.5Y8/2-Moist); ; Fine sand; Single grain grade of structure; Dry; Loose consistence; 0-
	2%, Substrate material, coarse fragments; Clear, Wavy change to - 
	A5	0.36 - 0.84 m	White (10YR8/2-Moist); ; Fine sand; Single grain grade of structure; Dry; Loose consistence; 50-
	90%, undisturbed, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	3MM LAYER OF BLEACHED FS ON SURFACE:20-84CM GV FERRUGINISED:MASSIVE IRONSTONE AT 79CM:                        
	          
	Site Notes
	PLANTAGENET LD

	Project Name:	MEX
	Project Code:	MEX	Site ID:	P164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.2A	 0.018A
	0.05 - 0.2	5.7A	 0.012A
	0.2 - 0.36	5.5A	 0.009A
	0.36 - 0.84	6A	 0.012A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.36
	0.36 - 0.84
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.2
	0.2 - 0.36
	0.36 - 0.84

	Project Name:	MEX
	Project Code:	MEX	Site ID:	P164	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour