Project Name:	NST
	Project Code:	NST	Site ID:	P132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	10 chains north of a point 60 chains west from 
	intersection of roads Nos 7134 and 5881:
	Date Desc.:	25/07/52	Elevation:	No Data
	Map Ref.:	Sheet No. : 2529   1:100000	Rainfall:	380
	Northing/Long.:	118.055277777778	Runoff:	Rapid
	Easting/Lat.:	-34.2597222222222	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Igneous rock (unidentified) 
	Land Form
	Rel/Slope Class: 	Gently undulating plains <9m  	Pattern Type:	Peneplain
	1-3%
	Morph. Type:	Simple-slope	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Mottled Magnesic Red Kurosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Shrub, , . *Species includes - None recorded
	Tall Strata - Tree mallee, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.04 m	Pale brown (10YR6/3-Moist); ; Sand; Single grain grade of structure; Moist; Very weak 
	consistence; 2-10%, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, , ; Field pH 6 (pH 
	meter); ManyClear, Irregular change to - 
	B1	0.04 - 0.25 m	Reddish brown (2.5YR4/4-Moist); ; Sandy medium clay; Moderately moist; Weak consistence; 2-
	10%, Gravel, coarse fragments; Field pH 5.5 (pH meter); Clear, Irregular change to - 
	B2	0.25 - 0.63 m	Reddish brown (2.5YR5/4-Moist); , 10YR68; , 5Y52; Sandy medium clay; Dry; Weak 
	consistence; 10-20%, Quartz, coarse fragments; Common (10 - 20 %), Ferruginous, , ; Field pH 
	5.5 (pH meter); Clear, Smooth change to - 
	B3	0.63 - 1.37 m	Light brownish grey (10YR6/2-Moist); , 2.5YR54; Sandy medium clay; Dry; Strong consistence; 
	2-10%, Gravel, coarse fragments; Field pH 6.5 (pH meter); 
	C	1.37 - 2.01 m	Light brownish grey (10YR6/2-Moist); , 2.5YR54; Sandy medium clay; Dry; Strong consistence; 
	0-2%, Gravel, coarse fragments; Field pH 6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	Site Notes
	PLANTAGENET LD

	Project Name:	NST
	Project Code:	NST	Site ID:	P132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.04	5.6A	 0.042A
	0.04 - 0.25	5.3A	 0.074A	 0.2K	 2.5	 0.06	 0.21	 3B
	0.25 - 0.63	5.3A	 0.33A
	0.63 - 1.37	6.7A	 1.35A
	1.37 - 2.01	6A	 1.65A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.04
	0.04 - 0.25
	0.25 - 0.63
	0.63 - 1.37
	1.37 - 2.01
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.04
	0.04 - 0.25
	0.25 - 0.63
	0.63 - 1.37
	1.37 - 2.01

	Project Name:	NST
	Project Code:	NST	Site ID:	P132	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour