Project Name:	PIN
	Project Code:	PIN	Site ID:	P272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	E. Bettenay	Locality:	Main highway near air strip:
	Date Desc.:	01/02/56	Elevation:	 15 metres
	Map Ref.:	Sheet No. : 2032   1:100000	Rainfall:	0
	Northing/Long.:	115.879722222222	Runoff:	Slow
	Easting/Lat.:	-32.6169444444445	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Rolling plains <9m 10-32%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Bleached-Ferric Mesotrophic Grey Kandosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Podzol
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - , , . *Species includes - None recorded
	Mid Strata - Tree, , . *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.05 m	Greyish brown (10YR5/2-Moist); ; Sand; Field pH 6.5 (pH meter); Diffuse, Smooth change to - 
	A2	0.05 - 0.23 m	Light brownish grey (10YR6/2-Moist); ; Sand; Field pH 6.5 (pH meter); Diffuse, Smooth change 
	to - 
	A3	0.23 - 0.58 m	Light olive grey (5Y6/2-Moist); ; Loamy sand; Field pH 6 (pH meter); Diffuse, Smooth change to - 
	0.58 - 1.02 m	Light olive grey (5Y6/2-Moist); , 2.5Y86; Sandy loam; Field pH 6 (pH meter); 
	1.02 - 1.4 m	Light olive grey (5Y6/2-Moist); , 10YR56; Sandy clay loam; 
	1.4 - 1.73 m	Light olive grey (5Y6/2-Moist); , 10YR56; Sandy medium clay; 20-50%, Substrate material, 
	coarse fragments; 
	Morphological Notes
	Observation Notes
	140-173CM AL GV IS FERRUGINOUS:                                                                                         
	Site Notes
	MURRAY

	Project Name:	PIN
	Project Code:	PIN	Site ID:	P272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.5A	 0.036A	 0.6K	 0.8	 0.08	 0.19
	0.05 - 0.23	5.8A	 0.015A
	0.23 - 0.58	5.6A	 0.015A
	0.58 - 1.02	5.5A	 0.024A	 0.3K	 0.5	 0.01	 0.04	 2.3E	 3.2B
	1.02 - 1.4	6A	 0.042A
	1.4 - 1.73	5.1A	 0.08A	 0.6K	 1.9	 0.04	 0.23	 5.3E	 8.1B
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 0.001D	 0.053B	 57D	 35	 2	 4
	0.05 - 0.23	 0.56D	 0.001D	 0.019B
	0.23 - 0.58	 53D	 37	 2	 8
	0.58 - 1.02	 0.001D	 0.016B	 49D	 33	 2	 16
	1.02 - 1.4
	1.4 - 1.73
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.05 - 0.23
	0.23 - 0.58
	0.58 - 1.02
	1.02 - 1.4
	1.4 - 1.73

	Project Name:	PIN
	Project Code:	PIN	Site ID:	P272	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance