Project Name:	REG
	Project Code:	REG	Site ID:	T237	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	R.F. Isbell	Locality:	9.3KM north of Kalumbaru Mission (Pago Land 
	System):
	Date Desc.:	09/09/74	Elevation:	 50 metres
	Map Ref.:	Sheet No. : 4269   1:100000	Rainfall:	940
	Northing/Long.:	126.625	Runoff:	Slow
	Easting/Lat.:	-14.25	Drainage:	Rapidly drained
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	  Qa	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Firm
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Regolithic Orthic Tenosol     	Principal Profile Form:	Uc4.21
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance other than grazing by hoofed animals
	Vegetation:	Low Strata - Tussock grass, 0.51-1m, Mid-dense. *Species includes - Sorghum plumosum, Triodia mitchelii
	Tall Strata - Tree, 6.01-12m, Sparse. *Species includes - Eucalyptus tetrodonta, Eucalyptus miniata
	Surface Coarse Fragments:	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very firm 
	consistence; Gradual change to - 
	A1	0.1 - 0.2 m	Dark greyish brown (10YR4/2-Moist); ; Sand; Single grain grade of structure; Very firm 
	consistence; 
	A2	0.2 - 0.3 m	Dark yellowish brown (10YR4/4-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Gradual change to - 
	A2	0.3 - 0.6 m	Dark yellowish brown (10YR4/4-Moist); ; Sand; Single grain grade of structure; Very weak 
	consistence; Gradual change to - 
	B2	0.6 - 0.9 m	Yellowish brown (10YR5/6-Moist); ; Sand; Single grain grade of structure; Weak consistence; 
	Gradual change to - 
	B2	0.9 - 1.2 m	Yellowish brown (10YR5/6-Moist); , 5YR78, 2-10% ; , 2-10% ; Sand; Single grain grade of 
	structure; Weak consistence; Gradual change to - 
	B2	1.2 - 1.8 m	Yellowish brown (10YR5/6-Moist); , 5YR78, 2-10% ; , 10YR51, 2-10% ; Sand; Single grain grade
	 of structure; Weak consistence; Clear change to - 
	C	1.8 - 2.1 m	Light grey (10YR7/2-Moist); , 2.5YR68; , 10YR58; Clayey sand; Wet; 
	Morphological Notes
	Observation Notes
	Site Notes
	NTH KIMBERLY

	Project Name:	REG
	Project Code:	REG	Site ID:	T237	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	5.4A	<0.05A	<0.01B	 0.43	 0.03	 0.03	 0.65F	 1.2F
	0.2 - 0.3	5.3A	<0.05A	<0.01B	 0.24	 0.01	 0.01	 0.79F	 1.1F
	0.3 - 0.6	5.3A	<0.05A	<0.01B	 0.17	 0.01	<0.01	 0.85F	 1.1F
	0.9 - 1.2	5.3A	<0.05A	<0.01B	 0.27	 0.01	 0.01	 0.57F	 0.9F
	1.8 - 2.1	5.1A	<0.05A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.7D	 3A	 0.009A	 0.03A	 0.04A	 0	 67A	 24	 1	 6
	 3.2B
	0.2 - 0.3	 0.4D	 3A	 0.009A	 0.016A	 0.04A	 0	 63A	 27	 2	 8
	 2.1B
	0.3 - 0.6	 5A	 0.009A	 0.04A	 0	 60A	 30	 1	 9
	 3.2B
	0.9 - 1.2	 0.007A	 0.05A	 0	 58A	 31	 1	 10
	1.8 - 2.1	 0	 57A	 29	 1	 13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.2 - 0.3
	0.3 - 0.6
	0.9 - 1.2
	1.8 - 2.1

	Project Name:	REG
	Project Code:	REG	Site ID:	T237	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	10A1	Total sulfur - X-ray fluorescence
	12_HF_CU	Total element - Cu(mg/kg) - HF/HClO4 Digest
	12_HF_ZN	Total element - Zn(mg/kg) - HF/HClO4 Digest
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15G_C	Exchange acidity (hydrogen and aluminium) - meq per 100g of soil - By 1M KCl exch. acidity by 
	titration to pH 8.4
	15J1	Effective CEC
	17A1	Total potassium - X-ray fluorescence
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A1	Total phosphorus - X-ray fluorescence
	9B_9C	Available P (mg/kg) - Bicarbonate P - 0.5M NaHCO3 extractable
	9G_BSES	Available P (mg/kg) - Acid P - 0.005M H2SO4 (BSES)
	P10_CF_C	Clay (%) - Coventry and Fett pipette method
	P10_CF_CS	Coarse sand (%) - Coventry and Fett pipette method
	P10_CF_FS	Fine sand (%) - Coventry and Fett pipette method
	P10_CF_Z	Silt (%) - Coventry and Fett pipette method
	P10_GRAV	Gravel (%)