Project Name:	SEA
	Project Code:	SEA	Site ID:	P195	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	2 chains west of Canning River where Seaforth Road 
	crosses river:
	Date Desc.:	19/12/53	Elevation:	No Data
	Map Ref.:	Rainfall:	0
	Northing/Long.:	6448800 AMG zone: 50	Runoff:	Rapid
	Easting/Lat.:	407050  Datum: AGD66	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Silt 
	Land Form
	Rel/Slope Class: 	Undulating plains <9m 3-10%	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Levee	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Regolithic Orthic Tenosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Alluvial soil
	All necessary analytical data are available.
	Site Disturbance:	Complete clearing. Pasture, native or improved, but never cultivated
	Vegetation:
	Tall Strata - Tree, , Isolated plants. *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.13 m	Dark yellowish brown (10YR3/4-Moist); ; Loam (Fibric); Dry; Weak consistence; Moderately 
	plastic; Normal plasticity; Field pH 5.5 (pH meter); Diffuse change to - 
	A2	0.13 - 0.46 m	Dark yellowish brown (10YR3/4-Moist); ; Fine sandy loam; Dry; Loose consistence; Slightly 
	plastic; Normal plasticity; Field pH 6 (pH meter); Diffuse change to - 
	B1	0.46 - 1.55 m	Dark yellowish brown (10YR3/4-Moist); , 10YR33; Fine sandy loam; Dry; Loose consistence; 
	Slightly plastic; Normal plasticity; Field pH 6 (pH meter); 
	B2	1.55 - 1.9 m	Grey (10YR6/1-Moist); , 2.5YR44; Clayey sand; Field pH 6 (pH meter); 
	B3	1.9 - 2.13 m	Light grey (10YR7/1-Moist); , 10YR56; Clayey sand; Field pH 6.5 (pH meter); 
	Morphological Notes
	Observation Notes
	190-213CM CLAYEY SAND WITH CLAY POCKETS:                                                                                
	Site Notes
	SOUTH-WEST LD

	Project Name:	SEA
	Project Code:	SEA	Site ID:	P195	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.13	5.4A
	0.13 - 0.46	5.7A
	0.46 - 1.55	5.4A
	1.55 - 1.9	5.5A
	1.9 - 2.13	5.4A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.13	 7.98D	 0.04D	 0.401B	 20D	 44	 23	 14
	0.13 - 0.46
	0.46 - 1.55	 36D	 43	 10	 12
	1.55 - 1.9
	1.9 - 2.13
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.13
	0.13 - 0.46
	0.46 - 1.55
	1.55 - 1.9
	1.9 - 2.13

	Project Name:	SEA
	Project Code:	SEA	Site ID:	P195	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance