Project Name:	SES
	Project Code:	SES	Site ID:	P41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	K. Fitzgerald	Locality:	Cooper's main gate:
	Date Desc.:	16/02/50	Elevation:	No Data
	Map Ref.:	Sheet No. : 2529   1:100000	Rainfall:	0
	Northing/Long.:	118.3175	Runoff:	Slow
	Easting/Lat.:	-34.4941666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Unconsolidated material (unidentified) 
	Land Form
	Rel/Slope Class: 	Level plain <9m <1%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Plain	Slope Category:	Level
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Calcic Mottled-Mesonatric Brown Sodosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:
	Tall Strata - Tree, , . *Species includes - Eucalyptus tetrodonta
	Surface Coarse Fragments:
	Profile Morphology
	A1	0 - 0.025 m	Greyish brown (10YR5/2-Moist); ; Fine sand (Fibric); Single grain grade of structure; Smooth 
	change to - 
	A2	0.025 - 0.15 m	Light brownish grey (10YR6/2-Moist); ; Fine sand; Single grain grade of structure; 2-10%, 
	Substrate material, coarse fragments; Diffuse, Smooth change to - 
	B1	0.23 - 0.46 m	Brown (10YR4/3-Moist); , 10YR56; , 5YR44; Sandy medium clay; Massive grade of structure; 
	Diffuse, Irregular change to - 
	B2	0.51 - 0.96 m	Yellowish brown (10YR5/6-Moist); , 10YR52; Sandy medium clay; 2-10%, Gravel, coarse 
	fragments; Diffuse change to - 
	C1	0.99 - 1.07 m	Greyish brown (10YR5/2-Moist); , 10YR56; Sandy medium clay; 20-50%, Charcoal, coarse 
	fragments; Diffuse change to - 
	Morphological Notes
	Observation Notes
	51-96CM GV = SPONGOLITE AND CHERT PIECES:99-107CM SPONGOLITE FRAGMENTS ALSO:                                            
	Site Notes

	Project Name:	SES
	Project Code:	SES	Site ID:	P41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.025	6A	 0.021A
	0.025 - 0.15	6A	 0.018A
	0.23 - 0.46	7.3A	 0.199A	 1K	 4.5	 0.83	 1.74	 8.1B
	0.51 - 0.96	9.4A	 0.958A
	0.99 - 1.07	9.3A	 1.31A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.025	 0.54D	 0.001D	 0.022B	<1	 51D	 44	 3	 2
	0.025 - 	 0.35D	 0.001D	 0.015B	 6	 46D	 49	 4	<1
	0.15
	0.23 - 0.46	 0.02A	 0.4D	 0.002D	 0.028B	 2	 32D	 39	 2	 27
	0.51 - 0.96	 4.07A	 0.14D	 0.003D	 0.01B	 9	 24D	 35	 2	 39
	0.99 - 1.07	 5.1A	 0.07D	 0.003D	 0.006B	 26	 27D	 30	 0	 42
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.025
	0.025 - 0.15
	0.23 - 0.46
	0.51 - 0.96
	0.99 - 1.07

	Project Name:	SES
	Project Code:	SES	Site ID:	P41	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	19A1	Carbonates - rapid titration
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance