Project Name:	SOU
	Project Code:	SOU	Site ID:	P738	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Logging Road 2.5KM from Thomson Road:
	Date Desc.:	02/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2228   1:100000	Rainfall:	0
	Northing/Long.:	116.683333333333	Runoff:	No Data
	Easting/Lat.:	-34.9166666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Dystrophic Brown Chromosol     	Principal Profile Form:	Dy5.52
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:	Limited clearing, for example selective logging
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); ; Loamy sand; Weak grade of structure; Loose 
	consistence; 2-10%, Substrate material, coarse fragments; 
	0.05 - 0.1 m	Strong brown (7.5YR5/6-Moist); ; Sand; Single grain grade of structure; 2-10%, Substrate 
	material, coarse fragments; 
	0.1 - 0.2 m	Reddish yellow (7.5YR6/6-Moist); ; Sand; Single grain grade of structure; 2-10%, Substrate 
	material, coarse fragments; 
	0.2 - 0.4 m	Reddish yellow (7.5YR6/6-Moist); ; Loamy sand; 2-10%, Substrate material, coarse fragments; 
	0.4 - 0.6 m	Strong brown (7.5YR5/8-Moist); ; Sandy loam; Very weak consistence; 2-10%, Substrate 
	material, coarse fragments; 
	0.6 - 0.8 m	Strong brown (7.5YR5/8-Moist); ; Sandy loam (Heavy); Very firm consistence; 0-2%, Substrate 
	material, coarse fragments; 
	0.8 - 1 m	Yellowish brown (10YR5/8-Moist); ; Loamy sand; Loose consistence; 50-90%, Substrate 
	material, coarse fragments; 
	1 - 1.2 m	Yellowish brown (10YR5/8-Moist); ; Loamy sand; 50-90%, Substrate material, coarse fragments;
	1.2 - 1.4 m	Yellowish brown (10YR5/8-Moist); , 5YR44; Sandy medium clay; Massive grade of structure; 
	Very firm consistence; 2-10%, Substrate material, coarse fragments; 
	1.4 - 1.6 m	Yellowish brown (10YR5/8-Moist); , 7.5YR44; , 5YR44; Sandy medium clay; Massive grade of 
	structure; Very firm consistence; 2-10%, Substrate material, coarse fragments; 
	Morphological Notes
	Observation Notes
	GRAVELS THROUGHOUT PROFILE FERRUGINISED:140-160CM SOME QUARTZ GRIT ALSO:                                                
	Site Notes

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P738	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	6.6A	 0.006A	 1.97K	 0.53	 0.16	 0.08
	0.1 - 0.2	6.5A	 0.006A	 0.94K	 0.46	 0.05	 0.19
	0.4 - 0.6	6.8A	 0.003A
	0.8 - 1	6.8A	 0.003A	 0.66K	 0.3	 0.11	 0.08
	1.2 - 1.4	6.7A	 0.003A	 0.49K	 0.34	 0.11	 0.08
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 1.65D
	0.1 - 0.2
	0.4 - 0.6
	0.8 - 1
	1.2 - 1.4	 48D	 34	 3	 17
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.1 - 0.2
	0.4 - 0.6
	0.8 - 1
	1.2 - 1.4

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P738	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance