Project Name:	SOU
	Project Code:	SOU	Site ID:	P759	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	W.M. MacArthur	Locality:	Nutcracker Road 3.6KM west of Stan Road: flank of 
	Mt. Lindsay:
	Date Desc.:	04/11/82	Elevation:	No Data
	Map Ref.:	Sheet No. : 2328   1:100000	Rainfall:	0
	Northing/Long.:	117.316666666667	Runoff:	No Data
	Easting/Lat.:	-34.8666666666667	Drainage:	No Data
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Mountains
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):	Hardsetting
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Mottled Magnesic-Natric Brown Kurosol     	Principal Profile Form:	Dy5.81
	ASC Confidence:	Great Soil Group:	Yellow podzolic soil
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Very dark grey (10YR3/1-Moist); ; Loamy sand; Single grain grade of structure; 20-50%, fine 
	gravelly, 2-6mm, Quartz, coarse fragments; 
	0.05 - 0.1 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; 
	0.1 - 0.2 m	Light brownish grey (10YR6/2-Moist); ; Sand; Single grain grade of structure; 2-10%, Quartz, 
	coarse fragments; 
	0.2 - 0.3 m	Greyish brown (10YR5/2-Moist); ; Sand; Single grain grade of structure; Firm consistence; 10-
	20%, Quartz, coarse fragments; 
	0.3 - 0.4 m	Yellowish brown (10YR5/6-Moist); , 10YR32; Medium clay; Moderate grade of structure, Angular 
	blocky; Fine, (0 - 5) mm crack; 20-50%, Quartz, coarse fragments; 
	0.4 - 0.5 m	Yellowish brown (10YR5/8-Moist); , 10YR52; , 10YR43; Medium clay; Moderate grade of 
	structure, Angular blocky; Fine, (0 - 5) mm crack; Very firm consistence; 10-20%, Quartz, coarse 
	fragments; 
	0.5 - 0.7 m	Pale brown (10YR6/3-Moist); , 10YR56; Medium clay; 10-20%, Quartz, coarse fragments; 
	0.8 - 0.9 m	Pale olive (5Y6/3-Moist); ; Medium clay; Massive grade of structure; 2-10%, Quartz, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	80-90CM PROBABLY SAPROLITE:30-50CM ORGANIC STAINS ALONG FRACTURE FACES:                                                 
	Site Notes

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P759	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05	5.4A	 0.003A	 2.89K	 1.55	 0.15	 0.21
	0.1 - 0.2	5A	 0.003A	 0.82K	 1.28	 0.07	 0.09
	0.3 - 0.4	5.2A	 0.006A
	0.5 - 0.7	5.3A	 0.003A	 0.12K	 1.43	 0.28	 0.17
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	 5.9D
	0.1 - 0.2
	0.3 - 0.4
	0.5 - 0.7	 37D	 16	 4	 43
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05
	0.1 - 0.2
	0.3 - 0.4
	0.5 - 0.7

	Project Name:	SOU
	Project Code:	SOU	Site ID:	P759	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance