Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FNW14-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	F.J. Hingston	Locality:	P. Last, Merredin
	Date Desc.:	01/01/67	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	118.2833233	Runoff:	No Data
	Easting/Lat.:	-31.583333	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.62
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Confidence level not specified	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.05 m	Brown (10YR5/3-Moist); , 0-2% ; Fine sand; 2-10%, coarse fragments; 
	0.05 - 0.1 m	Brown (10YR5/3-Moist); , 0-2% ; Fine sand; 2-10%, coarse fragments; 
	0.1 - 0.15 m	Light yellowish brown (10YR6/4-Moist); , 0-2% ; Fine sand; 2-10%, coarse fragments; 
	0.15 - 0.2 m	Light yellowish brown (10YR6/4-Moist); , 0-2% ; Fine sand; 2-10%, coarse fragments; 
	0.2 - 0.3 m	Light yellowish brown (10YR6/4-Moist); , 0-2% ; Loamy sand; 2-10%, coarse fragments; 
	0.3 - 0.4 m	Light yellowish brown (10YR6/4-Moist); , 0-2% ; Sandy loam; 20-50%, coarse fragments; 
	0.4 - 0.5 m	Reddish yellow (5YR6/6-Moist); , 20-50% ; Light clay; 20-50%, coarse fragments; 
	0.5 - 0.6 m	Reddish yellow (5YR6/6-Moist); , 20-50% ; Light clay; 2-10%, coarse fragments; 
	0.6 - 0.7 m	Reddish yellow (5YR6/8-Moist); , 20-50% ; Light clay; 2-10%, coarse fragments; 
	0.7 - 0.8 m	Light reddish brown (5YR6/4-Moist); , 20-50% ; Light clay; 2-10%, coarse fragments; 
	0.8 - 0.9 m	Light reddish brown (5YR6/4-Moist); , 20-50% ; Light clay; 2-10%, coarse fragments; 
	0.9 - 1 m	Yellow (10YR7/8-Moist); , 20-50% ; Sandy clay loam; 2-10%, coarse fragments; 
	Morphological Notes
	Observation Notes
	Soil parent material - laterite
	Site Notes

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FNW14-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05
	0 - 0.1	5.72I	0.9B	0.3	0.2	0.2	11M	2.9A	1.6D	6.90
	0.05 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	65C	22	2	8
	0 - 0.1	0.56G	11H	0.04A	1.52	5
	3.2I
	3.7G
	13.2F
	0.05 - 0.1	58C	28	2	8
	0.1 - 0.15	57C	29	4	9
	0.15 - 0.2	54C	29	4	12
	0.2 - 0.3	53C	33	5	10
	0.3 - 0.4
	0.4 - 0.5	46C	27	5	20
	0.5 - 0.6	48C	24	5	21
	0.6 - 0.7	45C	27	6	21
	0.7 - 0.8	44C	26	8	21
	0.8 - 0.9	50C	30	4	15
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	3.7A
	0 - 0.1
	0.05 - 0.1	3.6A
	0.1 - 0.15	4.2A
	0.15 - 0.2	6.5A
	0.2 - 0.3	4.4A
	0.3 - 0.4	7.7A
	0.4 - 0.5	11A
	0.5 - 0.6	9.9A
	0.6 - 0.7	9.9A
	0.7 - 0.8	11.1A
	0.8 - 0.9	9.4A
	0.9 - 1

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FNW14-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FNW14-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F4	Exchangeable aluminium by 1M ammonium acetate (pH5.8). Abdullah and Riley (1966).
	15J_BASES	Sum of Bases
	18E2	Fluoride-extractable potassium (Bray 1-K) - AAS
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5A_C_2.5	Chloride - 1:2.5 soil/water extract
	6B1	Total organic carbon - Heanes wet oxidation
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1d	(Ammonium+nitrate)-N, in presence of nitrite
	7C1e	Nitrate-N, in presence of nitrite
	7D1	CaSO4 extractable nitrate. O'Brien and Fiore (1962)
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour
	9D2	Lactate-extractable phosphorus - automated colour
	9E2	Fluoride-extractable phosphorus (Bray 1-P) - automated colour
	P10_GRAV	Gravel (%)
	P10_NR_C	Clay (%) - Not recorded
	P10_NR_CS	Coarse sand (%) - Not recorded
	P10_NR_FS	Fine sand (%) - Not recorded
	P10_NR_Z	Silt (%) - Not recorded
	P3A_NR	Bulk density - Not recorded
	P3B_NR_15	15 BAR Moisture % - Not recorded