Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW2-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	F.J. Hingston	Locality:	K.Cahill, Merredin
	Date Desc.:	01/01/67	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	118.15	Runoff:	No Data
	Easting/Lat.:	-31.5	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Gc2.1
	ASC Confidence:	Great Soil Group:	Solonized brown 
	Confidence level not specified	soil
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.05 m	Reddish brown (5YR4/4-Moist); , 0-2% ; Clay loam; 0-2%, coarse fragments; 
	A	0.05 - 0.1 m	Yellowish red (5YR4/6-Moist); , 0-2% ; Clay loam; 0-2%, coarse fragments; 
	A	0.1 - 0.15 m	Yellowish red (5YR4/8-Moist); , 0-2% ; Clay loam; 0-2%, coarse fragments; 
	A	0.15 - 0.2 m	Yellowish red (5YR4/8-Moist); , 0-2% ; Clay loam; 0-2%, coarse fragments; 
	A	0.2 - 0.3 m	Strong brown (7.5YR5/8-Moist); , 0-2% ; Light clay; 0-2%, coarse fragments; 
	A	0.3 - 0.4 m	Strong brown (7.5YR5/6-Moist); , 0-2% ; Light clay; 0-2%, coarse fragments; 
	0.4 - 0.5 m	Strong brown (7.5YR5/8-Moist); , 0-2% ; Light clay; 0-2%, coarse fragments; 
	0.5 - 0.6 m	Strong brown (7.5YR5/8-Moist); , 0-2% ; Light clay; 0-2%, coarse fragments; 
	0.6 - 0.7 m	Yellowish red (5YR5/8-Moist); , 0-2% ; Light clay; 0-2%, coarse fragments; 
	0.7 - 0.8 m	Yellowish red (5YR5/8-Moist); , 0-2% ; Medium heavy clay; 0-2%, coarse fragments; 
	0.8 - 0.9 m	Yellowish red (5YR4/8-Moist); , 0-2% ; Medium heavy clay; 0-2%, coarse fragments; 
	0.9 - 1 m	Yellowish red (5YR4/8-Moist); ; Medium heavy clay; 0-2%, coarse fragments; 
	Morphological Notes
	Observation Notes
	Soil parent material - lake parna
	Site Notes

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW2-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05
	0 - 0.1	8.07I	0.29E	76.3M
	0.05 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	11.1I
	0 - 0.1	1.26G	13.7H	0.11A	1.20
	7.6G
	28.3F
	0.05 - 0.1	4.8I
	0.1 - 0.15	2.3I
	0.15 - 0.2	2.1I
	0.2 - 0.3	2.5I
	0.3 - 0.4	1.5I
	0.4 - 0.5	1.5I
	0.5 - 0.6	1.6I
	0.6 - 0.7	2I
	0.7 - 0.8	1.8I
	0.8 - 0.9	1.4I
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	10.2A
	0 - 0.1
	0.05 - 0.1	7.7A
	0.1 - 0.15	9.4A
	0.15 - 0.2	10.4A
	0.2 - 0.3	13A
	0.3 - 0.4	11.4A
	0.4 - 0.5	11.7A
	0.5 - 0.6	14.9A
	0.6 - 0.7	13.5A
	0.7 - 0.8	12A
	0.8 - 0.9	16.1A
	0.9 - 1

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW2-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15F4	Exchangeable aluminium by 1M ammonium acetate (pH5.8). Abdullah and Riley (1966).
	3A_C_2.5	EC of 1:2.5 soil/water extract
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5A_C_2.5	Chloride - 1:2.5 soil/water extract
	6B1	Total organic carbon - Heanes wet oxidation
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1d	(Ammonium+nitrate)-N, in presence of nitrite
	7C1e	Nitrate-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9BUFF_0	Buffering Capacity by 0.01M CaCl2, solution of 0 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_0.5	Buffering Capacity by 0.01M CaCl2, solution of 0.5 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_1	Buffering Capacity by 0.01M CaCl2, solution of 1 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_2	Buffering Capacity by 0.01M CaCl2, solution of 2 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_4	Buffering Capacity by 0.01M CaCl2, solution of 4 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9C2	Olsen-extractable phosphorus - automated colour
	9D2	Lactate-extractable phosphorus - automated colour
	9E2	Fluoride-extractable phosphorus (Bray 1-P) - automated colour
	9R1	Resin extractable phosphorus - automated colour (CSIRO Div of Soil Tech Mem 63/1972)
	P3A_NR	Bulk density - Not recorded
	P3B_NR_15	15 BAR Moisture % - Not recorded