Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW20-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	F.J. Hingston	Locality:	R. Lloyd, Dumbleyung
	Date Desc.:	01/01/67	Elevation:	No Data
	Map Ref.:	1:100000	Rainfall:	No Data
	Northing/Long.:	117.816667	Runoff:	No Data
	Easting/Lat.:	-33.8	Drainage:	No Data
	Geology
	ExposureType:	Undisturbed soil core	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Granite 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	 N/A    	Principal Profile Form:	Dy3.43
	ASC Confidence:	Great Soil Group:	Solodic soil
	Confidence level not specified
	Site Disturbance:	Cultivation. Rainfed
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	A	0 - 0.05 m	Dark greyish brown (10YR4/2-Moist); , 0-2% ; Fine sand; 0-2%, coarse fragments; 
	A	0.05 - 0.1 m	Dark greyish brown (10YR4/2-Moist); , 0-2% ; Fine sand; 0-2%, coarse fragments; 
	A	0.1 - 0.15 m	Greyish brown (10YR5/2-Moist); , 0-2% ; Fine sand; 0-2%, coarse fragments; 
	A	0.15 - 0.2 m	Greyish brown (10YR5/2-Moist); , 0-2% ; Fine sand; 0-2%, coarse fragments; 
	A	0.2 - 0.3 m	Pale brown (10YR6/3-Moist); , 2-10% ; Coarse sand; 0-2%, coarse fragments; 
	A	0.3 - 0.4 m	Very pale brown (10YR7/3-Moist); , 2-10% ; Coarse sand; 0-2%, coarse fragments; 
	A	0.4 - 0.5 m	Light grey (10YR7/2-Moist); , 2-10% ; Coarse sand; 0-2%, coarse fragments; 
	0.5 - 0.6 m	Yellowish brown (10YR5/6-Moist); , 20-50% ; Coarse sand; 0-2%, coarse fragments; 
	0.6 - 0.7 m	Brownish yellow (10YR6/6-Moist); , 20-50% ; Medium heavy clay; 0-2%, coarse fragments; 
	0.7 - 0.8 m	Brownish yellow (10YR6/6-Moist); , 20-50% ; Clay loam, sandy; 0-2%, coarse fragments; 
	0.8 - 0.9 m	Brownish yellow (10YR6/8-Moist); , 20-50% ; Clay loam, sandy; 0-2%, coarse fragments; 
	0.9 - 1 m	Brownish yellow (10YR6/8-Moist); , 20-50% ; Clay loam, sandy; 0-2%, coarse fragments; 
	Morphological Notes
	Observation Notes
	Soil parent material - laterite
	Site Notes

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW20-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.05
	0 - 0.1	6.26I	0.119E	2B	0.6	0.1	0.4	12M	3.6A	3.1D	11.11
	0.05 - 0.1
	0.1 - 0.15
	0.15 - 0.2
	0.2 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 0.9
	0.9 - 1
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.05	20I
	0 - 0.1	1.09G	14.2H	0.08A	1.34	2
	10.8G
	14.8F
	0.05 - 0.1	12.4I
	0.1 - 0.15	4.8I
	0.15 - 0.2	3I
	0.2 - 0.3	1.1I
	0.3 - 0.4	0.4I
	0.4 - 0.5	0.2I
	0.5 - 0.6	0.3I
	0.6 - 0.7	0.4I
	0.7 - 0.8	0.4I
	0.8 - 0.9	0.4I
	0.9 - 1
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.05	3.6A
	0 - 0.1
	0.05 - 0.1	2.7A
	0.1 - 0.15	1.8A
	0.15 - 0.2	1.7A
	0.2 - 0.3	1.6A
	0.3 - 0.4	5A
	0.4 - 0.5	9.1A
	0.5 - 0.6	8.6A
	0.6 - 0.7	10.9A
	0.7 - 0.8	10.6A
	0.8 - 0.9	10.1A
	0.9 - 1

	Project Name:	Wheat experiments in Western Australia - 1967,1968 & 1970
	Project Code:	WAWheatEx	Site ID:	FPW20-67	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15A2_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, pretreatment for 
	soluble salts
	15A2_CEC	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_K	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_MG	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15A2_NA	Exchangeable bases- 1M ammonium chloride at pH 7.0, pretreatment for soluble salts
	15F4	Exchangeable aluminium by 1M ammonium acetate (pH5.8). Abdullah and Riley (1966).
	15J_BASES	Sum of Bases
	3A_C_2.5	EC of 1:2.5 soil/water extract
	4A_C_2.5	pH of soil - pH of 1:2.5 soil/water suspension
	5A_C_2.5	Chloride - 1:2.5 soil/water extract
	6B1	Total organic carbon - Heanes wet oxidation
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1d	(Ammonium+nitrate)-N, in presence of nitrite
	7C1e	Nitrate-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9BUFF_0	Buffering Capacity by 0.01M CaCl2, solution of 0 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_0.5	Buffering Capacity by 0.01M CaCl2, solution of 0.5 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_1	Buffering Capacity by 0.01M CaCl2, solution of 1 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_2	Buffering Capacity by 0.01M CaCl2, solution of 2 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9BUFF_4	Buffering Capacity by 0.01M CaCl2, solution of 4 ppm phosphorus added (CSIRO Div of Soil Tech 
	Mem 63/1972)
	9C2	Olsen-extractable phosphorus - automated colour
	9D2	Lactate-extractable phosphorus - automated colour
	9E2	Fluoride-extractable phosphorus (Bray 1-P) - automated colour
	9R1	Resin extractable phosphorus - automated colour (CSIRO Div of Soil Tech Mem 63/1972)
	P10_GRAV	Gravel (%)
	P3A_NR	Bulk density - Not recorded
	P3B_NR_15	15 BAR Moisture % - Not recorded