Project Name:	YRK
	Project Code:	YRK	Site ID:	P302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Information
	Desc. By:	M.J. Mulcahy	Locality:	L.D. 2/80 in the south west corner of block Z:
	Date Desc.:	19/09/56	Elevation:	No Data
	Map Ref.:	Sheet No. : 2234   1:100000	Rainfall:	460
	Northing/Long.:	116.929166666667	Runoff:	Rapid
	Easting/Lat.:	-31.7983333333333	Drainage:	Moderately well drained
	Geology
	ExposureType:	No Data	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Gneiss 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	No Data
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	Gently inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Ferric Eutrophic Yellow Chromosol     	Principal Profile Form:	N/A
	ASC Confidence:	Great Soil Group:	Lateritic podzolic 
	Analytical data are incomplete but reasonable confidence.	soil
	Site Disturbance:
	Vegetation:
	Tall Strata - Tree, , . *Species includes - None Recorded
	Surface Coarse Fragments:
	Profile Morphology
	0 - 0.14 m	Pale brown (10YR6/3-Moist); ; Sand; Single grain grade of structure; Loose consistence; 50-
	90%, Substrate material, coarse fragments; 
	0.19 - 0.32 m	Light yellowish brown (10YR6/4-Moist); ; Loamy sand; 50-90%, Substrate material, coarse 
	fragments; Sharp change to - 
	0.34 - 0.53 m	Yellowish brown (10YR5/4-Moist); , 2.5YR44; Sandy loam; 50-90%, Substrate material, coarse 
	fragments; 
	0.76 - 0.86 m	Brownish yellow (10YR6/8-Moist); , 10R34; Loam; 2-10%, Substrate material, coarse fragments; 
	0.96 - 1.07 m	Brownish yellow (10YR6/8-Moist); , 10R34; , 10R53; Loam; 2-10%, Substrate material, coarse 
	fragments; 
	1.17 - 1.22 m	Dark reddish brown (2.5YR3/4-Moist); , 10YR68; Sandy loam; 
	1.37 - 1.42 m	Dark reddish brown (2.5YR3/4-Moist); , 10YR68; Sandy loam; 
	1.47 - 1.57 m	Brownish yellow (10YR6/6-Moist); , 2.5YR34, 2-10% ; , 2-10% ; Sandy loam; 2-10%, fine gravelly,
	 2-6mm, Quartz, coarse fragments; 
	1.68 - 1.73 m	Brownish yellow (10YR6/6-Moist); , 2.5YR34, 2-10% ; , 2.5YR54, 2-10% ; Sandy loam; 10-20%, 
	fine gravelly, 2-6mm, Quartz, coarse fragments; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), 
	Concretions; 
	2.13 - 2.23 m	Brownish yellow (10YR6/6-Moist); , 2.5YR34; Loam; 10-20%, fine gravelly, 2-6mm, Quartz, 
	coarse fragments; Few (2 - 10 %), Ferruginous, Fine (0 - 2 mm), Concretions; 
	2.44 - 2.49 m	Brownish yellow (10YR6/6-Moist); , 2.5YR34; Clay loam; 2-10%, Gravel, coarse fragments; 
	2.49 - 2.59 m	Brownish yellow (10YR6/6-Moist); , 2.5YR34; , 2.5YR54; Clay loam; 2-10%, Gravel, coarse 
	fragments; 
	Morphological Notes
	Observation Notes
	0-53CM AL GV IS FERRUGINOUS ALSO HAS <10% QZ GRIT:117-142CM MATRIX + MOTTLES LAMINATED:                            

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Site Notes
	YORK

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.14	6.2A	 0.033A	 2.4K	 0.8	 0.18	 0.04	 2.8E	 6.2B
	0.19 - 0.32	6.4A	 0.018A	 1.3K	 1.1	 0.06	 0.04	 1.6E	 4.1B
	0.34 - 0.53	6.5A	 0.036A	 1.6K	 2.1	 0.07	 0.12	 3.2E	 7.1B
	0.76 - 0.86	6.2A	 0.051A
	0.96 - 1.07	6A	 0.033A	 1.5K	 2.4	 0.05	 0.2
	1.17 - 1.22	6.1A	 0.033A
	1.37 - 1.42	6A	 0.033A
	1.47 - 1.57	6A	 0.03A	 1.3K	 1.8	 0.02	 0.19
	1.68 - 1.73	6A	 0.033A
	2.13 - 2.23	6A	 0.039A
	2.44 - 2.49	6.1A	 0.045A
	2.49 - 2.59	6.1A	 0.048A	 0.8K	 3.7	 0.05	 0.46
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.14	 0.25D	 0.008D	 0.088B	 42	 49D	 40	 4	 5
	0.19 - 0.32	 0.005D	 49	 48D	 39	 4	 10
	0.34 - 0.53	 0.005D	 59	 40D	 24	 7	 29
	0.76 - 0.86
	0.96 - 1.07	 32D	 32	 14	 20
	1.17 - 1.22
	1.37 - 1.42
	1.47 - 1.57	 38D	 30	 13	 17
	1.68 - 1.73
	2.13 - 2.23
	2.44 - 2.49
	2.49 - 2.59	 17D	 27	 19	 32
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.14
	0.19 - 0.32
	0.34 - 0.53
	0.76 - 0.86
	0.96 - 1.07
	1.17 - 1.22
	1.37 - 1.42
	1.47 - 1.57
	1.68 - 1.73
	2.13 - 2.23
	2.44 - 2.49
	2.49 - 2.59

	Project Name:	YRK
	Project Code:	YRK	Site ID:	P302	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (WA)
	Laboratory Analyses Completed for this profile
	15_NR_CA	Exch. basic cations (Ca++) - meq per 100g of soil - Not recorded
	15_NR_K	Exch. basic cations (K++) - meq per 100g of soil - Not recorded
	15_NR_MG	Exch. basic cations (Mg++) - meq per 100g of soil - Not recorded
	15_NR_NA	Exch. basic cations (Na++) - meq per 100g of soil - Not recorded
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7_NR	Total nitrogen (%) - Not recorded
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance