Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C1	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Property owner, Robert Addison
	Date Desc.:	27/09/05	Elevation:	100 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	950
	Northing/Long.:	5434173 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	455484  Datum: GDA94	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Tb	Substrate Material:	Basalt 
	Landform
	Rel/Slope Class: 	Undulating low hills 30-90m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	72 degrees
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thick Non-gravelly Clay-loamy 	Principal Profile Form:	N/A
	Clayey Medium
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	0-2%, cobbly, 60-200mm, , 
	Profile Morphology
	Ap	0 - 0.3 m	Reddish brown (5YR5/3-Moist); , 0-0% ; Clay loam; Strong grade of structure, 5-10 mm, Polyhedral; 
	Strong grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Few (<1 per 100mm2) Fine (1-2mm) 
	macropores, Moderately moist; Weak consistence; Slightly plastic; Very sticky; Very few (0 - 2 %), 
	Ferruginous, Medium (2 -6 mm), Nodules; Common, very fine (0-1mm) roots; Abrupt, Smooth change to 
	- 
	B1t	0.3 - 0.45 m	Dark reddish brown (5YR3/4-Moist); Substrate influence, 2.5YR36, 0-2% , 5-15mm, Distinct; Clay loam; 
	Moderate grade of structure, 10-20 mm, Subangular blocky; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Rough-ped fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately 
	moist; Weak consistence; Slightly plastic; Very sticky; 0-2%, coarse gravelly, 20-60mm, subangular, 
	dispersed, coarse fragments; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; Few, very 
	fine (0-1mm) roots; Gradual, Smooth change to - 
	B21t	0.45 - 0.8 m	Dark red (2.5YR3/6-Moist); Mottles, 5YR53, 0-2% , 0-5mm, Faint; Substrate influence, 2.5YR36, 0-2% , 
	0-5mm, Distinct; Clay loam; Moderate grade of structure, 10-20 mm, Subangular blocky; Moderate grade
	 of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak consistence; Slightly 
	plastic; Very sticky; Very few (0 - 2 %), Ferruginous, Medium (2 -6 mm), Nodules; Gradual, Smooth 
	change to - 
	B22t	0.8 - 1.1 m	Dark red (2.5YR3/6-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 10-20 mm, Subangular 
	blocky; Moderate grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Moderately moist; Weak 
	consistence; Slightly plastic; Very sticky; 
	Morphological Notes
	Ap	Penetration resistance: Soft
	B1t	Penetration resistance: Firm. B1T Horizon sampled from .30 to .40m, Label C1C.
	B21t	Penetration resistance: Stiff. B21T Horizon sampled from .50 to .80m, Label C1D.
	B22t	Penetration resistance: Very Stiff. B22T Horizon sampled from .85 to 1.10m, Label C1E.
	Observation Notes
	Poppy regrowth. Ryegrass pasture sprayed off. Substrate not reached during Soil Pit observation but positively Tertiary Basalt. Soil Class is
	 Burnie Clay Loam
	Site Notes
	 Geomorphic activity was eroded with the geomorphic agent Sheet wash. The inundation frequency is no inundation.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C1	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5C	0.101A	10.21A	2.49	1.13	0.31	0.1D	14.39B
	5.8A	0G
	0.25A
	0.2 - 0.275	5.2C	0.045A	7.92A	1.62	0.54	0.17	0.1D	10.39B
	6.1A	0.09G
	0.14A
	0.3 - 0.4	5.5C	0.038A	6.31A	0.71	0.13	0.21	0.02635D	7.39635B
	5.9A	0G
	0.03635A
	0.5 - 0.8	5.7C	0.064A	5.9A	0.54	0.09	0.26	0.01135D	6.81135B
	5.9A	0G
	0.02135A
	0.85 - 1.1	5.7C	0.06A	5.17A	1.16	0.1	0.23	0.01D	6.68B
	5.9A	0G
	0.02A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	4.31B	213H	0.36D
	73I
	0.2 - 0.275	2.75B	56H	0.22D
	12I
	0.3 - 0.4	1.67B	5H	0.11D
	1.9I
	0.5 - 0.8	0.77B	4H	0.08D
	1.2I
	0.85 - 1.1	0.54B	4H	0.07D
	1.5I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C1	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour