Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C10	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Property owner, Brian Bonde. Property name, Main Farm. 
	Site located in Slaughterhouse paddock.
	Date Desc.:	17/11/05	Elevation:	140 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	1108
	Northing/Long.:	5439842 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	426116  Datum: GDA94	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Tb	Substrate Material:	Basalt 
	Landform
	Rel/Slope Class: 	Rolling low hills 30-90m 10-32%	Pattern Type:	Hills
	Morph. Type:	Upper-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	12 % 	Aspect:	20 degrees
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Red Ferrosol Thick Non-gravelly Clay-loamy 	Principal Profile Form:	N/A
	Clay-loamy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A11p	0 - 0.12 m	Dark reddish brown (5YR3/4-Moist); Mottles, 2.5YR34, 0-0% ; Clay loam; Strong grade of structure, 10-
	20 mm, Subangular blocky; Moderate grade of structure, 5-10 mm, Polyhedral; Rough-ped fabric; Few 
	(<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak consistence; Non-plastic; 
	Moderately sticky; Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	A12p	0.12 - 0.3 m	Dark reddish brown (5YR3/4-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moderate grade of structure, 2-5 mm, Polyhedral; Rough-ped fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak consistence; Non-plastic; 
	Moderately sticky; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -6 mm), Nodules; Common, very 
	fine (0-1mm) roots; Sharp, Smooth change to - 
	B1t	0.3 - 0.6 m	Dark reddish brown (2.5YR3/4-Moist); Mottles, 7.5YR46, 0-2% , 0-5mm; Clay loam; Moderate grade of 
	structure, 20-50 mm, Subangular blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; 
	Rough-ped fabric; Moist; Firm consistence; Non-plastic; Moderately sticky; 2-10%, coarse gravelly, 20-
	60mm, subrounded, dispersed, Basalt, coarse fragments; Few (2 - 10 %), Ferromanganiferous, Medium 
	(2 -6 mm), Nodules; Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B2t	0.6 - 1 m	Dark reddish brown (2.5YR3/4-Moist); Mottles, 0-2% , 0-5mm; Clay loam; Moderate grade of structure, 
	50-100 mm, Subangular blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; Rough-ped 
	fabric; Moist; Firm consistence; Slightly plastic; Slightly sticky; 2-10%, coarse gravelly, 20-60mm, 
	subrounded, dispersed, Basalt, coarse fragments; Very few (0 - 2 %), Ferromanganiferous, Medium (2 -
	6 mm), Nodules; Few, very fine (0-1mm) roots; 
	Morphological Notes
	A11p	Penetration resistance: Soft
	A12p	Penetration resistance: Firm
	B1t	Penetration resistance: Stiff. B1 Horizon sampled from .30 to .55m, Label C10C.
	B2t	Penetration resistance: Stiff. B2 Horizon sampled from .65 to .95m, Lable C10D.
	Observation Notes
	Substrate of Tertiary Basalt not reached during Soil Pit observation. Soil class is Burnie or Lapoinya. Vegetaion is Rye grass Pasture

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C10	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Notes
	Element Slope Class: Gentle. Geomophic Activity is Eroded and the Geomorphic Agent is Volcanic. The inundaion frequency is no 
	inundation.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C10	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.4C	0.064A	14.34A	2.34	1.01	0.19	0.1D	18.02B
	6A	0.09G
	0.14A
	0.2 - 0.275	5.4C	0.057A	14.5A	2.11	0.85	0.19	0D	17.68B
	6.2A	0.07G
	0.03A
	0.3 - 0.55	4.8C	0.065A	7.49A	0.6	0.15	0.27	0D	8.84B
	5.5A	0.64G
	0.33A
	0.65 - 0.95	4.9C	0.062A	6.37A	0.33	0.12	0.25	0D	7.34B
	5.5A	1.32G
	0.27A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	4.32B	225H	0.4D
	51.5I
	0.2 - 0.275	4.28B	170H	0.39D
	39.7I
	0.3 - 0.55	1.28B	12H	0.17D
	3.5I
	0.65 - 0.95	0.98B	10H	0.12D
	2.9I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C10	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour