Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C20	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	D.B. Kidd	Locality:	Togari
	Date Desc.:	20/04/05	Elevation:	30 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	1270
	Northing/Long.:	5467575 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	323325  Datum: GDA94	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Backplain	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Humose-Acidic Dermosolic Oxyaquic Hydrosol Thick Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Black (10YR2/1-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, 5-10 mm, Subangular blocky; 
	Moderate grade of structure, 2-5 mm, Granular; Sandy (grains prominent) fabric; Few (<1 per 100mm2) 
	Fine (1-2mm) macropores, Moist; Very weak consistence; Non-plastic; Non-sticky; Field pH 7.1 (pH 
	meter); Common, very fine (0-1mm) roots; Clear, Irregular change to - 
	A12	0.12 - 0.3 m	Very dark brown (10YR2/2-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; Sandy (grains prominent) 
	fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Moist; Very weak consistence; Non-plastic; 
	Non-sticky; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Field pH 7.1 
	(pH meter); Common, very fine (0-1mm) roots; Sharp, Wavy change to - 
	2O1b	0.3 - 0.32 m	Organic Layer; Black (10YR2/1-Moist); , 0-0% ; Fibric peat; Single grain grade of structure; Sandy 
	(grains prominent) fabric; Few (<1 per 100mm2) Fine (1-2mm) macropores, Moist; Loose consistence; 
	Non-plastic; Non-sticky; Field pH 6.8 (pH meter); Many, very fine (0-1mm) roots; Sharp, Irregular 
	change to - 
	2A1b	0.32 - 0.43 m	Black (10YR2/1-Moist); , 0-0% ; Sandy peat; Moderate grade of structure, 10-20 mm, Subangular blocky; 
	Moderate grade of structure, 5-10 mm, Subangular blocky; Sandy (grains prominent) fabric; Moist; Weak 
	consistence; Non-plastic; Non-sticky; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, 
	coarse fragments; Field pH 6.8 (pH meter); Common, very fine (0-1mm) roots; Clear, Irregular change 
	to - 
	2A2b	0.43 - 0.6 m	Very dark greyish brown (10YR3/2-Moist); Mottles, 10YR61, 2-10% , 0-5mm, Faint; Loamy sand (Light); 
	Weak grade of structure, 10-20 mm, Subangular blocky; Weak grade of structure, 2-5 mm, Granular; 
	Sandy (grains prominent) fabric; Moist; Very weak consistence; Non-plastic; Slightly sticky; 2-10%, fine 
	gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Field pH 6.7 (pH meter); Common, 
	very fine (0-1mm) roots; Gradual, Irregular change to - 
	2B2b	0.6 - 1 m	Very dark greyish brown (10YR3/2-Moist); Mottles, 10YR51, 2-10% , 0-5mm, Faint; Sandy clay loam; 
	Moderate grade of structure, 20-50 mm, Subangular blocky; Moderate grade of structure, 10-20 mm, 
	Subangular blocky; Sandy (grains prominent) fabric; Moist; Weak consistence; Non-plastic; Slightly 
	sticky; 2-10%, fine gravelly, 2-6mm, subangular, dispersed, Quartz, coarse fragments; Field pH 5.1 (pH 
	meter); Common, very fine (0-1mm) roots; 
	Morphological Notes

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C20	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	A11	EC, 0.1dS/m.
	A12	EC, 0.0dS/m.
	2O1b	EC, 0.1dS/m.
	2A1b	EC, 0.0dS/m.
	2A2b	EC, 0.0dS/m. Sampled.
	2B2b	EC, 0.0dS/m. Sampled.
	Observation Notes
	Charcoal in top four horizons of approx. 1cm diameter.
	Site Notes
	Property owner, Tony Craven.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C20	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.9C	0.149A	12.93A	4.97	0.22	0.25	0D	18.37B
	6.6A	0G
	0A
	0.2 - 0.275	5C	0.076A	5.65A	3.74	0.13	0.16	0D	9.68B
	5.9A	0.15G
	0A
	0.43 - 0.6	4.3C	0.089A	1.98A	0.55	0.33	0.2	0.25825D	4.09425B
	5.2A	0.56G
	1.03425A
	0.6 - 0.9	4C	0.063A	1.39A	0.51	0.17	0.1	0.34375D	4.13375B
	4.9A	1.41G
	1.96375A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	4.69B	144H	0.39D
	0I
	0.2 - 0.275	4.36B	39H	0.27D
	0I
	0.43 - 0.6	3.43B	58H	0.15D
	33.3I
	0.6 - 0.9	1.84B	6H	0.11D
	3.1I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C20	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour