Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C22	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Green Acres, Near Montagu. Owned by John Grey
	Date Desc.:	18/04/05	Elevation:	7 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	1065
	Northing/Long.:	5485666 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	327609  Datum: GDA94	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Qa	Substrate Material:	Soil pit, No Data
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Alluvial fan
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Fan	Slope Category:	Level
	Slope:	1 % 	Aspect:	5 degrees
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Arenic Inceptic Tenosol Medium Non-gravelly Loamy Sandy 	Principal Profile Form:	N/A
	Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Australian Soil Classification:	Mapping Unit:	N/A
	Basic Arenic Black-Orthic Tenosol Medium Non-gravelly Loamy 	Principal Profile Form:	N/A
	Sandy Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	0-2%, cobbly, 60-200mm, , 
	Profile Morphology
	A1	0 - 0.2 m	Black (10YR2/1-Moist); , 0-0% ; Sandy loam; Moderate grade of structure, 5-10 mm, Polyhedral; Weak 
	grade of structure, <2 mm, Polyhedral; Sandy (grains prominent) fabric; Moderately moist; Very weak 
	consistence; Non-plastic; Slightly sticky; Field pH 6.6 (pH meter); Many, fine (1-2mm) roots; Gradual, 
	Smooth change to - 
	A3	0.2 - 0.4 m	Black (10YR2/1-Moist); , 0-0% ; Sandy clay loam; Weak grade of structure, 50-100 mm, Angular blocky; 
	Weak grade of structure, 20-50 mm, Angular blocky; Sandy (grains prominent) fabric; Few (<1 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Very weak consistence; Non-plastic; Slightly 
	sticky; Cultivation pan, Uncemented, Continuous, Concretionary; Field pH 6.6 (pH meter); Common, very 
	fine (0-1mm) roots; Clear, Smooth change to - 
	2B1	0.4 - 0.52 m	Black (10YR2/1-Moist); , 0-0% ; Silty clay loam; Massive grade of structure; Sandy (grains prominent) 
	fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Very weak consistence; 
	Slightly plastic; Normal plasticity; Slightly sticky; Organic pan, Weakly cemented, Continuous, Massive; 
	Field pH 6.8 (pH meter); Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	2B2	0.52 - 0.75 m	Black (10YR2/1-Moist); , 10YR51, 0-2% , 5-15mm, Distinct; Clayey sand; Massive grade of structure; 
	Sandy (grains prominent) fabric; Many (>5 per 100mm2) Fine (1-2mm) macropores, Moderately moist; 
	Very weak consistence; Non-plastic; Slightly sticky; Field pH 6.9 (pH meter); Few, very fine (0-1mm) 
	roots; Clear, Smooth change to - 
	2BC	0.75 - 1.1 m	Dark grey (10YR4/1-Moist); , 0-0% ; Clayey sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Moist; Very weak consistence; Non-plastic; Slightly sticky; Field pH 7 (pH meter); 
	Morphological Notes
	A1	Penetration Resisance: soft, Salinity measure in dSm^-1 0
	A3	Penetration Resisance: stiff, Salinity measure in dSm^-1 0. Appeared to be compacted from 
	tramping or Machinery

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C22	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	2B1	Penetration Resisance: stiff, Salinity measure in dSm^-1 0
	2B2	Penetration Resisance: stiff, Salinity measure in dSm^-1 0
	2BC	Penetration Resisance: soft, Salinity measure in dSm^-1 0.1
	Observation Notes
	Vegetation Type was Irrigated Pasture. Site was humped and hollowed
	Site Notes
	Mode of Geomorphic Activity: Aggraded. Agent: Wind. Inundation frequency: None.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C22	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.4C	0.168A	12.35A	5.51	0.31	0.53	0D	18.7B
	6.2A	0.37G
	0A
	0.2 - 0.275	5.7C	0.092A	13.12A	5.31	0.19	0.47	0D	19.09B
	6.6A	0G
	0A
	0.4 - 0.52	6.6C	0.102A	11.29A	4.21	0.14	0.45	0.134125D	16.22925B
	7.2A
	0G
	0.13925A
	0.52 - 0.75	6.2C	0.087A	7.18A	3.29	0.09	0.34	0.08D	10.99B
	6.8A	0G
	0.09A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	4.89B	87H	0.52D
	0I
	0.2 - 0.275	2.69B	10H	0.21D
	0I
	0.4 - 0.52	1.57B	8H	0.16D
	4I
	0.52 - 0.75	0.77B	4H	0.09D
	2.3I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C22	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour