Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C34	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	H. Hawkins	Locality:	Windmill Paddock, on Woodscote near Wesley Vale
	Date Desc.:	28/08/06	Elevation:	132 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	874
	Northing/Long.:	5440531 AMG zone: 55	Runoff:	Rapid
	Easting/Lat.:	457192  Datum: GDA94	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Tb	Substrate Material:	Soil pit, Basalt 
	Landform
	Rel/Slope Class: 	Rolling low hills 30-90m 10-32%	Pattern Type:	Low hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	21 % 	Aspect:	No Data
	Surface Soil Condition 	Recently cultivated
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Red Ferrosol Medium Non-gravelly Loamy 	Principal Profile Form:	N/A
	Clay-loamy Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A1p	0 - 0.22 m	Dark reddish brown (2.5YR2/3-Moist); , 0-0% ; Loam; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Moderate grade of structure, 2-5 mm, Subangular blocky; Earthy fabric; Fine, (0 - 5) 
	mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak 
	consistence; Slightly plastic; Normal plasticity; Slightly sticky; Few cutans, <10% of ped faces or walls 
	coated, distinct; Many, very fine (0-1mm) roots; Abrupt, Wavy change to - 
	B21t	0.22 - 0.78 m	Dark reddish brown (2.5YR2/3-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 20-50 mm, 
	Prismatic; Moderate grade of structure, 2-5 mm, Prismatic; Earthy fabric; Few (<1 per 100mm2) Very 
	fine (0.075-1mm) macropores, Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately moist; 
	Weak consistence; Slightly plastic; Normal plasticity; Slightly sticky; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Common, very fine (0-1mm) roots; Few, coarse (>5mm) roots; Clear, 
	Wavy change to - 
	B22t	0.78 - 1 m	Dark reddish brown (2.5YR2/3-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 10-20 mm, 
	Prismatic; Moderate grade of structure, 2-5 mm, Prismatic; Earthy fabric; Moderately moist; Weak 
	consistence; Slightly plastic; Normal plasticity; Slightly sticky; Few, coarse (>5mm) roots; 
	Morphological Notes
	A1p	C34A sampled 0-75mm
	B21t	Colour of Clay Skins coating Ped Faces: 2.5YR 2.5/4. C34B sampled 200-275mm, C34C 
	sampled 300-600mm, C34D sampled 600-780mm
	B22t	Colour of Clay Skins coating Ped Faces: 2.5YR 2.5/4. C34E sampled 7800-1000mm
	Observation Notes
	When pitted Stuart was about to sow peas
	Site Notes
	Mode of Geomorphi Activity: Eroded or Aggraded, Geomorphic Agent: Sheet Wash. Inundation Frequency: None.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C34	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.2C	0.139A	13.89A	2.37	1.42	0.43	0.01D	18.27B
	5.9A	0.1G
	0.16A
	0.2 - 0.275	5.2C	0.144A	14.64A	2.49	1.42	0.47	0.01D	19.17B
	5.9A	0.12G
	0.15A
	0.3 - 0.6	4.3C	0.136A	2.59A	0.87	0.48	0.33	0.22D	6.53B
	4.8A	1.36G
	2.26A
	0.6 - 0.78	4.5C	0.145A	2.19A	0.84	0.38	0.32	0.42D	6.34B
	4.8A	1.85G
	2.61A
	0.78 - 1	4.4C	0.137A	1.53A	0.58	0.19	0.35	0.54D	6.27B
	4.5A	3.4G
	3.62A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	7.99B	154H	0.55D
	40.9I
	0.2 - 0.275	8.86B	140H	0.57D
	39.1I
	0.3 - 0.6	1.38B	6H	0.09D
	1.2I
	0.6 - 0.78	0.74B	3H	0.06D
	0.1I
	0.78 - 1	0.62B	3H	0.05D
	0.6I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C34	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour