Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C44	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	H. Hawkins	Locality:	Plantation Forestry off Stoodley Rd
	Date Desc.:	22/06/06	Elevation:	161 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	1098
	Northing/Long.:	5419140 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	449460  Datum: GDA94	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	No Data
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Low hills
	Morph. Type:	Lower-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Gently inclined
	Slope:	3 % 	Aspect:	No Data
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Acidic Dystrophic Brown Ferrosol Medium Non-gravelly Clay-	Principal Profile Form:	Db3.11
	loamy Clayey Very deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	O1	0 - 0.02 m	Organic Layer; Black (5YR2.5/1-Moist); , 0-0% ; Moderately moist; Loose consistence; Sharp, Smooth 
	change to - 
	A1	0.02 - 0.2 m	Dark brown (7.5YR3/2-Moist); , 0-0% ; Clay loam; Moderate grade of structure, 20-50 mm, Subangular 
	blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; Earthy fabric; Moderately moist; Firm 
	consistence; Moderately plastic; Normal plasticity; Slightly sticky; Many, very fine (0-1mm) roots; 
	Common, fine (1-2mm) roots; Abrupt, Wavy change to - 
	B1	0.2 - 0.64 m	Reddish brown (5YR4/4-Moist); Mottles, 5YR58, 0-2% , 5-15mm, Distinct; Light clay; Moderate grade of
	 structure, 20-50 mm, Subangular blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; 
	Earthy fabric; Moderately moist; Firm consistence; Moderately plastic; Subplastic; Slightly sticky; 
	Common cutans, 10-50% of ped faces or walls coated, faint; Few, fine (1-2mm) roots; Few, fine (1-2mm) 
	roots; Gradual, Wavy change to - 
	B2	0.64 - 1.02 m	Strong brown (7.5YR4/6-Moist); , 0-0% ; Light clay; Strong grade of structure, 20-50 mm, Subangular 
	blocky; Moderate grade of structure, 5-10 mm, Subangular blocky; Earthy fabric; Moderately moist; Firm 
	consistence; Moderately plastic; Normal plasticity; Moderately sticky; Common cutans, 10-50% of ped 
	faces or walls coated, faint; 
	Morphological Notes
	O1	no macropores in the pit face but large >15mm diameter worms seen when doing AS and BD 
	sampling.
	A1	Significant fungal growth inA1, white dispersed but particularly focused around roots. C44A 
	sampled 0-75mm
	B1	More clay skins in the B21 than B22. Charcoal throughout solum, dispersed, fine gravel size, 
	weak. C44B sampled 200-275mm. C44C sampled 350-600mm
	B2	Charcoal throughout solum, some stratification, medium gravel size, weak. C44D sampled 350-
	950mm
	Observation Notes
	vegetation was a pine plantation. Substrate was not reached
	Site Notes
	Mode of Geomorphic Activity: Eroded or aggraded, Agent: Sheet Wash. Inundation frequency: None.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C44	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	4.7C	0.063A	6.02A	2.14	0.47	0.14	0.01D	9.41B
	5.5A	0.26G
	0.64A
	0.2 - 0.275	4.4C	0.041A	2.78A	1.16	0.32	0.12	0.16D	5.98B
	5.3A	1.01G
	1.6A
	0.35 - 0.6	4.2C	0.029A	0.61A	0.34	0.23	0.1	0.19D	4.04B
	4.9A	2.31G
	2.76A
	0.65 - 0.95	4.2C	0.028A	1.03A	0.47	0.18	0.11	0.24D	4.74B
	4.9A	2.8G
	2.95A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	3.73B	8H	0.29D
	3.1I
	0.2 - 0.275	2.2B	5H	0.2D
	1.7I
	0.35 - 0.6	0.94B	2H	0.11D
	1I
	0.65 - 0.95	0.45B	3H	0.06D
	1I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	C44	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour