Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N17	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Tulluchcorum, near Fingal
	Date Desc.:	20/09/05	Elevation:	224 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	616
	Northing/Long.:	5386672 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	573975  Datum: GDA94	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ts	Substrate Material:	Soil pit, No Data
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Terraced land (alluvial)
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Terrace flat	Slope Category:	Very gently sloped
	Slope:	3 % 	Aspect:	320 degrees
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Subnatric Brown Sodosol Thick Non-gravelly 	Principal Profile Form:	N/A
	Loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	Analytical data are incomplete but reasonable confidence.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	Ap	0 - 0.22 m	Dark brown (10YR3/3-Moist); , 0-0% ; Fine sandy loam; Moderate grade of structure, 2-5 mm, 
	Polyhedral; Weak grade of structure, 5-10 mm, Polyhedral; Sandy (grains prominent) fabric; Few (<1 per 
	100mm2) Very fine (0.075-1mm) macropores, Moist; Very weak consistence; Non-plastic; Slightly sticky; 
	Common, very fine (0-1mm) roots; Abrupt, Irregular change to - 
	A2	0.22 - 0.32 m	Yellowish brown (10YR5/4-Moist); Mechanical, 7.5YR58, 2-10% , 0-5mm, Distinct; Mottles, 10YR33, 2-
	10% , 5-15mm, Distinct; Loamy coarse sand; Massive grade of structure; Sandy (grains prominent) 
	fabric; Moist; Very weak consistence; Non-plastic; Slightly sticky; Few (2 - 10 %), Ferruginous, Coarse 
	(6 - 20 mm), Nodules; Densipan, Weakly cemented, Continuous, Massive; Few, very fine (0-1mm) roots; 
	Clear, Wavy change to - 
	B1t	0.32 - 0.7 m	Yellowish brown (10YR5/6-Moist); Mottles, 10YR54, 2-10% , 5-15mm, Faint; Medium clay; Massive 
	grade of structure; Smooth-ped fabric; Moist; Weak consistence; Very plastic; Normal plasticity; Very 
	sticky; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, Quartz, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated, distinct; Gradual, Smooth change to - 
	B2t	0.7 - 0.98 m	Yellowish brown (10YR5/6-Moist); Mottles, 10YR54, 10-20% , 5-15mm, Faint; Medium clay; Massive 
	grade of structure; Smooth-ped fabric; Moderately moist; Firm consistence; Very plastic; Normal 
	plasticity; Very sticky; Common cutans, 10-50% of ped faces or walls coated, distinct; 
	Morphological Notes
	Ap	Penetration resisance: Soft
	A2	Thixotrophic A2, Penetration resisance: Soft
	B1t	Penetration resisance: Firm. Cutans coated ped faces. Sampled 32-70 cm labeled N17c
	B2t	Penetration resisance: Firm, Cutans coated ped faces. Sampled 70-98cm labelled as N17D
	Observation Notes
	Soil Class: Newham. Vegetation: Ryegrass Pasture. Substrate Material was not reached. Probably Tertiary river sediments.
	Site Notes
	Pit located at start of transect. Mode of Geomorphic Agent: Eroded or aggraded. Geomorphic Agent over bank stream. Element Slope 
	Class: Very Gentle. Inundation of less than once per 100yrs.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N17	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	6.2C	0.096A	6.48A	0.94	0.38	0.1	0.24D	8.15B
	6.8A	0G
	0.25A
	0.2 - 0.275	5.9C	0.061A	4.22A	0.79	0.26	0.08	0.17D	5.53B
	6.6A	0G
	0.18A
	0.32 - 0.7	4.8C	0.059A	4.27A	11.37	0.32	1.34	0.13695D	17.6735B
	6.1A	0.08G
	0.3735A
	0.7 - 0.98	5.6C	0.05A	1.71A	10.01	0.22	1.65	0.0109075	13.70998B
	7A	D
	0G
	0.1199825
	A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	1.74B	139H	0.14D
	49.1I
	0.2 - 0.275	1.16B	92H	0.08D
	33.4I
	0.32 - 0.7	0.57B	2H	0.06D
	1I
	0.7 - 0.98	0.33B	1H	0.03D
	0.7I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N17	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour