Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N41	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Sand Paddock, Scone, Near Perth
	Date Desc.:	14/07/06	Elevation:	149 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	619
	Northing/Long.:	5393770 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	515383  Datum: GDA94	Drainage:	Well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	Ts	Substrate Material:	Soil pit, , Sand 
	Landform
	Rel/Slope Class: 	Undulating rises 9-30m 3-10%	Pattern Type:	Alluvial plain
	Morph. Type:	Crest	Relief:	No Data
	Elem. Type:	Dune	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	290 degrees
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Melanic Ferric Chernic Tenosol Thick Non-gravelly Sandy Clayey 	Principal Profile Form:	N/A
	Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A11	0 - 0.12 m	Very dark greyish brown (10YR3/2-Moist); ; Moderately moist; Non-plastic; Slightly sticky; Many, very fine
	 (0-1mm) roots; Gradual, Smooth change to - 
	A12	0.12 - 0.4 m	Dark brown (10YR3/3-Moist); ; Moderately moist; Non-plastic; Slightly sticky; Common, very fine (0-
	1mm) roots; Clear, Wavy change to - 
	A2	0.4 - 0.7 m	Dark yellowish brown (10YR3/4-Moist); Mottles, 10YR44, 2-10% , 5-15mm, Faint; Moderately moist; 
	Non-plastic; Slightly sticky; Few, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	B2	0.7 - 0.9 m	Strong brown (7.5YR4/6-Moist); Mottles, 7.5YR58, 2-10% , 15-30mm, Prominent; Mottles, 7.5YR56, 2-
	10% , 5-15mm, Prominent; Moderately moist; Slightly plastic; Slightly sticky; Abrupt, Wavy change to - 
	B3	0.9 -  m	; Moderately moist; 
	Morphological Notes
	Observation Notes
	Pasture.
	Site Notes
	Mode of Geomorphic Activity: Eroded or Aggraded, Agent: Wind. No inundation.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N41	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	6.7C	0.113A	6.19A	0.83	0.38	0.38	0.03D	7.82B
	7.2A	0G
	0.04A
	0.15 - 0.225	5.5C	0.069A	2.49A	0.45	0.22	0.38	0.04D	3.62B
	6.5A	0G
	0.08A
	0.4 - 0.7	6.3C	0.034A	1.23A	0.36	0.08	0.2	0.01D	1.89B
	6.9A	0G
	0.02A
	0.7 - 0.9	6.5C	0.054A	1.8A	2.37	0.14	0.47	0.01D	4.81B
	7.4A	0G
	0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	1.81B	39H	0.17D
	20.3I
	0.15 - 0.225	1.19B	24H	0.19D
	13.2I
	0.4 - 0.7	0.13B	5H	0.06D
	2.1I
	0.7 - 0.9	0.11B	4H	0.02D
	0.8I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N41	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour