Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N43	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Kurani, Near Bridport
	Date Desc.:	09/06/06	Elevation:	19 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	643
	Northing/Long.:	5473196 AMG zone: 55	Runoff:	Very slow
	Easting/Lat.:	558746  Datum: GDA94	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Not parent material
	Geol. Ref.:	Qa	Substrate Material:	Soil pit, 2 m deep,, Granite 
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Sand plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Swale	Slope Category:	Level
	Slope:	1 % 	Aspect:	352 degrees
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Parapanic Sesquic Semiaquic Podosol Medium Non-gravelly 	Principal Profile Form:	N/A
	Loamy Sandy Very deep
	ASC Confidence:	Great Soil Group:	N/A
	No analytical data are available but confidence is fair.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	O	0 - 0.03 m	Organic Layer; Very dark brown (10YR2/2-Moist); , 0-0% ; Sandy loam; Weak grade of structure, 2-5 mm,
	 Polyhedral; Single grain grade of structure; Sandy (grains prominent) fabric; Few (<1 per 100mm2) 
	Very fine (0.075-1mm) macropores, Moderately moist; Very weak consistence; Non-plastic; Non-sticky; 
	Many, very fine (0-1mm) roots; Abrupt, Smooth change to - 
	A1	0.03 - 0.15 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Loamy sand; Weak grade of structure, 2-5 mm, Polyhedral; 
	Single grain grade of structure; Sandy (grains prominent) fabric; Common (1-5 per 100mm2) Very fine 
	(0.075-1mm) macropores, Moderately moist; Very weak consistence; Non-plastic; Non-sticky; Common, 
	very fine (0-1mm) roots; Clear, Wavy change to - 
	A21	0.15 - 0.25 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR42, 2-10% , 0-5mm, Faint; Loamy sand; Single grain 
	grade of structure; Sandy (grains prominent) fabric; Few (<1 per 100mm2) Very fine (0.075-1mm) 
	macropores, Moist; Loose consistence; Non-plastic; Non-sticky; Common, fine (1-2mm) roots; Gradual, 
	Broken change to - 
	A22	0.25 - 0.6 m	Greyish brown (10YR5/2-Moist); Mottles, 10YR42, 2-10% , 0-5mm, Faint; Loamy sand; Single grain 
	grade of structure; Sandy (grains prominent) fabric; Moderately moist; Loose consistence; Non-plastic; 
	Non-sticky; Few, very fine (0-1mm) roots; Clear, Smooth change to - 
	B1s	0.6 - 0.8 m	 (/-Moist); Substrate influence, 10YR32, 10-20% , 30-mm, Distinct; Loamy sand; Massive grade of 
	structure; Sandy (grains prominent) fabric; Moderately moist; Strong consistence; Non-plastic; Non-
	sticky; Ortstein, Strongly cemented, Continuous, Massive; Few, very fine (0-1mm) roots; Abrupt, Wavy 
	change to - 
	2B21	0.8 - 1.15 m	Greyish brown (2.5Y5/3-Moist); , 0-0% ; Coarse sand; Single grain grade of structure; Sandy (grains 
	prominent) fabric; Moderately moist; Loose consistence; Non-plastic; Non-sticky; 2-10%, fine gravelly, 2-
	6mm, subrounded, dispersed, coarse fragments; Gradual, Wavy change to - 
	2B22	1.15 - 1.25 m	Light brownish grey (2.5Y6/3-Moist); , 0-0% ; Sand; Single grain grade of structure; Moist; Loose 
	consistence; Non-plastic; Non-sticky; 
	Morphological Notes
	A21	N43C 15-25cm
	A22	N43D 30-60cm
	B1s	N43E 60-80cm
	2B21	N43F 80-110cm
	2B22	N43G 115-125cm
	Observation Notes
	Vegetation: pasture. Underlying material is likely to be derived from granite but profile formed from aeolian sand.
	Site Notes
	Aggraded by wind. No inundation

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N43	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	4.9C	0.079A	9.53A	2.69	0.47	0.32	0.09D	13.11B
	6.1A	0.03G
	0.1A
	0.15 - 0.225	4.5C	0.058A	6.09A	1.07	0.25	0.24	0.07D	7.74B
	5.8A	0.03G
	0.09A
	0.15 - 0.25	4.7C	0.027A	1.19A	0.21	0.1	0.1	0.05D	1.67B
	6.1A	0.02G
	0.07A
	0.3 - 0.6	5.4C	0.022A	0.31A	0.08	0.07	0.12	0.03D	0.63B
	6.3A	0.02G
	0.05A
	0.6 - 0.8	4.3C	0.079A	1.77A	0.72	0.18	0.61	0.19D	4.71B
	5.5A	0.88G
	1.43A
	0.8 - 0.11	6.1C	0.025A	0.21A	0.2	0.07	0.13	0.09D	0.77B
	6.5A	0G
	0.16A
	0.115 - 0.125	6.8C	0.124A	0.33A	1.11	0.11	0.31	0.02D	1.93B
	7.6A	0G
	0.07A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	4.28B	14H	0.47D
	8.2I
	0.15 - 0.225	2.94B	6H	0.2D
	3.8I
	0.15 - 0.25	0.63B	2H	0.04D
	1.7I
	0.3 - 0.6	0.21B	2H	0.02D
	1.2I
	0.6 - 0.8	0.27B	8H	0.09D
	5.1I
	0.8 - 0.11	0.13B	2H	0.02D
	0.9I
	0.115 - 0.125	0.05B	2H	0.02D
	0.6I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N43	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour