Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N44	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	H. Hawkins	Locality:	St Mathias Vineyard, Roseveares
	Date Desc.:	05/06/06	Elevation:	48 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	797
	Northing/Long.:	5423621 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	501227  Datum: GDA94	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.9 m deep,Dolerite 
	Landform
	Rel/Slope Class: 	Rolling low hills 30-90m 10-32%	Pattern Type:	Hills
	Morph. Type:	Mid-slope	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	23 % 	Aspect:	324 degrees
	Surface Soil Condition 	Firm
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Mesotrophic Brown Ferrosol Medium Moderately gravelly 	Principal Profile Form:	Dy4.11
	Clay-loamy Clayey Moderately deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.25 m	 (/-Moist); , 0-0% ; Clay loam; Strong grade of structure, 10-20 mm, Subangular blocky; Moderate grade 
	of structure, 2-5 mm, Subangular blocky; Earthy fabric; Fine, (0 - 5) mm crack; Moderately moist; Weak 
	consistence; Slightly plastic; Normal plasticity; Slightly sticky; 20-50%, cobbly, 60-200mm, subrounded, 
	dispersed, Dolerite, coarse fragments; 20-50%, medium gravelly, 6-20mm, subrounded, dispersed, 
	Dolerite, coarse fragments; Few, very fine (0-1mm) roots; Many, fine (1-2mm) roots; Abrupt, Irregular 
	change to - 
	B2	0.25 - 0.57 m	Strong brown (7.5YR5/6-Moist); Mechanical, 7.5YR32, 2-10% , 15-30mm, Distinct; Medium clay; Weak 
	grade of structure, 20-50 mm, Angular blocky; Rough-ped fabric; Moist; Firm consistence; Very plastic; 
	Normal plasticity; Moderately sticky; 20-50%, cobbly, 60-200mm, subrounded, dispersed, Dolerite, coarse
	 fragments; 20-50%, cobbly, 60-200mm, subrounded, dispersed, Dolerite, coarse fragments; Common 
	cutans, 10-50% of ped faces or walls coated, faint; Few, very fine (0-1mm) roots; Few, fine (1-2mm) roots;
	 Clear, Irregular change to - 
	BC	0.57 - 0.9 m	Brown (7.5YR4/4-Moist); Substrate influence, 10YR76, 20-50% , 5-15mm, Distinct; Light clay; Moderate 
	grade of structure, 20-50 mm, Polyhedral; Rough-ped fabric; Moderately moist; Strong consistence; 
	Slightly plastic; Normal plasticity; Very sticky; 20-50%, cobbly, 60-200mm, subrounded, dispersed, 
	Dolerite, coarse fragments; 20-50%, medium gravelly, 6-20mm, subrounded, dispersed, Dolerite, coarse 
	fragments; 90-100%, medium gravelly, 6-20mm, angular, dispersed, Dolerite, coarse fragments; 
	Morphological Notes
	B2	Clay skins coated Ped Faces. N44C 32-50
	BC	N44D 60-90cm
	Observation Notes
	Substrate at a depth greater than 90cm.
	Site Notes
	Mode of Geomorphic Activity: Erroded. Agent: Sheet Wash. No inundation

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N44	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.9C	0.081A	21.76A	8.9	1.45	0.22	0.03D	32.39B
	6.5A	0G
	0.06A
	0.125 - 0.2	5.6C	0.062A	15.82A	7.19	0.89	0.22	0.03D	24.17B
	6.4A	0G
	0.05A
	0.32 - 0.5	5.7C	0.078A	14.44A	21.47	0.34	0.73	0.03D	37.03B
	6.8A	0G
	0.05A
	0.6 - 0.9	6.1C	0.084A	14.45A	24.88	0.32	1.6	0.02D	41.28B
	7.3A	0G
	0.03A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	3.66B	87H	0.43D
	29.8I
	0.125 - 0.2	3.06B	29H	0.34D
	11.5I
	0.32 - 0.5	0.82B	3H	0.11D
	0.8I
	0.6 - 0.9	0.49B	3H	0.08D
	1I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	N44	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour