Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S20	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	R. Moreton	Locality:	Tony Shoobridge. "Fenton Forest" near New Norfolk.
	Date Desc.:	17/05/06	Elevation:	39 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	538
	Northing/Long.:	5274846 AMG zone: 55	Runoff:	Moderately rapid
	Easting/Lat.:	489827  Datum: GDA94	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Qa	Substrate Material:	Soil pit, Sandstone 
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Alluvial plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Terrace flat	Slope Category:	Very gently sloped
	Slope:	2 % 	Aspect:	50 degrees
	Surface Soil Condition 	Soft
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Eutrophic Brown Dermosol Medium Non-gravelly Clay-	Principal Profile Form:	Gn4.33
	loamy Clayey Deep
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A1	0 - 0.32 m	Very dark grey (10YR3/1-Moist); , 0-0% ; Fine sandy clay loam; Moderate grade of structure, 20-50 mm, 
	Subangular blocky; Moderate grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Fine, (0 - 
	5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak 
	consistence; Slightly plastic; Slightly sticky; 2-10%, medium gravelly, 6-20mm, rounded, dispersed, 
	Dolerite, coarse fragments; Common, very fine (0-1mm) roots; Clear, Smooth change to - 
	A3	0.32 - 0.42 m	Very dark grey (10YR3/1-Moist); Mechanical, 7.5YR43, 10-20% , 15-30mm, Distinct; Mechanical, 
	7.5YR44, 2-10% , 15-30mm, Distinct; Clay loam, fine sandy; Moderate grade of structure, 5-10 mm, 
	Subangular blocky; Moderate grade of structure, 10-20 mm, Subangular blocky; Earthy fabric; Fine, (0 - 
	5) mm crack; Few (<1 per 100mm2) Very fine (0.075-1mm) macropores, Moderately moist; Weak 
	consistence; Moderately plastic; Moderately sticky; Common cutans, 10-50% of ped faces or walls 
	coated, distinct; Few, very fine (0-1mm) roots; Gradual, Smooth change to - 
	B1t	0.42 - 0.89 m	Brown (7.5YR4/4-Moist); Mottles, 7.5YR32, 10-20% , 5-15mm, Distinct; Light clay; Strong grade of 
	structure, 20-50 mm, Angular blocky; Strong grade of structure, 10-20 mm, Angular blocky; Rough-ped 
	fabric; Fine, (0 - 5) mm crack; Few (<1 per 100mm2) Fine (1-2mm) macropores, Moderately moist; Weak
	 consistence; Moderately plastic; Moderately sticky; Common cutans, 10-50% of ped faces or walls 
	coated, distinct; Few, very fine (0-1mm) roots; Diffuse, Smooth change to - 
	B2t	0.89 - 1.05 m	Strong brown (7.5YR4/6-Moist); Mottles, 7.5YR33, 10-20% , 5-15mm, Distinct; Light clay; Strong grade 
	of structure, 10-20 mm, Angular blocky; Strong grade of structure, 5-10 mm, Angular blocky; Rough-ped 
	fabric; Moist; Weak consistence; Moderately plastic; Moderately sticky; Common cutans, 10-50% of ped 
	faces or walls coated, distinct; Clear, Wavy change to - 
	B3t	1.05 - 1.2 m	Dark yellowish brown (10YR4/4-Moist); Mottles, 10YR43, 2-10% , 0-5mm, Faint; Medium clay; Moderate 
	grade of structure, 50-100 mm, Angular blocky; Earthy fabric; Moist; Weak consistence; Very plastic; Very
	 sticky; 
	Morphological Notes
	A3	The colour of the clayskins 7.5YR 3/2. A3 horizon has evidence of B1 material in it. A3 not 
	sampled as it was a narrow horizon
	B1t	The colour of the clayskins 7.5YR 3/2. Sampled S20C sampled from depth 45-75cm
	B2t	The colour of the clayskins 7.5YR 3/2. Sampled S20D sampled from depth 87-105cm
	B3t	Sampled S20E sampled from depth 105-120cm
	Observation Notes
	Vegetation is pasture. Soil type likely to have formed from Quaternary sediments that in turn overlie sandstone.
	Site Notes
	Mode of Geomorphic Activity: Eroded. Agent: Overbank Stream. Inundation frequency: less than once per 100 years, for less than a day to a 
	depth of less than 50mm.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S20	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	6.1C	0.124A	15.42A	2.02	1.46	0.1	0.02D	19.03B
	6.9A	0G
	0.03A
	0.2 - 0.275	6.2C	0.077A	14.1A	2.32	0.93	0.16	0.03D	17.55B
	7.1A	0G
	0.04A
	0.45 - 0.75	6.6C	0.058A	19.94A	5.21	0.32	0.28	0.02D	25.81B
	7.7A	0G
	0.06A
	0.87 - 1.05	6.7C	0.05A	11.9A	8.95	0.34	0.25	0.01D	21.49B
	7.8A	0G
	0.05A
	1.05 - 1.2	7C	0.059A	12.51A	17.42	0.54	0.36	0.01D	30.84B
	8.1A	0G
	0.01A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	2.07B	227H	0.27D
	85.5I
	0.2 - 0.275	1.45B	147H	0.17D
	58.5I
	0.45 - 0.75	0.59B	12H	0.07D
	6.1I
	0.87 - 1.05	0.3B	11H	0.04D
	5.6I
	1.05 - 1.2	0.35B	11H	0.04D
	4.2I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S20	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour