Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S36	Observation ID:	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Site Information
	Desc. By:	H. Hawkins	Locality:	Black flat paddock, 'Brooklands' near Campbell Town
	Date Desc.:	18/09/06	Elevation:	273 metres
	Map Ref.:	GPS S.A. Off	Rainfall:	497
	Northing/Long.:	5328110 AMG zone: 55	Runoff:	Slow
	Easting/Lat.:	532315  Datum: GDA94	Drainage:	Moderately well drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	Probable
	Geol. Ref.:	Qa	Substrate Material:	Soil pit, 0.77 m deep,Alluvium 
	Landform
	Rel/Slope Class: 	Gently undulating plains <9m  1-3%	Pattern Type:	Plain
	Morph. Type:	Flat	Relief:	No Data
	Elem. Type:	Terrace flat	Slope Category:	Level
	Slope:	1 % 	Aspect:	No Data
	Surface Soil Condition 	Self-mulching
	Erosion
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Self-Mulching Black Vertosol Non-gravelly Fine Medium 	Principal Profile Form:	N/A
	fine Moderately deep 
	ASC Confidence:	Great Soil Group:	N/A
	All necessary analytical data are available.
	Site Disturbance
	Vegetation
	Surface Coarse Fragments	No surface coarse fragments
	Profile Morphology
	A11p	0 - 0.03 m	Black (10YR2/1-Moist); , 0-0% ; Light clay; Weak grade of structure, <2 mm, Granular; Dry; Strong 
	consistence; Very plastic; Normal plasticity; Slightly sticky; Few, coarse (>5mm) roots; Sharp, Smooth 
	change to - 
	A12	0.03 - 0.48 m	Black (10YR2/1-Moist); , 0-0% ; Light medium clay; Moderate grade of structure, 200-500 mm, 
	Columnar; Moderate grade of structure, 100-200 mm, Angular blocky; Rough-ped fabric; Coarse, (10 - 
	20) mm crack; Very coarse, (20 - 50) mm crack; Dry; Very strong consistence; Very plastic; Normal 
	plasticity; Moderately sticky; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, coarse fragments; 
	Many cutans, >50% of ped faces or walls coated, distinct; Common cutans, 10-50% of ped faces or walls 
	coated, faint; Common, very fine (0-1mm) roots; Few, coarse (>5mm) roots; Clear, Wavy change to - 
	A13	0.48 - 0.77 m	Black (10YR2/1-Moist); , 0-0% ; Medium clay (Heavy); Weak grade of structure, 100-200 mm, Angular 
	blocky; Rough-ped fabric; Dry; Very strong consistence; Very plastic; Normal plasticity; Moderately 
	sticky; 0-2%, medium gravelly, 6-20mm, subangular, dispersed, coarse fragments; Many cutans, >50% of
	 ped faces or walls coated, distinct; Common cutans, 10-50% of ped faces or walls coated, faint; Few, very
	 fine (0-1mm) roots; 
	Morphological Notes
	A11p	Sample S36A 0-75mm
	A12	Colour of clayskins coating ped faces 1G 3/N. Sample S36B 150-225mm, S36C 250-450mm
	A13	Colour of Clay skins 2G 3/5PB. S36D 500-750mm
	Observation Notes
	Lucene planted in October 2005. Farmer said 150mm rain since December. Substrate of river cobbles, AT shape, constant cover over base 
	of pit at 77cm.
	Site Notes
	Mode of Geomorphic Activity: Aggraded. Geomorphic Agent: Over bank stream and sheet wash. Inundation frequency: <once per 100 years.

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S36	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.075	5.7C	0.142A	42.02A	18.68	0.54	1.01	0.09D	62.38B
	6.5A	0G
	0.13A
	0.15 - 0.225	6C	0.103A	37.99A	19.61	0.34	0.91	0.07D	58.99B
	6.9A	0G
	0.14A
	0.25 - 0.45	5.8C	0.083A	12.27A	3.43	0.23	0.28	0.04D	16.34B
	6.3A	0.06G
	0.13A
	0.5 - 0.75	5.2C	0.025A	8.11A	2.08	0.09	0.24	0.09D	10.97B
	6.7A	0.1G
	0.45A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.075	6.03B	131H	0.49D
	43.2I
	0.15 - 0.225	4.28B	37H	0.34D
	13.3I
	0.25 - 0.45	3.38B	56H	0.28D
	19.7I
	0.5 - 0.75	0.84B	6H	0.06D
	1.3I
	Laboratory Analyses Completed for this profile
	10B_NR	Extractable sulfur (mg/kg) - Not recorded
	12_NR_FE	Total element - Fe(%) - Not recorded
	12A1_CU	DTPA - extractable copper, zinc, manganese and iron
	12A1_FE	DTPA - extractable copper, zinc, manganese and iron
	12A1_MN	DTPA - extractable copper, zinc, manganese and iron
	12A1_ZN	DTPA - extractable copper, zinc, manganese and iron
	12C1	Calcium chloride extractable boron - manual colour
	15_NR_AL	Aluminium Cation - meq per 100g of soil - Not recorded
	15_NR_H	Hydrogen Cation - meq per 100g of soil - Not recorded
	15A1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_K	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_MG	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15A1_NA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) - 1M ammonium chloride at pH 7.0, no pretreatment for soluble 
	salts
	15G_C_AL2	Exchangeable aluminium - meq per 100g of soil - Aluminium By KCl extraction and detremination By AAS
	15G1	Exchange acidity (hydrogen and aluminium) by 1M potassium chloride
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	15N1	Exchangeable sodium percentage (ESP)
	18A1	Bicarbonate-extractable potassium
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension

	Project Name:	SCEAM - Soil Condition Evaluation & Monitoring Project, Tasmania
	Project Code:	SCEAM	Site ID:	S36	Observation 	1
	Agency Name:	TAS Department of Primary Industries and Fisheries
	4B2	pH of 1:5 soil/0.01M calcium chloride extract - following Method 4A1
	6B2	Total organic carbon - high frequency induction furnace, volumetric
	7A5	Total nitrogen - high frequency induction furnace, thermal conductivity
	7C1a	Ammonium-N, in presence or absence of nitrite
	7C1b	(Nitrate+nitrite)-N, in presence of nitrite
	9B2_COL	Bicarbonate-extractable phosphorus - automated colour. Based on Colwell (1965). Method no longer 
	recommended
	9C2	Olsen-extractable phosphorus - automated colour