Project Name:	APL
	Project Code:	APL	Site ID:	H273	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	K.D. Nicholls	Locality:	Sammys Orchard
	Date Desc.:	23/04/70	Elevation:	No Data
	Map Ref.:	Rainfall:	800
	Northing/Long.:	147.0666667	Runoff:	Slow
	Easting/Lat.:	-42.99166667	Drainage:	Poorly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Auger boring, 1.4 m deep,Mudstone 
	Land Form
	Rel/Slope Class: 	No Data	Pattern Type:	Terrace (alluvial)
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	No Data	Slope Category:	No Data
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Eutrophic Mottled-Mesonatric Grey Sodosol     	Principal Profile Form:	Dy3.42
	ASC Confidence:	Great Soil Group:	Solodic soil
	No analytical data are available but confidence is fair.
	Site Disturbance:	Cultivation. Irrigated, past or present
	Vegetation:
	Surface Coarse Fragments:
	Profile Morphology
	Ap	0 - 0.1 m	Dark greyish brown (10YR4/2-Moist); ; Sandy loam; Weak grade of structure, 2-5 mm, 
	Subangular blocky; Moderately moist; Firm consistence; Non-plastic; 2-10%, fine gravelly, 2-
	6mm, angular, Quartz, coarse fragments; Diffuse change to - 
	A1	0.1 - 0.13 m	Dark greyish brown (10YR4/2-Moist); Light grey (10YR7/2-Dry); ; Sandy loam; Weak grade of 
	structure, 2-5 mm, Subangular blocky; Moderately moist; Firm consistence; Non-plastic; 2-10%, 
	fine gravelly, 2-6mm, angular, Quartz, coarse fragments; Clear change to - 
	A1A2	0.13 - 0.2 m	Dark greyish brown (10YR4/2-Moist); Light grey (10YR7/2-Dry); ; Sandy loam (Heavy); Weak grade
	 of structure, 2-5 mm, Subangular blocky; Moderately moist; Very firm consistence; Non-plastic; 
	A2	0.2 - 0.24 m	Grey (10YR6/1-Dry); ; Sandy loam (Heavy); Massive grade of structure; Common (1-5 per 
	100mm2) Fine (1-2mm) macropores, Moderately moist; Very firm consistence; Non-plastic; Few 
	(2 - 10 %), Ferruginous, , ; Sharp, Tongued change to - 
	BA2	0.24 - 0.3 m	Dark greyish brown (10YR4/2-Moist); , 7.5YR56; Medium clay; Moderate grade of structure, 50-
	100 mm, Prismatic; Moderate grade of structure, 20-50 mm, Subangular blocky; Fine, (0 - 5) mm 
	crack; Moist; Firm consistence; Slightly plastic; Normal plasticity; 
	B	0.3 - 0.4 m	Dark greyish brown (2.5Y4/2-Moist); , 7.5YR58; Medium heavy clay; Moderate grade of structure, 
	50-100 mm, Prismatic; Moderate grade of structure, 20-50 mm, Subangular blocky; Fine, (0 - 5) 
	mm crack; Moist; Very plastic; Normal plasticity; FewDiffuse change to - 
	B	0.4 - 0.5 m	Dark greyish brown (2.5Y4/2-Moist); , 7.5YR58; Medium heavy clay; Weak grade of structure, 50-
	100 mm, Prismatic; Weak grade of structure, 20-50 mm, Subangular blocky; Fine, (0 - 5) mm 
	crack; Moist; Moderately plastic; Normal plasticity; FewDiffuse change to - 
	B	0.5 - 0.6 m	Strong brown (7.5YR5/8-Moist); , 2.5Y62; Medium clay; Weak grade of structure, 20-50 mm, 
	Subangular blocky; Moist; Moderately plastic; Normal plasticity; Diffuse change to - 
	BC	0.6 - 0.7 m	Strong brown (7.5YR5/8-Moist); , 2.5Y62; Medium clay; Massive grade of structure; Moist; 
	Moderately plastic; Normal plasticity; Diffuse change to - 
	BC	0.7 - 0.8 m	Strong brown (7.5YR5/8-Moist); , 2.5Y62; Medium clay; Massive grade of structure; Moist; Firm 
	consistence; Non-plastic; Diffuse change to - 

	Project Name:	APL
	Project Code:	APL	Site ID:	H273	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	C	0.8 - 1 m	Light brownish grey (2.5Y6/2-Moist); , 7.5YR58; , 10YR56; Heavy clay; Massive grade of 
	structure; Moist; Weak consistence; Non-plastic; Common (10 - 20 %), Manganiferous, , 
	Concretions; Diffuse change to - 
	1.1 - 1.3 m	Light brownish grey (2.5Y6/2-Moist); , 7.5YR58; , 10YR56; Sandy light clay; Massive grade of 
	structure; Weak consistence; Non-plastic; Few (2 - 10 %), Manganiferous, , Concretions; Diffuse
	 change to - 
	Morphological Notes
	Observation Notes
	110-130CM RESIDUAL STRUCTURE OF HIGHLY W`D DR BOULDERS:ODD DR GV 20-200MM SCATTERED THROUGH 
	PROFILE:                    
	Site Notes
	SAMMYS ORCHARD

	Project Name:	APL
	Project Code:	APL	Site ID:	H273	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.1	6A	 0.16A
	0.1 - 0.13	5.6A	 0.12A
	0.13 - 0.2	5.1A	 0.1A
	0.2 - 0.24	5.7A	 0.05A
	0.24 - 0.3	5.5A	 0.09A
	0.3 - 0.4	5.5A	 0.11A
	0.4 - 0.5	5.7A	 0.12A
	0.5 - 0.6	5.9A	 0.12A
	0.6 - 0.7	6.3A	 0.13A
	0.7 - 0.8	6.7A	 0.15A
	0.8 - 1	7A	 0.16A
	1.1 - 1.3	7.1A	 0.14A
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.1	 0.204A	 15D	 42	 23	 14
	0.1 - 0.13	 0.204A	 15D	 43	 23	 14
	0.13 - 0.2	 0.166A
	0.2 - 0.24	 0.037A	 23D	 41	 23	 12
	0.24 - 0.3
	0.3 - 0.4	 0.087A	 5D	 12	 9	 71
	0.4 - 0.5	 0.09A	 3D	 8	 12	 76
	0.5 - 0.6	 3D	 9	 15	 71
	0.6 - 0.7
	0.7 - 0.8	 12D	 21	 18	 46
	0.8 - 1
	1.1 - 1.3	 16D	 28	 24	 27
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.1
	0.1 - 0.13
	0.13 - 0.2
	0.2 - 0.24
	0.24 - 0.3
	0.3 - 0.4
	0.4 - 0.5
	0.5 - 0.6
	0.6 - 0.7
	0.7 - 0.8
	0.8 - 1
	1.1 - 1.3

	Project Name:	APL
	Project Code:	APL	Site ID:	H273	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	3A1	EC of 1:5 soil/water extract
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	MIN_EC	Exchange Capacity - Minerology
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	XRD_C_Gt	Geothite - X-Ray Diffraction
	XRD_C_Is	Interstratified clay minerals - X-Ray Diffraction
	XRD_C_K2O	K2O - X-Ray Diffraction or Clay Fraction (air dry)
	XRD_C_Ka	Kaolin - X-Ray Diffraction
	XRD_C_Qz	Quartz - X-Ray Diffraction
	XRD_C_Vm	Vermiculte - X-Ray Diffraction