Project Name:	CAP
	Project Code:	CAP	Site ID:	H149	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Site Information
	Desc. By:	G.M. Dimmock	Locality:	Near quarry edge site of hole 520:3.2KM WNW from 
	Boat Harbour:
	Date Desc.:	03/07/56	Elevation:	 152 metres
	Map Ref.:	Sheet No. : 8016   1:100000	Rainfall:	1140
	Northing/Long.:	145.595833333333	Runoff:	Rapid
	Easting/Lat.:	-40.9208333333333	Drainage:	Imperfectly drained
	Geology
	ExposureType:	Soil pit	Conf. Sub. is Parent. Mat.:	No Data
	Geol. Ref.:	No Data	Substrate Material:	Soil pit, 0.7 m deep,Quartzite 
	Land Form
	Rel/Slope Class: 	Rolling hills 90-300m 10-32%	Pattern Type:	Hills
	Morph. Type:	No Data	Relief:	No Data
	Elem. Type:	Hillslope	Slope Category:	Moderately inclined
	Slope:	0 % 	Aspect:	No Data
	Surface Soil Condition (dry):
	Erosion:
	Soil Classification
	Australian Soil Classification:	Mapping Unit:	N/A
	Haplic Petroferric Bleached-Leptic Tenosol     	Principal Profile Form:	Uc4.3
	ASC Confidence:	Great Soil Group:	Podzol
	All necessary analytical data are available.
	Site Disturbance:	No effective disturbance. Natural
	Vegetation:	Low Strata - Sedge, , Sparse. *Species includes - None recorded
	Mid Strata - Heath shrub, , Sparse. *Species includes - None recorded
	Tall Strata - Tree, , . *Species includes - Eucalyptus similis, Banksia serrata
	Surface Coarse Fragments:	20-50%, , , Gravel
	Profile Morphology
	A1	0 - 0.06 m	Very dark grey (10YR3/1-Moist); ; Sand (Fibric); Single grain grade of structure; Moist; Very firm 
	consistence; 10-20%, coarse gravelly, 20-60mm, Quartzite, coarse fragments; AbundantDiffuse 
	change to - 
	A1	0.06 - 0.15 m	Very dark greyish brown (10YR3/2-Moist); ; Sand (Fibric); Single grain grade of structure; Moist; 
	Very firm consistence; 10-20%, coarse gravelly, 20-60mm, Quartzite, coarse fragments; 
	AbundantDiffuse change to - 
	A1A2	0.15 - 0.23 m	Dark grey (10YR4/1-Moist); ; Sand; Single grain grade of structure; Moist; Firm consistence; 50-
	90%, coarse gravelly, 20-60mm, Gravel, coarse fragments; ManyDiffuse change to - 
	A2	0.25 - 0.46 m	Grey (10YR5/1-Moist); ; Sand; Single grain grade of structure; Moist; Loose consistence; 50-
	90%, coarse gravelly, 20-60mm, Gravel, coarse fragments; CommonDiffuse change to - 
	0.51 - 0.66 m	Light grey (10YR7/1-Moist); ; Sand; Massive grade of structure; Rigid consistence; 50-90%, 
	Gravel, coarse fragments; Other pans, Moderately cemented, Massive; 
	Morphological Notes
	Observation Notes
	AT 61CM VLG STRONGLY CEMENTED SANDY HARDPAN (IRON PAN):                                                                 
	Site Notes
	WELLINGTON

	Project Name:	CAP
	Project Code:	CAP	Site ID:	H149	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Test Results:
	Depth	pH	1:5 EC	Exchangeable Cations 	Exchangeable	CEC	ECEC	ESP
	Ca	Mg	K	Na	Acidity
	 m	 dS/m	Cmol (+)/kg 	%
	0 - 0.06	4.5A	 7.1H	 3.4	 0.24	 0.26	 34.4H	 54B
	 43E
	0.06 - 0.15	4.3A
	0.15 - 0.23	4.4A
	0.25 - 0.46	4.2A
	0.51 - 0.66
	Depth	CaCO3	Organic	Avail.	Total	Total	Total	Bulk 	Particle  Size  Analysis
	C	P	P	N	K	Density	GV	CS	FS	Silt	Clay
	 m	%	%	 mg/kg	%	%	%	 Mg/m3	%
	0 - 0.06	 10D	 0.006D	 0.374A	 6	 32B	 38	 7	 4
	0.06 - 0.15	 4.4D	 0.156A	 9
	0.15 - 0.23	 0.102A
	0.25 - 0.46
	0.51 - 0.66	 52	 42D	 39	 17	 4
	Depth	COLE	Gravimetric/Volumetric Water Contents	K sat	K unsat
	Sat.	0.05 Bar	0.1 Bar	0.5 Bar	1 Bar	5 Bar	15 Bar
	 m	g/g -  m3/m3	mm/h	mm/h
	0 - 0.06
	0.06 - 0.15
	0.15 - 0.23
	0.25 - 0.46
	0.51 - 0.66

	Project Name:	CAP
	Project Code:	CAP	Site ID:	H149	Observation ID:	1
	Agency Name:	CSIRO Division of Soils (TAS)
	Laboratory Analyses Completed for this profile
	15E1_CA	Exchangeable bases (Ca2+,Mg2+,Na+,K+) by compulsive exchange, no pretreatment for soluble 
	15E1_K	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_MG	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15E1_NA	Exchangeable bases, CEC and AEC by compulsive exchange, no pretreatment for soluble salts
	15G_C_H1	Exchangeable hydrogen - meq per 100g of soil - Hydrogen By back titration of A or B
	15G1_H	Hydrogen Cation - meq per 100g of soil - 1M KCl Exch. Acidity By titration to pH 8.0
	15J_H	Sum of Ex. cations + Ex. acidity - Sum of basic exch. cations and exch. (Hydrogen)
	2_LOI	Loss on Ignition (%)
	2A1	Air-dry moisture content
	4A1	pH of 1:5 soil/water suspension
	5A2	Chloride - 1:5 soil/water extract, automated colour
	6A1_UC	Organic carbon (%) - Uncorrected Walkley and Black method
	7A2	Total nitrogen - semimicro Kjeldahl , automated colour
	9A_HCL	Total element - P(%) - By boiling HCl
	P10_GRAV	Gravel (%)
	P10_PB_C	Clay (%) - Plummet balance
	P10_PB_CS	Coarse sand (%) - Plummet balance
	P10_PB_FS	Fine sand (%) - Plummet balance
	P10_PB_Z	Silt (%) - Plummet balance
	P10A1_C	Clay (%) - Pipette
	P10A1_CS	Coarse sand (%) - Pipette
	P10A1_FS	Fine sand (%) - Pipette
	P10A1_Z	Silt (%) - Pipette